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Movie files of RAM 60m depth calculations with attenuation, provided as separate files. The following figures show one snapshot from each calculation and the filename for each movie file.
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