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· The new cold forging method integrates knurl formation within the die, enhancing production efficiency by eliminating additional forging step.

· Prototype productions validates the cold forging process, confirming a 120% improvement in production rate, from 25 units to 55 units per minute.

· Comparative analysis shows better geometric continuity and morphology.

· [bookmark: _GoBack]Prototype productions confirm the reliability and accuracy of FEM-based software.
