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	Operational Parameters
	Value

	He flow (upper)
	0.8 L min-1

	He flow (lower)
	0.1 L min-1

	Ar flow
	0.4 L min-1

	Ar auxiliary gas flow
	0.9 L min-1

	Ar plasma gas flow
	14.2 L min-1

	ICP power
	1350 W

	Einzel lens 
	7.4 V

	Sampling depth
	11 mm

	Injector diameter
	1.5 mm
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