Table S1: Technical information for PET/CT imaging procedures of the five different institutions.

	
PET Parameters
	Saarland University Medical Center Homburg
	University Hospital Ludwig Maximilian University of Munich
	Johannes Gutenberg University Medical Center 
(in collaboration with the Radiology and Nuclear Medicine Practice at the Köln Triangle, Cologne)
	Charité Universitätsmedizin Berlin
	University Medical Center Würzburg

	Tracer
	[68Ga]Ga-PSMA-11
	[18F]PSMA-1007
	[68Ga]Ga-PSMA-11
[18F]PSMA-1007
	[68Ga]Ga-PSMA-11
	[68Ga]Ga-PSMA I&T
[18F]PSMA-1007

	Time: injection to imaging [min]
	
60 min
	
60 min
	[68Ga]Ga-PSMA-11:
~ 60 min
[18F]PSMA-1007:
~ 90 min
	
60 min
	[68Ga]Ga-PSMA I&T:
~ 60 min
[18F]PSMA-1007:
~90 min

	
PET/CT scanner Model
	Siemens Biograph
mCT 40

	GE Discovery 
690
	Philips Gemini 
TF 16 

	Philips Gemini 
TF 16 

	Siemens Biograph
mCT 128 flow 

	Pixel matrix size
	200x200
	256x256
	168x168
	144x144

	200x200

	Acquisition time/bed position [min]
	2 min
	2 min
	2 min.
	3 min

	2 min

	Extended field of view [cm]
	21.4 cm
	15.4 cm
	21.8 cm
	18.0 cm

	78.0 cm

	Slice thickness [mm]
	3.0 mm
	3.27 mm
	3.0 mm
	4.0 mm

	3.0 mm

	Reconstruction Parameters
	
	
	
	
	

	No. of iterations
	3
	3
	2
	3

	3

	No. of subsets
	21
	36
	14
	33

	21

	Reconstructed slice thickness [mm]
	5.0 mm
	5.0 mm
	4.0 mm
	4 mm

	5.0 mm

	Low dose CT / Diagnostic CT
	Low dose CT
	Diagnostic CT
	Low-dose CT
	Low dose CT
	Low-dose CT



