Supplemental Digital Content 3. Fracture reduction and implant placement details per implant type and the occurrence of implant failure. 
	Implant type
	
	
	No implant failure
	Implant failure

	DHS
	Reduction
	
	
	
	
	

	
	
	Perfect
	4 (66.7)
	2 (33.3)
	
	

	
	
	Acceptable
	7 (58.3)
	5 (62.5)
	
	

	
	
	Poor
	8 (42.1)
	1 (12.5)
	
	

	
	TAD
	
	
	
	
	

	
	
	Adequate
	22 (75.9)
	7 (24.1)
	
	

	
	
	Inadequate
	1 (100.0)
	0 (0.0)
	
	

	PFNA
	Reduction
	
	
	
	
	

	
	
	Perfect
	22 (95.7)
	1 (4.3)
	
	

	
	
	Acceptable
	40 (100.0)
	0 (0.0)
	
	

	
	
	Poor
	28 (100.0)
	0 (0.0)
	
	

	
	TAD
	
	
	
	
	

	
	
	Adequate
	88 (98.9)
	1 (1.1)
	
	

	
	
	Inadequate
	3 (100.0)
	0 (0.0)
	
	


TAD mean tip-apex distance in millimetres, AP anterior-posterior, Ax axial. 
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