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Supplemental File Table 1. Surgical details and further operations
	
	
	
	Total
	ORCT
	CBCT
	p-value

	Navigated 
screws
	Total
	6733
	3515
	3218
	0.3661

	
	Median (range)
	8 (1-24)
	8 (1-24)
	8 (1-20)
	

	Fused 
levels
	Total
	3254
	1678
	1576
	0.5901

	
	Median (range)
	4 (1-15)
	4 (1-15)
	4 (1-11)
	

	Screw system 
(n, %)
	Rigid
	746 (87.5)
	383 (87.2)
	363 (87.7)
	0.0507

	
	Semi-rigid
	107 (12.5)
	56 (12.8)
	51 (12.3)
	

	
	Carbon
	221 (25.9)
	134 (30.5)
	87 (21.0)
	

	Decompression
	Cases (n, % of total)
	572 (67.1)
	284 (64.7)
	288 (69.6)
	0.1449

	
	Levels per patient
	Total (median, range)
	2
	0-8
	1
	0-8
	2
	0-8
	0.0275

	
	
	Decompressed (median, range)
	2
	1-8
	2
	1-8
	2
	1-8
	0.1526

	360° fusion 
(n, %)
	VBR
	129 (15.1)
	66 (15.0)
	63 (15.2)
	0.1629

	
	XLIF
	60 (7.0)
	28 (6.4)
	32 (7.7)
	

	
	ALIF
	26 (3.0)
	8 (1.8)
	18 (4.3)
	



The table shows details on surgical procedures, navigated screws, fused levels, used systems, additional decompressions and later surgeries for the whole cohort as well as for the comparison between operating room intraoperative computed-tomography (ORCT)-based and cone-beam intraoperative computed-tomography (CBCT)-based pedicle screw placements. Later surgical procedures such as vertebral body replacement (= VBR), extreme lateral intervertebral fusion (= XLIF), or anterior lumbar interbody fusion (=ALIF) are not included in the present analysis. 
