	Safety Factor
	Guidelines for limit equilibrium of a slope

	˂1.0
	Unsafe

	1.0-1.25
	Questionable safety

	1.25-1.40
	Satisfactory for routine cuts and fills
Questionable for dams, or where failure would be catastrophic

	˃1.40
	Satisfactory for dam
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