Supplementary Table 1 Composition of the domestic and brewery wastewater samples measured in the MFC sensors (CODD = dissolved COD; BODin = amount of BOD5 (in mg) injected to the anode chamber of the cells)
	Domestic wastewater
	
	
	
	
	
	
	
	
	
	
	
	
	

	Sample No.
	1
	2
	3
	4
	5
	6
	7
	8
	9
	10
	11
	
	
	

	COD (mg l-1)
	188
	187
	351
	335
	278
	433
	123
	235
	382
	356
	328
	
	
	

	CODD (mg l-1)
	71
	59
	119
	95
	93
	194
	33
	70
	90
	126
	91
	Average
	SD
	RSD (%)

	BOD5 (mg l-1)
	101
	95
	263
	192
	213
	312
	84
	167
	261
	257
	214
	
	
	

	BODin (mg)
	6.1
	5.7
	15.8
	11.5
	12.8
	18.7
	5.0
	10.0
	15.7
	15.4
	12.8
	
	
	

	CODD/COD
	0.38
	0.32
	0.34
	0.28
	0.34
	0.45
	0.27
	0.30
	0.24
	0.35
	0.28
	0.32
	0.06
	18.5

	BOD5/COD
	0.54
	0.51
	0.75
	0.57
	0.77
	0.72
	0.68
	0.71
	0.68
	0.72
	0.65
	0.66
	0.09
	13.1

	Average measurement time (d)
	0.9
	1.1
	3.5
	3.3
	2.8
	3.7
	2.7
	3.0
	3.9
	3.8
	2.9
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Brewery wastewater
	
	
	
	
	
	
	
	
	
	
	
	
	

	Sample No.
	1
	2
	3
	4
	5
	6
	7
	8
	9
	10
	
	
	
	

	COD (mg l-1)
	250
	497
	188
	834
	197
	439
	124
	87
	736
	304
	
	
	
	

	CODD (mg l-1)
	159
	263
	98
	537
	115
	300
	76
	51
	580
	221
	
	Average
	SD
	RSD (%)

	BOD5 (mg l-1)
	146
	330
	143
	660
	142
	293
	81
	59
	501
	194
	
	
	
	

	BODin (mg)
	8.8
	19.8
	8.6
	39.6
	8.5
	17.6
	4.9
	3.5
	30.1
	11.6
	
	
	
	

	CODD/COD
	0.64
	0.53
	0.52
	0.64
	0.59
	0.68
	0.62
	0.59
	0.79
	0.73
	
	0.63
	0.08
	13.3

	BOD5/COD
	0.58
	0.66
	0.76
	0.79
	0.72
	0.67
	0.65
	0.68
	0.68
	0.64
	
	0.68
	0.06
	8.8

	Average measurement time (d)
	1.4
	3.0
	1.5
	3.9
	1.3
	2.3
	0.7
	0.5
	3.2
	2.0
	
	
	
	



Supplementary Table 2 Data and analysis of the linear regression parameters of the Q vs. BOD5 correlation for real wastewaters. 
Slope = slope of the correlation line (C / mg BOD5 l-1)
Inters. = calculated intersection of the correlation line with the abscissa (mg BOD5 l-1)
Domestic = slope and intersection of the linear correlation fitted to domestic wastewater measurement points (see Fig. 5a)
Brewery = slope and intersection of the linear correlation fitted to brewery wastewater measurement points (see Fig. 5b)
Average = average value of slope and intersections obtained for domestic and brewery wastewaters
RD = relative difference between the slope of domestic and brewery wastewater related to the Average
D = difference between the intersection values obtained for domestic and brewery correlations
DOM+BREW = slope and intersection of the linear correlation fitted to all real wastewater measurement points (domestic and brewery together, see Fig. 5c)
	 
	Domestic
	Brewery
	Average
	RD (%)
	D
	DOM+BREW

	 
	Slope
	Inters.
	Slope
	Inters.
	Slope
	Inters.
	Slope
	Inters.
	Slope
	Inters.

	MFC "A"
	0.585
	45.584
	0.564
	27.873
	0.575
	36.729
	3.6
	17.710
	0.572
	21.032

	MFC "B"
	0.568
	42.720
	0.556
	17.544
	0.562
	30.132
	2.2
	25.176
	0.574
	19.014

	MFC "C"
	0.511
	30.733
	0.519
	34.416
	0.515
	32.575
	1
	-3.683
	0.514
	16.721

	Average
	0.555
	39.679
	0.546
	26.611
	0.551
	33.145
	
	
	0.553
	18.922

	SD
	0.039
	7.878
	0.024
	8.507
	0.031
	3.335
	 
	 
	0.034
	2.157
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