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Fig. S1 Size distribution of rice straw and energy reeds fiber (a and b) and pressure versus time used for biocomposites production (c)
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