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Fig. S1. Sustainable output voltage generation capability of MEG at high relative humidity (>95%) for continuous 3 h.

1

image1.png
Voltage (V)

o N o o =
N IS o © =)
L L

o
=)

o
=)

0.5

10 15 20
Time (hour)

25

3.0




