Supplementary Data
[bookmark: _GoBack]Preparing, by cutting, composite material specimens for density and tensile testing.
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Figure. S1 - Tensile tests and density measurement specimens (10x2x1 cm). The composite in the figure was prepared with Glyc/CA=0.5 and sawdust=Glyc (values in weight).
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Figure. S2 – Typical data from tensile tests.
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