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Appendix 1 – Information on the primary (measured) variables used in the study.
	Variable
	Sampling method
	Analysis
	Data availability

	Phosphorus concentration (plake)
	Measured at depths of 0.4, 5, 10, 15 and 20 m (+ additional depths that varied during the study period) from samples collected using Niskin bottles
	Spectrophotometric determination of reactive P following persulfate oxidation in an autoclave
	1984-2018

	Hypolimnetic dissolved oxygen (DO)
	Measured at depths of 20, 30, 50 100 m (N. basin) and 20, 30, 50 and 90 m (+ additional depths that varied during the study period) from water samples collected using Niskin bottles, and measured with DO sensor along profiles (steps of 0.5-1 m) from 1987.
	Winkler titration
	1984-2018

	Primary productivity (PPR)
	Measured at 0.4, 1.25, 2.5, 3.75, 5, 6.5, 8, 10, 12.5, 15 and 20 m using the dark and light bottle methods with 14C as Carbon tracer
	Measurement of 14C in incubated bottles using scintillation counting, before and after acidification
	1984-2018

	Temperature
	Measured at 0.4, 5, 10, 15 and 20 m using resistance thermometers (accuracy: ±0.05°C or better)
	--
	1984-2018

	Conductivity
	[bookmark: _GoBack]Measured along profiles (steps of 0.5-1 m) using multi-parameter instruments
	--
	1987-2018




