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[bookmark: _GoBack]Supplementary Material 10: Flow velocity at 105 L/s (A) and 80 L/s (C) water discharge and turbulent kinetic energy at 105 L/s (B) and 80 L/s (D) water discharge over the prototype barrier. Measurement points are indicated by the red spots and the flow direction is shown by the blue arrow labelled F.
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