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CV curves of Fe3O4 NPs dispersed in carbon paste (CP) (Black lines) and of CP only (Red lines). Supporting electrolyte: NaCl 0.5 M. The potentials are relative to that of the Ag|AgCl|KCl 3 M electrode. The potential scan rate is 50 mV/s.
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