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Fig. S1  Secondary electron micrograph of an AMZ4 sample cut parallel to the build-height (a), together with composition for Zr, Cu, Nb and Al from energy dispersive X-ray analysis (b). From the region indicated by the red box in (a), composition profiles are plot which show a homogeneous chemical distribution (c).
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