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Fig. S1. SP-%1F Nquist and Bode Diagram
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Fig. S2. SP-%5F Nquist and Bode Diagram
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Fig. S3. SP-%7.5F Nquist and Bode Diagram
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Fig. S4. SP-%10F Nquist and Bode Diagram
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Fig. S5. SP-%12.5F Nquist and Bode Diagram
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