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Figure S1. Effect of nanofiber amount on the equilibrium concentration of CIP in the solution Ce and CIP E.
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Figure S2. Zeta potential of a hydrogel nanofiber as a function of pH. C16A = 35 mol %.
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