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Figure S1 Normalized Raman spectra of as received, activated (vacuum, 110 C) and compressed (25 bar) HKUST-1. The spectra are vertically shifted for clarity.
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