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[bookmark: _GoBack]Figure 1. TEM image of AuNR@SiO2 prepared at pH=8.
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Fig.2. TEM image of AuNR@SiO2 prepared by reducing the CTAB concentration to 5.0E-4 M.
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Fig.3. TEM image of AuNR@SiO2 prepared by reducing the CTAB concentration to 2.5E-4 M.
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Fig.4. TEM image of AuNR@SiO2 prepared by increasing the CTAB concentration to 4.0E-3 M.
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