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[bookmark: _GoBack]Online Resources 1 and 2 show the landslides organized according to latitude, longitude, landslide area, height difference of slide, aspect, slope angle (average), topographic features, and geological formation. To focus on DSGSD, ID numbers are assigned to topographic features and areas in that order.
Online Resource 1 Landslide data (N = 38)
	ID
	Latitude
	Longitude
	Area (m2) 
	H (m) 
	Aspect
	Slope Angle (°)
	Topographic Features
	Geologic Formation

	1
	34.1914
	135.8928
	7,500
	112
	NNE
	35.3 
	6
	Obadanigawa

	2
	34.1230
	135.7478
	5,100
	96
	E
	37.1 
	6
	Miyama

	3
	34.0782
	135.6136
	48,000
	56
	N
	45.8 
	4 and 6
	Miyama

	4
	34.0638
	135.6468
	28,700
	176
	WSW
	37.3 
	4 and 6
	Miyama

	5
	34.2248
	135.8360
	26,400
	124
	SSE
	30.8 
	4 and 6
	Yukawa

	6
	34.1448
	135.7723
	6,600
	108
	NE
	45.2 
	4 and 6
	Miyama

	7
	34.1448
	135.6443
	35,900
	176
	SW
	39.3 
	2, 5, and 6
	Yukawa

	8
	34.0556
	135.6388
	29,900
	254
	NE
	32.5 
	4 and 6
	Miyama

	9
	34.1637
	135.7611
	9,200
	128
	E
	34.7 
	2, 3, and 6
	Miyama

	10
	34.1696
	135.7626
	9,400
	92
	SW
	39.3 
	3, 4, and 6
	Miyama

	11
	34.1265
	135.7375
	14,000
	114
	NW
	29.8 
	1, 4, and 6
	Miyama

	12
	34.0663
	135.7005
	4,500
	94
	NNE
	32.7 
	1, 2, 4, and 6
	Miyama

	13
	34.0834
	135.7651
	20,600
	154
	N
	35.9 
	1, 4, and 6
	Miyama

	14
	34.0145
	135.6930
	8,500
	165
	NW
	28.2 
	3, 4, 5, and 6
	Ryujin

	15
	34.1821
	135.6968
	42,100
	174
	N
	31.3 
	2, 4, 5, and 6
	Hanazono

	16
	34.1183
	135.6765
	48,100
	308
	NW
	38.5 
	4, 5, and 6
	Miyama

	17
	34.1358
	135.5992
	5,044
	103
	W
	34.1 
	4, 5, and 6
	Yukawa

	18
	34.0423
	135.7303
	14,300
	154
	NNW
	35.9 
	1, 2, 4, 5, and 6
	Miyama

	19
	34.0307
	135.7018
	34,100
	234
	NE
	40.1 
	1, 3, 4, 5, and 6
	Ryujin

	20
	34.1401
	135.6660
	13,500
	136
	ENE
	37.8 
	1, 2, 3, 5, and 6
	Yukawa

	21
	34.0627
	135.6828
	7,400
	64
	W
	37.7 
	1, 3, 4, 5, and 6
	Miyama

	22
	34.0985
	135.8048
	14,700
	126
	NNW
	36.4 
	2, 3, 4, and 5
	Miyama

	23
	34.0570
	135.6281
	42,300
	218
	WSW
	35.1 
	1, 2, 3, 4, 5, and 6
	Miyama

	24
	34.1204
	135.7735
	5,100
	158
	NW
	38.4 
	2, 3, 5, and 6
	Miyama

	25
	34.1281
	135.7810
	48,000
	226
	WSW
	32.2 
	3, 4, 5, and 6
	Miyama

	26
	34.1937
	135.8514
	18,200
	134
	NNW
	34.4 
	3, 4, and 6
	Hanazono

	27
	34.1367
	135.7467
	1,400
	32
	NE
	40.9 
	2, 3, 4, and 5
	Miyama

	28
	34.0154
	135.6951
	51,700
	227
	NNW
	36.4 
	1, 2, 4, and 6
	Ryujin

	29
	34.0159
	135.6980
	22,500
	92
	NNW
	28.2 
	2, 3, 4, and 6
	Ryujin

	30
	34.2195
	135.8346
	77,200
	124
	ESE
	28.9 
	2, 4, 5, and 6
	Hanazono

	31
	34.2195
	135.8434
	38,600
	120
	NNW
	32.5 
	1, 2, 4, 5, and 6
	Hanazono

	32
	34.1544
	135.7413
	59,000
	254
	ENE
	39.8 
	1, 2, 3, 4, 5, and 6
	Miyama

	33
	34.0414
	135.7608
	86,300
	396
	NNE
	43.5 
	1, 3, 4, 5, and 6
	Miyama

	34
	34.1398
	135.7698
	10,300
	144
	SW
	40.7 
	1, 3, 4, 5, and 6
	Miyama

	35
	34.1256
	135.7263
	254,900
	592
	NW
	35.5 
	1, 2, 3, 4, 5, and 6
	Miyama

	36
	34.1120
	135.7346
	19,200
	120
	NNE
	25.0 
	1, 3, 4, 5, and 6
	Miyama

	37
	34.1294
	135.7538
	182,700
	400
	NW
	37.5 
	1, 2, 3, 4, 5, and 6
	Miyama

	38
	34.1347
	135.7412
	195,100
	446
	NNW
	30.8 
	1, 2, 3, 4, 5, and 6
	Miyama


H: Elevation difference between the top and the end of the slide area, Angle Strike: maximum slope direction, Slope angle: angle between the top and end of the slide area (°). Topographic features, 1: Main scarp, 2: Minor scarp, 3: Frank, 4: Terminal Cliff, 5: Gully, 6: Irregular Undulation.

Online Resource 2 DSGSD data (N = 63)
	ID
	Latitude
	Longitude
	A (m2) 
	H (m)
	Aspect
	Slope Angle (°) 
	Topographic Features
	Geologic
Formation

	39
	34.0300
	135.6469
	58,800
	236
	NNW
	36.0 
	4 and 6
	Ryujin

	40
	34.2161
	135.8354
	59,100
	164
	E
	31.6 
	1, 4, and 6
	Obadanigawa

	41
	34.1382
	135.6999
	29,700
	209
	E
	39.3 
	1, 4, and 5
	Miyama

	42
	34.0513
	135.7320
	155,300
	322
	NNW
	33.7 
	4, 5, and 6
	Miyama

	43
	34.0957
	135.7881
	126,200
	249
	NNE
	38.4 
	1, 3, 4, 5, and 6
	Miyama

	44
	34.0517
	135.7498
	76,100
	323
	NNW
	34.9 
	1, 4, and 6
	Miyama

	45
	34.0535
	135.7545
	12,900
	139
	N
	32.2 
	1, 4, and 6
	Miyama

	46
	34.1417
	135.6787
	254,900
	592
	W
	37.3 
	1, 3, and 4
	Yukawa

	47
	34.1446
	135.7085
	13,900
	91
	NNW
	33.9 
	1, 4, and 5
	Miyama

	48
	34.1379
	135.7694
	44,600
	230
	NW
	40.0 
	3, 5, and 6
	Miyama

	49
	34.1130
	135.6796
	39,400
	241
	SSW
	39.9 
	1, 4, and 5
	Miyama

	50
	34.0392
	135.6473
	178,000
	315
	NNE
	38.8 
	1, 2, 3, and 6
	Miyama

	51
	34.1852
	135.7018
	9,200
	128
	NW
	37.8 
	1, 3, 4, and 6
	Hanazono

	52
	34.1451
	135.6863
	48,100
	308
	N
	33.8 
	1, 2, 3, and 4
	Yukawa

	53
	34.1377
	135.6860
	21,900
	128
	NE
	36.7 
	1, 2, 4, and 5
	Miyama

	54
	34.1591
	135.6983
	48,000
	226
	WSW
	37.5 
	1, 2, 3, and 4
	Miyama

	55
	34.1266
	135.7321
	18,500
	182
	SSW
	36.3 
	1 and 3
	Miyama

	56
	34.0967
	135.7821
	250,600
	251
	NNW
	38.2 
	1, 2, 3, 4, and 6
	Miyama

	57
	34.1588
	135.6880
	28,000
	136
	NE
	37.2 
	1, 3, 4, and 5
	Yukawa

	58
	34.1543
	135.6868
	10,300
	144
	SW
	38.1 
	1, 3, 4, 5, and 6
	Yukawa

	59
	34.1488
	135.6838
	6,600
	108
	N
	37.1 
	1, 4, 5, and 6
	Yukawa

	60
	34.1392
	135.6685
	39,400
	173
	NE
	36.7 
	1, 3, 4, 5, and 6
	Yukawa

	61
	34.1603
	135.7133
	5,100
	158
	W
	33.2 
	1, 2, 5, and 6
	Miyama

	62
	34.1309
	135.7351
	204,800
	443
	WNW
	37.3 
	1, 4, 5, and 6
	Miyama

	63
	34.0311
	135.6526
	113,100
	424
	NNW
	37.8 
	1, 2, 3, 4, 5, and 6
	Ryujin

	64
	34.0344
	135.7223
	8,500
	165
	NNW
	39.3 
	1, 2, 3, 4, 5, and 6
	Ryujin

	65
	34.1844
	135.7050
	80,600
	124
	NNE
	36.9 
	1, 3, 4, 5, and 6
	Hanazono

	66
	34.1617
	135.7550
	9,400
	92
	WNW
	35.2 
	1, 4, 5, and 6
	Hanazono

	67
	34.1341
	135.6446
	195,100
	446
	WNW
	39.1 
	2, 3, 4, 5, and 6
	Yukawa

	68
	34.1448
	135.6816
	25,400
	139
	N
	34.0 
	1, 3, 4, 5, and 6
	Yukawa

	69
	34.1590
	135.7121
	5,100
	96
	WNW
	35.1 
	1, 2, 3, 4, 5, and 6
	Miyama

	70
	34.1528
	135.7768
	282,800
	449
	SSE
	37.1 
	1, 4, 5, and 6
	Miyama

	71
	34.1929
	135.8534
	93,400
	278
	NW
	36.9 
	1, 3, 4, 5, and 6
	Hanazono

	72
	34.1792
	135.7094
	121,100
	258
	NNW
	35.9 
	1, 2, 3, 4, 5, and 6
	Hanazono

	73
	34.1398
	135.6768
	14,000
	114
	W
	37.2 
	1, 3, 4, 5, and 6
	Yukawa

	74
	34.1525
	135.7151
	93,900
	315
	SW
	39.0 
	1, 3, 4, 5, and 6
	Miyama

	75
	34.1498
	135.7153
	19,200
	120
	WNW
	36.6 
	1, 2, 3, 4, 5, and 6
	Miyama

	76
	34.1563
	135.7152
	182,700
	400
	SW
	39.2 
	1, 2, 3, 4, 5, and 6
	Miyama

	77
	34.1132
	135.7434
	27,500
	185
	NW
	36.8 
	1, 3, 4, 6
	Miyama

	78
	34.0408
	135.7263
	57,200
	247
	NNW
	35.8 
	1, 3, 4, 5, and 6
	Miyama

	79
	34.1763
	135.7025
	78,500
	195
	N
	36.2 
	1, 3, 4, 5, and 6
	Hanazono

	80
	34.1097
	135.7868
	251,200
	460
	NNE
	37.0 
	1, 2, 3, 4, 5, and 6
	Miyama

	81
	34.2225
	135.8278
	7,500
	181
	SW
	38.5 
	1, 2, 3, 4, 5, and 6
	Hanazono

	82
	34.0985
	135.7997
	14,500
	151
	NNE
	32.0 
	1, 2, 3, 4, 5, and 6
	Miyama

	83
	34.0310
	135.6535
	14,300
	154
	NW
	39.2 
	1, 2, 3, 4, 5, and 6
	Ryujin

	84
	34.1537
	135.6826
	1,400
	32
	S
	37.8 
	1, 2, 3, 4, 5, and 6
	Yukawa

	85
	34.1416
	135.6950
	187,200
	207
	SSE
	38.3 
	1, 2, 3, 4, 5, and 6
	Miyama

	86
	34.1553
	135.7650
	120,000
	520
	SSE
	37.0 
	1, 3, 4, 5, and 6
	Miyama

	87
	34.1375
	135.7978
	43,500
	154
	SSE
	37.6 
	1, 2, 3, 4, 5, and 6
	Miyama

	88
	34.1571
	135.7848
	171,700
	344
	WSW
	35.4 
	1, 2, 3, 4, 5, and 6
	Miyama

	89
	34.1530
	135.7895
	185,700
	431
	SE
	37.6 
	1, 2, 3, 4, 5, and 6
	Miyama

	90
	34.1431
	135.7114
	157,400
	198
	NE
	34.9 
	1, 2, 3, 4, 5, and 6
	Miyama

	91
	34.1143
	135.7076
	193,600
	382
	ENE
	40.7 
	1, 2, 3, 4, 5, and 6
	Miyama

	92
	34.1651
	135.7432
	13,500
	136
	SE
	33.7 
	1, 3, 4, 5, and 6
	Miyama

	93
	34.0710
	135.7122
	24,000
	188
	WSW
	32.7 
	1, 3, 4, 5, and 6
	Miyama

	94
	34.0270
	135.6374
	124,300
	146
	NE
	41.0 
	1, 2, 3, 4, 5, and 6
	Miyama

	95
	34.1643
	135.7407
	413,700
	435
	SE
	30.4 
	1, 2, 3, 4, 5, and 6
	Miyama

	96
	34.1410
	135.7143
	19,700
	148
	NE
	40.3 
	1, 3, 4, 5, and 6
	Miyama

	97
	34.0294
	135.7239
	51,700
	227
	NNW
	35.9 
	1, 2, 3, 4, 5, and 6
	Ryujin

	98
	34.0890
	135.7631
	39,500
	94
	NNW
	34.0 
	1, 3, 4, 5, and 6
	Miyama

	99
	34.0141
	135.6871
	77,200
	124
	ENE
	42.3 
	1, 2, 3, 4, 5, and 6
	Ryujin

	100
	34.0211
	135.6855
	38,600
	120
	E
	39.0 
	1, 2, 3, 4, 5, and 6
	Ryujin

	101
	34.1270
	135.6779
	51,200
	196
	NE
	40.6 
	1, 2, 3, 4, 5, and 6
	Yukawa


H: Elevation difference between the top and the end of the slide area, Angle Strike: maximum slope direction, slope angle: angle between the top and end of the slide area (°). Topographic features, 1: Main scarp, 2: Minor scarp, 3: Frank, 4: Terminal Cliff, 5: Gully, 6: Irregular Undulation.
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