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[bookmark: _Ref204851486]Figure S1 Maximum water-surface elevation (WSE) for all six synthetic storms under the SIR scenario: (a) Storm 290, (b) Storm 237, (c) Storm 297, (d) Storm 276, (e) Storm 432, and (f) Storm 620. Black lines represent storm tracks.
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[bookmark: _Ref204851729]Figure S2 Maximum water-surface elevation (WSE) for all six synthetic storms under the NIR scenario: (a) Storm 290, (b) Storm 237, (c) Storm 297, (d) Storm 276, (e) Storm 432, and (f) Storm 620. Black lines represent storm tracks.
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[bookmark: _Ref204851846]Figure S3 Maximum water-surface elevation (WSE) for all six synthetic storms under the AIR scenario: (a) Storm 290, (b) Storm 237, (c) Storm 297, (d) Storm 276, (e) Storm 432, and (f) Storm 620. Black lines represent storm tracks.
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