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Fig. S1. CO2 formation during TPO of loose contact catalyst/soot mixture (—) and corresponding COx formation of bare soot (—), each without SO2 exposure. TPO conditions: y(O2) = 1 V%, y(H2O) = 2 V%, N2 balance, F = 500 ml/min (STP), m = 0.53 g (blend) or 0.033 g (bare soot), DT/Dt = 3 K/min.
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Fig. S2. O2-TPD profile of the sample after 30 ppm SO2 exposure and treatment at 705 °C in gasoline model exhaust. TPD conditions: F(He) = 100 ml/min (STP), m ≈ 20 mg, DT/Dt = 10 K/min.
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