Table 1 The parameters used to perform the Multiple Reaction Monitoring quantification of ABA and IAA

	Monitored ions
	retention time
[min]
	collision energy
[eV]
	primary ion
(quantifier)
	secondary ions
(qualifier)

	ABA
	2.59
	4
4
	265.2
	229.1
247.1

	IAA
	2.17
	9
53
	176.1
	130.3
77.2

	D-IAA 
	2.13
	14
50
	181.1
	134.7
81.4

	D-ABA 
	2.56
	10
18
	271.2
	167.1
139.1


ABA abscisic acid, D-ABA deuterated ABA used as internal standard, D-IAA deuterated IAA used as internal standard, IAA indole-3-acetic acid 
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