Supplementary Material 1
Information on biochar production 
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Figure 1a -Design of the floor kiln used for the production of biochar derived from Gliricidia sepium (biochar II and its activated variants)
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Figure 1b – Floor kiln and Gliricidia sepium biomass[image: ] 
Figure 1c – Process of biochar II production from Gliricidia sepium in the floor kiln
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