Impact of storage time on characteristics of synthetic greywater with two different pollutant strengths to be treated or recycled
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[bookmark: _Hlk530892374]Online Resource 2 Physiochemical properties of fresh synthetic greywater

	Parameter
	Unit
	Low Concentration
	High Concentration

	
	
	n
	Mean
	SD
	Min
	Max
	n
	Mean
	SD
	Min
	Max

	pH
	‒
	81
	6.9
	0.48
	5.3
	7.9
	81
	8.4
	1.61
	5.4
	11.5

	Redox potential
	mV
	81
	34.1
	21.23
	-18.1
	111.2
	81
	-36.6
	74.22
	-182.1
	97.9

	Turbidity
	NTU
	81
	22.9
	7.14
	9.8
	41.6
	81
	188.9
	47.22
	18.3
	308.0

	Total suspended solids
	mg/L
	81
	39.9
	15.94
	10.0
	87.0
	81
	317.0
	58.35
	173.0
	473.0

	Electrical conductivity
	µS/cm
	81
	164.6
	63.24
	98.7
	452.0
	81
	988.5
	196.09
	612.0
	1677.0

	Dissolved oxygen
	mg/L
	81
	10.4
	1.24
	7.7
	12.3
	81
	10.5
	1.39
	6.9
	12.6

	Colour
	Pa/Co
	81
	214.5
	64.07
	26.0
	340.0
	81
	1587.8
	379.89
	787.0
	2499.0

	Temperature
	°C
	81
	17.7
	4.58
	6.7
	27.0
	81
	16.9
	5.40
	6.5
	27.8

	Biochemical oxygen demand
	mg/L
	81
	17.6
	8.00
	2.0
	40.0
	81
	34.7
	12.99
	10.0
	60.0

	Chemical oxygen demand
	mg/L
	81
	28.9
	14.47
	8.2
	86.7
	81
	129.2
	34.68
	63.9
	221.0

	Ammonia‒nitrogen
	mg/L
	81
	0.2
	0.22
	0.0
	1.1
	81
	0.4
	0.19
	0.1
	1.1

	Nitrate‒nitrogen
	mg/L
	81
	1.3
	1.21
	0.1
	7.6
	81
	8.9
	6.38
	0.2
	29.8

	Ortho‒phosphate‒phosphorus
	mg/L
	81
	8.4
	4.36
	3.3
	27.4
	81
	59.1
	14.16
	30.6
	94.2

	Element
	
	
	
	
	
	
	
	
	
	
	

	Aluminium
	mg/L
	45
	0.52
	0.528
	0.09
	1.56
	45
	2.13
	0.869
	0.76
	4.77

	Boron
	mg/L
	33
	0.14
	0.067
	0.10
	0.36
	33
	0.57
	0.068
	0.49
	0.72

	Calcium
	mg/L
	55
	10.54
	0.853
	8.51
	11.81
	45
	36.08
	8.750
	22.38
	50.72

	Cadmium
	mg/L
	42
	0.09
	0.056
	0.04
	0.23
	39
	7.36
	2.981
	3.67
	11.58

	Chromium
	mg/L
	54
	0.04
	0.063
	0.01
	0.23
	54
	3.20
	0.918
	1.67
	5.70

	Copper
	mg/L
	63
	0.16
	0.058
	0.10
	0.30
	63
	1.44
	0.435
	0.95
	2.03

	Iron
	mg/L
	48
	0.21
	0.102
	0.11
	0.43
	48
	6.41
	2.476
	2.48
	10.37

	Potassium
	mg/L
	12
	4.04
	0.448
	3.41
	4.65
	12
	60.16
	1.684
	58.31
	62.53

	Magnesium
	mg/L
	48
	1.45
	0.191
	1.19
	1.78
	48
	17.16
	2.119
	12.68
	20.33

	Manganese
	mg/L
	63
	0.17
	0.084
	0.07
	0.26
	63
	0.98
	0.257
	0.64
	1.29

	Sodium
	mg/L
	12
	14.32
	1.662
	12.01
	16.00
	12
	62.68
	14.538
	45.50
	76.92

	Nickel
	mg/L
	51
	0.04
	0.065
	0.01
	0.18
	51
	0.05
	0.065
	0.01
	0.20

	Zinc
	mg/L
	39
	0.21
	0.159
	0.01
	0.39
	39
	4.25
	1.500
	2.22
	6.34


n number of tested samples, SD standard deviation, Min minimum value, Max maximum value, NTU nephelometric turbidity unit
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