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Figure SM1: Photo of the flow-through reactor (FTR) setup.
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Figure SM2: Tracer test results for a) Biocide, Glass, and Lact FTRs, b) low salinity (LS1 and LS2) FTRs, c) brackish water (BW1 and BW2) FTRs.
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Figure SM3: Black color generated in the FTRs; Left: the beginning of the experiments, Middle: 5 weeks after begging of the experiments, Right: at the end of the experiments.
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