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Supplemental Figure 4. Response of chloroform over time using different septa. On the y-axis the area percentage for chloroform is displayed, and on the x-axis the time in hours is displayed. The response of chloroform on PTFE (blue line), barrier (red line) and PTFE + Aluminum liner (green line) is displayed over the exposure time. Using only a PTFE or a barrier septum, loss of chloroform is perceived after storage of only a few hours, respectively 50% and 20% after five hours. Around 90% of the chloroform is perceived when a PTFE septum is combined with an aluminum liner for a period of eight hours. Samples were analyzed by means of GC-MS.  Abbreviations: PTFE, polytetrafluoroethylene; Al, aluminum. 
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