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1. XRF data for the aluminum substrate:
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2. The images below present SEM images of the specimens after the 5-day immersion tests.
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Figure 1 SEM shows micrographs of uncoated a) and coated b) aluminum specimens after the 5-day immersion tests. Notably, the uncoated sample exhibits more significant changes in surface morphology.
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