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Fig. 1SM Aerobic granular sludge a) in a flask before polymer addition, b) in a flask after polymer addition, c) under a microscope (100x magnification) before polymer addition, d) under a microscope (100x magnification) after polymer addition 
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