	Supplementary Table 1. Three-way ANOVA-generated marginal mean CLCRRT by CRRT mode, filter type, and effluent flow rate

	CRRT mode
	Filter type
	Effluent flow rate (L/h)
	CLCRRT (L/h)
	95% CI

	CVVH
	HF1400
	2
	1.873
	1.674-2.072

	
	
	4
	3.107
	2.762-3.452

	
	M150
	2
	1.742
	1.543-1.941

	
	
	4
	3.129
	2.784-3.474

	CVVHD
	HF1400
	2
	1.881
	1.537-2.226

	
	
	4
	3.355
	3.010-3.700

	
	M150
	2
	1.768
	1.424-2.113

	
	
	4
	2.503
	2.158-2.848


	
Supplementary Table 2. Monte Carlo Simulated Percent Probability of Attaining 75% fT>MIC for Patients Receiving CRRT and Optimal Effluent Flow Rate-based Dosing Regimens

	Effluent flow rate (L/h)
	Optimal dosing regimen 
(3h infusion)
	MIC (mg/L)

	
	
	0.25
	0.5
	1
	2
	4
	8
	16

	0.5
	1.5 g q12h
	100
	100
	100
	100
	100
	94.7
	60.8

	1
	1.5 g q12h
	100
	100
	100
	99.5
	98.0
	85.1
	40.4

	1.5
	1.5 g q12h
	100
	100
	99.9
	99.5
	97.2
	79.6
	28.3

	2
	2 g q12h
	100
	100
	99.9
	99.7
	97
	83.9
	38.1

	2.5
	2 g q12h
	100
	99.8
	99.4
	98.2
	94.1
	76.0
	29.2

	3
	1.5 g q8h
	100
	100
	100
	99.9
	98.9
	89.3
	43.7

	3.5
	1.5 g q8h
	100
	100
	100
	100
	98.5
	84.9
	35.9

	4
	2 g q8h
	100
	100
	100
	100
	98.7
	91.2
	49.1

	4.5
	2 g q8h
	100
	100
	100
	99.6
	98.1
	85.0
	43.7

	5
	2 g q8h
	100
	100
	99.9
	99.6
	96.6
	79.9
	33.4




