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(d) Time Series Comparison for F’NC%S&5 and PNCge;S
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(e) Time Series Comparison for PNC?Em and PNC?E&O
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(b) Time Series Comparison for F’NCSS&1 and PNCSe;l
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