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Supplemental Figure 1. RVE model geometry (fiber volume fraction = 58.9%) and mesh configuration using C3D8 elements for fiber–matrix interface analysis. The fiber volume fraction of 58.9% corresponds to the exact geometric value imposed by the idealized hexagonal packing used for periodic boundary condition implementation, while the experimentally measured fiber volume fraction is 60%.
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