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Fig. S1 High magnification SEM of (a) LDH and (b) SHS.
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Fig. S2 3D surface roughness profiles of (a) Bare, (b) LDH and (c)SHS.
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Fig. S3 CAs and SAs of different liquids on SLIPS.
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Fig. S4 EDS spectrum of the (a) LDH and (b) SHS.
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[bookmark: _Hlk71836668]Fig. S5 (a) Change of CA of SHS immersed in 0.1 M HCl and NaOH solution for different time, (b) the SHS soaked in 0.1 M HCl and NaOH solution for 10 minutes.
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[bookmark: _GoBack]Fig. S6 Anti-fouling test of SHS in different liquids.
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