Supplementary Information
Electrocatalytic Performance Optimization of Co-MOF-74 and IrO2 Hybrid Catalysts for Acidic Oxygen Evolution Reaction
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Figure S1. (a) TOF values of all composite Co-MOF/IrO2 catalysts, varied with potentials, and (b) corresponding TOF values at 1.53 V (vs. RHE)
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Figure S2. Linear plot of anodic peak current (ip) vs v1/2 (where v is the scan rate) obtained from CV measurements in 10 mM potassium ferricyanide and 0.1 M KCl supporting electrolyte.
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