Supporting Information for
Life Cycle Assessment of the manufacturing and operation of distillation column for eliminating volatile and organic halogen compounds from process wastewater

Huyen Trang Do Thi1, Andras Jozsef Toth1,*

1 Environmental and Process Engineering Research Group, Department of Chemical and Environmental Process Engineering, Budapest University of Technology and Economics, H-1111, Hungary, Budapest, Műegyetem rkp. 3.
* Corresponding author. E-mail address: andrasjozseftoth@edu.bme.hu, Tel: +36 1 463 1490; Fax: +36 1 463 3197, ORCID: 0000-0002-5787-8557



Table S1 Life cycle inventory data
	Phase
	Materials
	Input
	Output
	Unit

	Manufacturinga
	Aluminum oxide
	3.08E-06
	-
	kg

	
	Glass coated
	1.67E-06
	
	kg

	
	Iron and steel
	5.42E-05
	
	kg

	
	Iron/Nickel/Chromium
	2.92E-06
	
	kg

	
	Stainless steel (AISI 304)
	2.38E-04
	
	kg

	
	Synthetic Rubber
	2.92E-06
	
	kg

	
	Water
	1.25E-04
	
	kg

	
	Electricity
	5.96E-04
	
	kWh

	Operationb
	1,1,2-Trichloroethane
	9.04E-09
	1.63E-21
	kg

	
	1,2-Dichloroethane
	3.90E-07
	1.54E-21
	kg

	
	1,4-Dioxane
	2.02E-07
	2.54E-09
	kg

	
	2-Hexanone
	1.00E-09
	1.01E-09
	kg

	
	Acetone
	2.90E-05
	5.36E-13
	kg

	
	Benzene
	2.34E-06
	1.79E-23
	kg

	
	Carbon tetrachloride
	4.00E-09
	1.06E-21
	kg

	
	Chloroform
	2.67E-07
	3.76E-22
	kg

	
	Dichloromethane
	1.02E-03
	5.36E-13
	kg

	
	Diethyl ether
	6.32E-08
	6.88E-24
	kg

	
	Ethanol
	1.11E-05
	1.95E-08
	kg

	
	Ethyl acetate
	1.59E-06
	7.69E-19
	kg

	
	Ethyl acetone
	1.13E-07
	4.90E-17
	kg

	
	Ethylbenzene
	4.93E-07
	2.44E-23
	kg

	
	Isobutanol
	6.63E-05
	2.01E-09
	kg

	
	Isopropanol
	2.18E-05
	1.53E-10
	kg

	
	Methanol
	4.43E-03
	1.00E-03
	kg

	
	Methyl Ethyl ketone
	3.13E-07
	5.36E-17
	kg

	
	Methyl Isobutyl Ketone
	5.83E-08
	2.47E-20
	kg

	
	m-Xylene
	1.90E-06
	2.33E-21
	kg

	
	n-Butanol
	1.70E-08
	5.47E-17
	kg

	
	n-Propanol
	2.01E-08
	1.84E-14
	kg

	
	o-Xylene
	3.64E-07
	3.80E-20
	kg

	
	p-Xylene
	4.97E-07
	2.44E-23
	kg

	
	t-Butanol
	3.01E-08
	5.41E-15
	kg

	
	Tetrachloroethylene
	3.50E-08
	1.91E-22
	kg

	
	Toluene
	1.70E-05
	0.00E+00
	kg

	
	Trichloroethylene
	7.17E-06
	3.70E-21
	kg

	
	Water
	9.94E-01
	9.99E-01
	kg

	
	Electricity
	4.08E-03
	-
	kWh


a Adapted from [1] 
b Adapted from [2] 
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