[bookmark: _GoBack]Supplementary material
Use of Defatted Cottonseed-Derived Biochar for Biodiesel Production: 
A Closed-Loop Approach


Table S1. GC analysis method
	Column
	DB-WAX (30 m × 0.25 mm × 0.25 µm)
	

	Injection volume
	1 µL
	
	

	Carrier gas
	N2
	
	

	Flow rate
	1 mL min-1
	
	

	Detector temperature
	240 ˚C
	
	

	Oven
	Heating rate (˚C/min)
	Temperature (˚C)
	Hold time (min)

	
	
	50
	3

	
	10
	180
	5

	
	5
	190
	5

	
	2
	220
	5

	
	2
	230
	10




