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Fig S1. (A) Sb concentration soils worldwide (A), in water bodies (B), and in bottom sediments of water bodies (C).
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Fig S2: Sb sorption capacity (A), and immobilization efficiency (B) onto pristine and functionalized biochars. 
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Figure S3: Transformation and mechanisms of Hg immobilization in biochar treated paddy soils
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