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Table S1:  Average number of irrigations, cumulative irrigation water applied and water saved over CF in five locations of two regions during 2021-22 and 2022-23
	Region
	Location
	Irrigation treatments
	2021-22
	2022-23

	
	
	
	No. of irrigation
	Cumulative water applied (mm) excluding rainfall
	Water saved over CF (%)
	No. of irrigation
	Cumulative water applied (mm) excluding rainfall
	Water saved over CF (%)

	Barishal
	Loc-1
	AWD
	8
	787
	26.0
	9
	 900
	21.1

	
	
	Saturation
	9
	885
	16.7
	10
	1000
	12.3

	
	
	CF
	11
	1063
	
	12
	1140
	-

	
	Loc-2
	AWD
	7
	679
	26.0
	8
	776
	21.0

	
	
	Saturation
	9
	855
	6.8
	9
	855
	13.6

	
	
	CF
	10
	917
	
	11
	990
	-

	
	Loc-3
	AWD
	8
	808
	30.8
	8
	84
	91.7

	
	
	Saturation
	10
	933
	20.1
	10
	950
	6.1

	
	
	CF
	12
	1168
	
	11
	1012
	-

	
	Loc-4
	AWD
	8
	792
	23.7
	7
	686
	23.8

	
	
	Saturation
	10
	937
	9.7
	9
	828
	8.0

	
	
	CF
	11
	1038
	
	10
	900
	-

	
	Loc-5
	AWD
	7
	733
	38.9
	7
	735
	26.6

	
	
	Saturation
	9
	867
	27.8
	9
	864
	13.7

	
	
	CF
	12
	1200
	
	11
	1001
	-

	Khulna
	Loc-1
	AWD
	8
	765
	21.9
	9
	855
	15.2

	
	
	Saturation
	10
	887
	9.4
	10
	900
	10.7

	
	
	CF
	11
	979
	
	12
	1008
	-

	
	Loc-2
	AWD
	8
	725
	32.5
	8
	736
	25.7

	
	
	Saturation
	10
	893
	16.9
	10
	900
	9.1

	
	
	CF
	11
	1074
	
	11
	990
	-

	
	Loc-3
	AWD
	7
	686
	29.3
	8
	752
	19.1

	
	
	Saturation
	9
	858
	11.5
	9
	864
	7.1

	
	
	CF
	10
	970
	
	10
	930
	-

	
	Loc-4
	AWD
	8
	725
	28.1
	8
	720
	26.5

	
	
	Saturation
	9
	834
	17.3
	9
	819
	16.3

	
	
	CF
	11
	1008
	
	11
	979
	-

	
	Loc-5
	AWD
	7
	691
	25.7
	8
	776
	24.1

	
	
	Saturation
	8
	779
	16.2
	10
	950
	7.1

	
	
	CF
	9
	930
	26.0
	11
	1023
	-


CF = continuous flooding; AWD = alternate wetting and drying. Cumulative irrigation water applied excludes rainfall. 
