


Supplemental
Supplemental A: List of bands available on the Micasense Dual-Camera System and the wavelengths covered by each band.
	MicaSense Band
	MicaSense λ

	Blue
	430-458 nm

	Blue 2
	465-485 nm

	Green
	550-570 nm

	Green 2
	524-538 nm

	Red
	663-673 nm

	Red 2
	642-658 nm

	Red Edge 1
	712-722 nm

	Red Edge 2
	700-710 nm

	Red Edge 3
	731-749 nm

	Near Infrared
	820-860 nm



Supplemental B: Table of the variance explained and mean squared error for each of the random forest models fit to the 12 approaches used to summarize the within crown pixel spectral values.
	Summarization Approach
	Variance Explained
	Mean Squared Error (MSE)

	Mean
	21.16
	92.20

	Median
	21.38
	90.82

	10th Percentile
	26.62
	86.46

	20th Percentile
	19.38
	95.90

	25th Percentile
	19.72
	94.58

	30th Percentile
	23.24
	90.16

	40th Percentile
	21.19
	92.93

	60th Percentile
	19.49
	95.06

	70th Percentile
	20.49
	97.39

	75th Percentile
	19.88
	97.02

	80th Percentile
	23.44
	91.38

	90th Percentile
	22.85
	91.81
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Supplemental C: Box plot of spectral band values from Lad et al., (2023). NDVI2: Normalized Difference Vegetation Index 2; FMCI: Foliar Moisture Content Index; PRI: Photosynthetic Reflectance Index.
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