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Supplementary Fig. S1. Coefficient of correlation showing inter-sensor variability of Atmotube Pro sensors collated together prior to data collection.



Supplementary Table S 1. PM2.5 Atmotube Pro sensor data descriptives (One-minute data)
	Location
	
	
	
	
	Percentiles
	

	
	
	AM
	SD
	GM
	GSD
	10th
	25th
	50th
	75th
	95th
	99th
	Max

	A
	Indoor
	20.0
	20.5
	16.3
	1.8
	9.0
	11.0
	15.0
	21.0
	40.0
	112.6
	283.0

	
	Outdoor
	17.1
	20.5
	13.7
	1.8
	7.0
	9.0
	13.0
	19.0
	33.0
	82.0
	485.0

	B
	Indoor
	20.3
	13.3
	17.5
	1.7
	9.0
	12.0
	17.0
	24.0
	46.0
	65.8
	296.0

	
	Outdoor
	18.1
	20.2
	15.4
	1.7
	8.0
	11.0
	15.0
	21.0
	38.0
	59.0
	892.0

	C
	Indoor
	20.1
	30.7
	15.7
	1.8
	8.0
	10.0
	16.0
	23.0
	40.0
	77.3
	834.0

	
	Outdoor
	16.3
	29.9
	12.4
	1.9
	6.0
	8.0
	12.0
	18.0
	33.0
	74.0
	886.0

	D
	Indoor
	17.0
	9.9
	14.6
	1.8
	7.0
	10.0
	15.0
	21.0
	39.0
	51.0
	64.0

	
	Outdoor
	14.0
	14.3
	12.1
	1.7
	6.0
	9.0
	13.0
	18.0
	26.0
	34.0
	785.0

	E
	Indoor
	15.9
	8.5
	14.0
	1.7
	7.0
	10.0
	15.0
	20.0
	30.0
	43.0
	140.0

	
	Outdoor
	20.6
	12.7
	17.7
	1.7
	9.0
	12.0
	18.0
	27.0
	42.0
	57.0
	376.0

	F
	Indoor
	18.5
	12.8
	15.3
	1.9
	7.0
	10.0
	15.6
	23.0
	40.0
	70.8
	179.0

	
	Outdoor
	28.2
	44.3
	21.1
	1.9
	10.0
	14.0
	20.0
	30.0
	59.0
	171
	868.0

	G
	Indoor
	15.1
	9.7
	12.8
	1.8
	6.0
	9.0
	12.0
	19.0
	36.0
	53.0
	73.0

	
	Outdoor
	15.6
	7.6
	13.9
	1.6
	7.0
	10.0
	14.0
	20.0
	30.0
	39.0
	58.0

	H
	Indoor
	15.4
	14.8
	12.7
	1.8
	6.0
	9.0
	12.0
	19.0
	31.0
	46.0
	331.0

	
	Outdoor
	22.7
	16.0
	19.4
	1.7
	10.0
	13.0
	19.0
	28.0
	47.0
	63.0
	256.0

	I
	Indoor
	21.6
	20.4
	17.8
	1.8
	8.0
	12.0
	18.0
	27.0
	43.0
	74.0
	573.0

	
	Outdoor
	19.0
	16.1
	16.0
	1.8
	8.0
	11.0
	16.0
	24.0
	41.0
	56.0
	567.0

	J
	Indoor
	17.8
	22.4
	14.8
	1.7
	7.0
	11.0
	15.0
	21.0
	36.0
	55.0
	793.0

	
	Outdoor
	18.8
	11.5
	16.3
	1.7
	9.0
	11.0
	16.0
	23.0
	40.0
	57.0
	293.0

	K
	Indoor
	15.2
	8.2
	13.5
	1.6
	7.0
	10.0
	14.0
	18.0
	29.0
	42.0
	141.0

	
	Outdoor
	19.3
	10.9
	16.9
	1.7
	9.0
	12.0
	17.0
	24.0
	38.0
	53.0
	196.0

	L
	Indoor
	14.5
	10.8
	12.1
	1.8
	6.1
	8.0
	12.0
	17.9
	31.0
	40.0
	178.9

	
	Outdoor
	18.4
	13.4
	15.7
	1.7
	8.0
	11.0
	16.0
	23.0
	35.0
	51.9
	365.0


Key: AM = Arithmetic mean; SD = Standard deviation; GM = Geometric mean; GSD = Geometric standard deviation

Supplementary Table S 2.PM2.5 Purple Air sensor data descriptives (Two-minute data)
	Location
	
	
	
	
	Percentiles
	

	
	
	AM
	SD
	GM
	GSD
	10th
	25th
	50th
	75th
	95th
	99th
	Max

	AK
	I
	50.3
	40.9
	37.2
	2.3
	14.8
	23.0
	36.9
	66.1
	137.2
	189.8
	529

	
	O
	62.7
	50.4
	46.8
	2.2
	19.3
	28.3
	46.7
	81.2
	172.6
	240.0
	584

	UI
	I
	60.6
	61.8
	39.8
	2.5
	13.7
	22.0
	36.2
	77.5
	194.2
	277.8
	990

	
	O
	64.3
	61.7
	43.7
	2.5
	16.8
	24.1
	40.4
	82.5
	202.5
	287.6
	852

	School
	H
	76.6
	59.7
	58.5
	2.1
	23.5
	33.2
	57.7
	98.8
	207.8
	285.3
	434


Key: I = Indoor; O = Outdoor; H = Hybrid; AM = Arithmetic mean; SD = Standard deviation; GM = Geometric mean; GSD = Geometric standard deviation
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