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Figure S1. Finite-element simulation results of the potential difference between the FEP and copper films at different positions. (a, b) Electric potential distributions of the device structure with contact-separating mode and sliding mode, respectively.
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Figure S2. The circuit for signal conditioning.
Video S1. TBJT as a finger-triggered active smart tactile switch.
Video S2. Demonstration of the TBJT in controlling a table lamp.
Video S3. Demonstration of the TBJT in controlling an electric fan.
Video S4. Demonstration of the TBJT in controlling a household security alarm.
1
17

