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Figure S1. Photograph of surfaces of the rotor and the stator.
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Figure S2. Enlarged view of the graph from Figure 1c.
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[bookmark: _Hlk193146394]Figure S3. Upper envelope of the result shown in Figure 3g. 
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