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Table S1 Patient distribution for different scanner manufacturers and magnetic field strengths
	Characteristics
	Magnetic Field Strength
	Manufacturer Details
	Patient Count

	Magnetic Field Strength
	1.5 T
	Optima MR450w, GE Healthcare, Little Chalfont, UK
	98
(10.63%)

	
	
	Signa HDx, GE Healthcare, Little Chalfont, UK
	53
(5.75%)

	
	
	Signa HDxt, GE Healthcare, Little Chalfont, UK
	138 (14.97%)

	
	
	Avanto, Siemens, Munich, Germany
	179 (19.41%)

	
	3 T
	Signa Excite, GE Healthcare, Little Chalfont, UK
	10 (1.08%)

	
	
	Signa HDx, GE Healthcare, Little Chalfont, UK
	219 (23.75%)

	
	
	Signa HDxt, GE Healthcare, Little Chalfont, UK
	110 (11.93%)

	
	
	Skyra, Siemens Healthcare, Little Chalfont, UK
	57 
(6.18%)

	
	
	Trio, Siemens, Munich, Germany
	1
 (0.11%)

	
	
	Trio Tim, Siemens, Munich, Germany
	57 
(6.18%)
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Table S2 Values of Different MRI acquisition parameters in the dataset
	MRI Acquisition Parameters
	Value Details
	Values

	Slice Thickness (mm)
	Range
	1.04 – 2.5

	
	Median
	2

	Repetition Time (ms)
	Range
	3.54-7.39

	
	Median
	5.2

	Echo Time (ms)
	Range
	1.25-2.76

	
	Median
	2.39

	Acquisition Matrix
	Minimum Array Size
	320 × 320

	
	Maximum Array Size
	448 × 448

	Flip Angle (degrees)
	Range
	7-12

	
	Median
	10

	FOV(mm)
	Range
	250-480

	
	Median
	350




