Supplementary Table statistics

	DIV
	7
	14
	21
	28
	35
	42
	49
	56

	BP HDPEI vs PLO
	0.75116
	0.80512
	0.80512
	0.80512
	0.81238
	0.75116
	0.80512
	0.80512

	BP LDPEI vs PLO
	0.62
	0.78201
	0.48436
	0.62
	0.78201
	0.78201
	0.78201
	0.62

	NB HDPEI vs PLO
	0.36836
	0.75122
	0.36836
	0.47909
	0.36836
	0.61668
	0.36836
	0.36836

	NB LDPEI vs PLO
	0.31076
	0.38838
	0.44539
	0.00046624
	0.0016893
	0.04673
	0.0027155
	0.38838

	AEBP HD vs BP LD
	3.0253e-05
	8.4694e-09
	7.9841e-15
	0.8253
	0.068536
	1.7064e-05
	1.0374e-08
	0.01677

	MFRBP HD vs BP LD
	5.588e-05
	0.0013068
	5.0903e-05
	0.001404
	5.0903e-05
	4.078e-08
	2.0085e-11
	0.00017153

	MBRBP HD vs BP LD
	/
	2.3758e-05
	0.83715
	0.80098
	0.086909
	0.0037129
	4.2859e-07
	6.3338e-05

	RSBP HD vs BP LD
	/
	0.026779
	0.78458
	0.00057857
	0.01662
	0.14192
	1.0124e-07
	1.8586e-07

	NBRBP HD vs BP LD
	/
	0.0060657
	0.0052081
	0.38186
	0.46285
	0.0028601
	3.8849e-07
	0.00040261

	AENB HD vs NB LD
	0.0085506
	4.8237e-06
	2.3686e-10
	4.577e-06
	6.9773e-07
	1.6173e-06
	1.4299e-06
	7.2612e-06

	MFRNB HD vs NB LD
	0.12585
	0.0041209
	1.763e-06
	0.10457
	0.051339
	3.2682e-09
	0.019898
	0.00084868

	MBRNB HD vs NB LD
	/
	/
	1.2254e-07
	0.0003467
	0.92473
	0.0049012
	0.020573
	0.0049012

	RSNB HD vs NB LD
	/
	0.18083
	0.040038
	0.60141
	0.18083
	0.00011633
	0.00031248
	0.0021981

	NBRNB HD vs NB LD
	/
	/
	0.90334
	0.081547
	0.3415
	0.081547
	0.00015625
	0.0016493

	AEBP HD vs NB HD
	0.00016683
	3.0748e-10
	0.17874
	3.1669e-05
	1.0871e-07
	6.0648e-12
	1.0246e-13
	6.7024e-13

	MFRBP HD vs NB HD
	1.6111e-05
	4.8014e-10
	0.001114
	0.12091
	0.00045884
	4.3184e-26
	8.904e-16
	1.093e-09

	MBRBP HD vs NB HD
	/
	2.7148e-12
	0.25879
	0.53389
	0.42789
	2.0476e-12
	1.6466e-10
	8.4895e-09

	RSBP HD vs NB HD
	/
	4.2257e-12
	0.00059423
	1.9465e-05
	0.00098861
	0.16576
	2.5304e-09
	2.5304e-09

	NBRBP HD vs NB HD
	/
	0.00038576
	6.6754e-05
	0.00029036
	0.060758
	5.9381e-06
	6.6572e-10
	3.2059e-09

	AEBP LD vs NB LD
	/
	/
	0.82048
	0.82048
	0.82048
	0.82048
	0.017315
	3.1178e-09

	MFRBP LD vs NB LD
	0.207
	0.00015651
	0.00014663
	0.19541
	0.40989
	0.0014723
	0.5402
	0.084421

	MBRBP LD vs NB LD
	/
	3.4556e-09
	7.7732e-11
	3.3474e-05
	0.2657
	0.078612
	7.1191e-07
	2.5134e-06

	RSBP LD vs NB LD
	/
	4.7418e-11
	2.5546e-09
	0.037033
	0.99654
	0.0014614
	0.0035966
	0.535

	NBRBP LD vs NB LD
	/
	/
	0.051011
	0.0017366
	0.023926
	0.4374
	3.5127e-09
	6.1163e-07



Supplementary Table 1A: First section: P-values of the comparison between PEI and PLO coatings. Second section: P-values of the comparison between BP HD and BP LD features. Third section: P-values of the comparison between NB HD and NB LD features. Fourth section: P-values of the comparison between BP HD and NB HD features. Fifth section: P-values of the comparison between BP LD and NB LD features.

DIV
BP HD vs BP LD
BP HD vs NB HD
BP HD vs NB LD
BP LD vs NB HD
BP LD vs NB LD
NB HD vs NB LD
MFR
0.0007
<0.0001
<0.0001
0.287
>0.9999
0.057
MBR
0.4279
0.0001
0.0461
<0.0001
<0.0001
0.1863
BD
0.5595
0.0513
<0.0001
<0.0001
<0.0001
0.3755
RS
>0.9999
>0.9999
<0.0001
>0.9999
<0.0001
<0.0001
MFIB
>0.9999
0.0017
<0.0001
0.0192
<0.0001
0.3976
NBR
>0.9999
0.0151
<0.0001
0.1147
<0.0001
0.3122
NBD
>0.9999
0.9115
<0.0001
0.5219
<0.0001
0.0002
STHpeak
>0.9999
0.0368
0.0084
>0.9999
0.5843
>0.9999

Supplementary Table 1B: P-values of the comparison between all conditions at their DIV max.













