{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":70393,"n_cols":10,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["model","scenario","region","variable","unit","2010","2020","2030","2040","2050"]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",1.866377077,3.768540359,5.581208145,6.722422549,6.360651517]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",229.51487227,213.70073307,203.149324736,179.111674596,137.258359734]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",82.752772589,60.700786595,74.533050355,72.792306962,60.424021863]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Nuclear","GW/yr",4.329571495,17.312833272,22.617401068,23.996317155,20.329444019]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",19.845887238,46.339752346,54.553408488,52.582261228,43.01939244]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.241516095,2.182479496,5.268053955,7.427999976]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Solar|PV","GW/yr",0.961168189,17.241951258,32.768162096,40.774067574,42.696597227]
["GCAM","Base","ASIA","Capacity Additions|Electricity|Wind","GW/yr",15.643007388,22.407701674,37.716131595,45.805752357,44.398935827]
["GCAM","Base","ASIA","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity|Electricity|Biomass|w/o CCS","GW",3.320771894,6.843501475,13.98438689,22.611138462,29.132728465]
["GCAM","Base","ASIA","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity|Electricity|Coal|w/o CCS","GW",633.333452239,1003.242963624,1306.195935987,1525.70741542,1679.064519922]
["GCAM","Base","ASIA","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity|Electricity|Gas|w/o CCS","GW",150.809593801,262.46960141,381.11618631,491.04503104,582.86627975]
["GCAM","Base","ASIA","Capacity|Electricity|Hydro","GW",140.501835209,148.324510093,156.175335349,168.754368039,186.061941122]
["GCAM","Base","ASIA","Capacity|Electricity|Nuclear","GW",37.264167232,65.218133774,101.227124196,139.092455184,174.124884044]
["GCAM","Base","ASIA","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","ASIA","Capacity|Electricity|Oil|w/o CCS","GW",194.739186974,241.78628789,283.828668005,312.025209307,340.29483764]
["GCAM","Base","ASIA","Capacity|Electricity|Solar|CSP","GW",0,0.353540655,3.448101412,12.466037788,26.178304639]
["GCAM","Base","ASIA","Capacity|Electricity|Solar|PV","GW",1.143816591,31.886443015,105.313573562,214.914878431,333.437281484]
["GCAM","Base","ASIA","Capacity|Electricity|Wind","GW",18.059051186,54.58648994,120.06114861,190.327858383,241.399805157]
["GCAM","Base","ASIA","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Concentration|CH4","ppb",15057.84,16182.48,17825.76,19557.36,20990.96]
["GCAM","Base","ASIA","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","ASIA","Concentration|N2O","ppb",2616.112,2686.872,2765.336,2851.088,2942.856]
["GCAM","Base","ASIA","Emissions|CO2","Mt CO2/yr",19706.70233398,25732.0980769,32427.2649118,37257.4191094,40527.0656015]
["GCAM","Base","ASIA","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",10356.91204497,15545.4691945,19626.6770597,22241.5167738,23862.2603075]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",10724.15561597,16076.0563595,20271.7669397,22930.3606338,24551.7196875]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",-5.2708e-06,2.22097e-05,3.0166e-05,-3.631e-05,3.7799e-05]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",9412.173677573,13889.575843967,17169.680073963,19095.92615338,20141.38561821]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",666.00476233,1181.86190442,1703.06902367,2165.61875263,2537.49837111]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",278.7336068,474.03128628,753.90364952,979.70617005,1182.89755897]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",367.2435714,530.5871603,645.089881,688.8438617,689.4593776]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",18410.6460997,26222.2458999,32869.364205,37440.6107191,40738.6950891]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",7477.8521801,9748.29426267,11630.9078287,12714.0635006,13284.3082332]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",5089.99648256,6440.30153623,7435.3512724,7961.96578405,8157.89456933]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",786.794910896,1262.21563863,1707.18290958,1940.68086272,2062.93902868]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",1601.06078707,2045.77708804,2488.37364531,2811.41685504,3063.47463531]
["GCAM","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",21289.7062038,32019.420807,40865.1093208,46967.7983123,51316.1690868]
["GCAM","Base","ASIA","Emissions|CO2|Land Use","Mt CO2/yr",1296.056232751,-490.147822611,-442.099293617,-183.191605049,-211.629481192]
["GCAM","Base","ASIA","Final Energy","EJ/yr",132.098459997,175.566710071,215.810300717,244.126185129,263.557173747]
["GCAM","Base","ASIA","Final Energy|Electricity","EJ/yr",20.62690329,33.2344819,45.653636421,56.69279619,66.019368389]
["GCAM","Base","ASIA","Final Energy|Gases","EJ/yr",8.249331486,14.063314256,19.772342075,23.760878422,26.611054973]
["GCAM","Base","ASIA","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Final Energy|Heat","EJ/yr",3.0529687,4.4048133,5.3412084,5.6816913,5.6656475]
["GCAM","Base","ASIA","Final Energy|Hydrogen","EJ/yr",0,0.08803276,0.248776976,0.47524675,0.768154505]
["GCAM","Base","ASIA","Final Energy|Industry","EJ/yr",72.133937079,99.896227854,122.483179825,137.542580987,146.758041467]
["GCAM","Base","ASIA","Final Energy|Liquids","EJ/yr",41.26959203,56.590263605,72.586640969,84.043501794,92.908102857]
["GCAM","Base","ASIA","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Final Energy|Residential and Commercial","EJ/yr",37.58757245,47.004492239,58.402831273,66.94520321,73.323708458]
["GCAM","Base","ASIA","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Final Energy|Solids","EJ/yr",39.984766329,53.450157333,62.221083445,65.989088663,66.034063775]
["GCAM","Base","ASIA","Final Energy|Solids|Biomass","EJ/yr",22.316849289,18.521061773,16.200766965,14.464056353,12.493851725]
["GCAM","Base","ASIA","Final Energy|Solids|Biomass|Traditional","EJ/yr",18.91489816,13.73564691,9.9866124,7.482982,5.55078177]
["GCAM","Base","ASIA","Final Energy|Solids|Coal","EJ/yr",36.5828152,48.66474247,56.00692888,59.00801431,59.09099382]
["GCAM","Base","ASIA","Final Energy|Transportation","EJ/yr",20.753906165,26.739945525,32.924490978,37.61531272,41.505255045]
["GCAM","Base","ASIA","Forcing","W/m2",14.90176,18.0636,22.11992,26.70136,31.59048]
["GCAM","Base","ASIA","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","ASIA","GDP|MER","billion US$2010/yr",9076.2487829,17558.3786235,28274.3349387,38203.7131843,47851.9097298]
["GCAM","Base","ASIA","GDP|PPP","billion US$2010/yr",20244.6583581,39941.5036559,65402.3733836,89683.8436821,114015.460166]
["GCAM","Base","ASIA","Land Cover|Cropland|Energy Crops","million ha",0,3.669201099,4.987745292,6.889428365,10.200613999]
["GCAM","Base","ASIA","Population","million",3678.493,4013.19,4269.945,4432.421,4498.859]
["GCAM","Base","ASIA","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","ASIA","Price|Primary Energy|Coal","US$2010/GJ",16.79633592,17.0775268,17.50809872,18.06394296,18.74772104]
["GCAM","Base","ASIA","Price|Primary Energy|Gas","US$2010/GJ",45.22,45.9489464,47.0887488,49.894456,53.6642536]
["GCAM","Base","ASIA","Price|Primary Energy|Oil","US$2010/GJ",88.6318137,92.1565835,97.4341774,101.4188346,102.7935549]
["GCAM","Base","ASIA","Price|Secondary Energy|Electricity","US$2010/GJ",271.4732958,245.3668854,245.7296467,246.3969001,247.6562448]
["GCAM","Base","ASIA","Primary Energy","EJ/yr",185.280164753,253.837750434,318.824182987,366.714148919,400.585640608]
["GCAM","Base","ASIA","Primary Energy|Biomass","EJ/yr",23.19311446,21.86175361,23.3367304,26.292496,26.18859977]
["GCAM","Base","ASIA","Primary Energy|Biomass|Electricity","EJ/yr",0.08377909,0.17265333,0.352808655,0.57045189,0.73498378]
["GCAM","Base","ASIA","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Biomass|Gases","EJ/yr",0.41151176,0.829439203,1.148798122,1.391845679,1.47866947]
["GCAM","Base","ASIA","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.007402432,0.019508284,0.034612136,0.049520796]
["GCAM","Base","ASIA","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Biomass|Liquids","EJ/yr",0.0156704,1.79076412,4.67312074,8.47734681,9.836811613]
["GCAM","Base","ASIA","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Biomass|Traditional","EJ/yr",18.91489816,13.73564691,9.9866124,7.482982,5.55078177]
["GCAM","Base","ASIA","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Biomass|w/o CCS","EJ/yr",23.19311446,21.86175361,23.3367304,26.292496,26.18859977]
["GCAM","Base","ASIA","Primary Energy|Coal","EJ/yr",87.3239386,125.553191,158.859719,185.498242,207.87552]
["GCAM","Base","ASIA","Primary Energy|Coal|Electricity","EJ/yr",15.9782428,25.31061608,32.953755787,38.49176724,42.36078296]
["GCAM","Base","ASIA","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.031439737,0.092388357,0.189447991,0.332567245]
["GCAM","Base","ASIA","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Coal|w/o CCS","EJ/yr",87.3239386,125.553191,158.859719,185.498242,207.87552]
["GCAM","Base","ASIA","Primary Energy|Fossil","EJ/yr",148.14127508,213.8217815,273.6594178,316.6992362,349.512708]
["GCAM","Base","ASIA","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Fossil|w/o CCS","EJ/yr",148.14127508,213.8217815,273.6594178,316.6992362,349.512708]
["GCAM","Base","ASIA","Primary Energy|Gas","EJ/yr",14.897151,27.482332,44.60204,61.63534,75.74191]
["GCAM","Base","ASIA","Primary Energy|Gas|Electricity","EJ/yr",2.7316425,5.6780118,8.7237819,11.6397163,14.1092945]
["GCAM","Base","ASIA","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.08478922,0.234533624,0.427815295,0.651751038]
["GCAM","Base","ASIA","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Gas|w/o CCS","EJ/yr",14.897151,27.482332,44.60204,61.63534,75.74191]
["GCAM","Base","ASIA","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Hydro","EJ/yr",3.5446927,3.7420494,3.9401163,4.2574702,4.6941195]
["GCAM","Base","ASIA","Primary Energy|Non-Biomass Renewables","EJ/yr",3.79110128,4.725041889,6.379785713,8.464925298,10.560426116]
["GCAM","Base","ASIA","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Oil","EJ/yr",45.92018548,60.7862585,70.1976588,69.5656542,65.895278]
["GCAM","Base","ASIA","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Oil|w/o CCS","EJ/yr",45.92018548,60.7862585,70.1976588,69.5656542,65.895278]
["GCAM","Base","ASIA","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Primary Energy|Solar","EJ/yr",7.21428E-3,0.208345009,0.697995288,1.446452905,2.288298836]
["GCAM","Base","ASIA","Primary Energy|Wind","EJ/yr",0.2391943,0.77464748,1.741674125,2.761002193,3.57800778]
["GCAM","Base","ASIA","Resource|Cumulative Extraction|Coal","EJ",420.592218,1005.659995,1740.2443725,2635.233581,3719.398796]
["GCAM","Base","ASIA","Resource|Cumulative Extraction|Gas","EJ",72.8645475,216.933898,420.8894335,768.3516785,1141.8898385]
["GCAM","Base","ASIA","Resource|Cumulative Extraction|Oil","EJ",82.4589795,319.4330229,584.80323425,796.97962875,966.1198332]
["GCAM","Base","ASIA","Secondary Energy|Electricity","EJ/yr",24.326561696,39.486910637,54.403885214,67.541529028,78.382792204]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Biomass","EJ/yr",0.08377909,0.17265333,0.352808655,0.57045189,0.73498378]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.08377909,0.17265333,0.352808655,0.57045189,0.73498378]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Coal","EJ/yr",15.978243,25.31061608,32.953755787,38.49176724,42.36078296]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",15.978243,25.31061608,32.953755787,38.49176724,42.36078296]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Fossil","EJ/yr",19.324015026,32.462704407,44.310696961,53.766313262,61.023468908]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",19.324015026,32.462704407,44.310696961,53.766313262,61.023468908]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Gas","EJ/yr",2.731642523,5.678012827,8.723960776,11.641682424,14.112823245]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",2.731642523,5.678012827,8.723960776,11.641682424,14.112823245]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0700198,0.27200758,0.426856066,0.549458461,0.593399658]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Hydro","EJ/yr",3.5446927,3.7420494,3.9401163,4.2574702,4.6941195]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",3.86112108,5.000505739,6.867310863,9.256986171,11.682257404]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Nuclear","EJ/yr",1.0576465,1.85104716,2.87306873,3.9477777,4.94208211]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Oil","EJ/yr",0.6141295,1.4740755,2.6329804,3.6328636,4.5498627]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.6141295,1.4740755,2.6329804,3.6328636,4.5498627]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Solar","EJ/yr",7.21428E-3,0.211801279,0.758664372,1.689055317,2.816730466]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,3.45627E-3,0.060669084,0.242602412,0.52843163]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Solar|PV","EJ/yr",7.21428E-3,0.208345009,0.697995288,1.446452905,2.288298836]
["GCAM","Base","ASIA","Secondary Energy|Electricity|Wind","EJ/yr",0.2391943,0.77464748,1.741674125,2.761002193,3.57800778]
["GCAM","Base","ASIA","Secondary Energy|Gases","EJ/yr",15.31604324,26.72279493,38.0600297,47.0766859,54.00281651]
["GCAM","Base","ASIA","Secondary Energy|Gases|Biomass","EJ/yr",0.30641165,0.61760116,0.86473479,1.0592429,1.13787601]
["GCAM","Base","ASIA","Secondary Energy|Gases|Coal","EJ/yr",0.17252059,0.42001977,0.78922491,1.455563,2.7375405]
["GCAM","Base","ASIA","Secondary Energy|Gases|Natural Gas","EJ/yr",14.837111,25.685174,36.40607,44.56188,50.1274]
["GCAM","Base","ASIA","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen","EJ/yr",0,0.088033017,0.248775894,0.475245941,0.768154101]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.00333831,0.00897352,0.01626735,0.02376956]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.00333831,0.00897352,0.01626735,0.02376956]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.02012153,0.06032921,0.12636215,0.22614592]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.02012153,0.06032921,0.12636215,0.22614592]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.007686467,0.020318134,0.037854511,0.060756569]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.05347765,0.15022467,0.27835273,0.431541092]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.05347765,0.15022467,0.27835273,0.431541092]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,0.00340906,8.93036E-3,0.0164092,0.02594096]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Liquids","EJ/yr",43.37750468,60.111744859,78.084605179,91.108694505,101.37671758]
["GCAM","Base","ASIA","Secondary Energy|Liquids|Biomass","EJ/yr",0.00761808,0.88570239,2.3349324,4.28283131,5.046425771]
["GCAM","Base","ASIA","Secondary Energy|Liquids|Coal","EJ/yr",0,0.87563253,4.65472557,10.72868648,18.16614453]
["GCAM","Base","ASIA","Secondary Energy|Liquids|Gas","EJ/yr",0.0363013,0.93456016,4.69356742,10.00549198,15.17773718]
["GCAM","Base","ASIA","Secondary Energy|Liquids|Oil","EJ/yr",43.232583,57.3290405,66.3212488,65.9655355,62.85568777]
["GCAM","Base","ASIA","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Temperature|Global Mean","?C",6.596088,8.13696,10.16008,12.52112,15.10656]
["GCAM","Base","ASIA","Water Consumption|Electricity","km3/yr",26.24000137,33.073142906,39.161697063,44.754104791,49.871883858]
["GCAM","Base","ASIA","Water Consumption|Electricity|Biomass","km3/yr",0.03240881,0.069181743,0.138993445,0.221778997,0.279775371]
["GCAM","Base","ASIA","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.03240881,0.069181743,0.138993445,0.221778997,0.279775371]
["GCAM","Base","ASIA","Water Consumption|Electricity|Coal","km3/yr",8.12824734,12.981699008,16.91892272,19.779030325,21.76250073]
["GCAM","Base","ASIA","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",8.12824734,12.981699008,16.91892272,19.779030325,21.76250073]
["GCAM","Base","ASIA","Water Consumption|Electricity|Cooling Pond","km3/yr",0.43650134,0.381155856,0.316440106,0.21620593,0.116133617]
["GCAM","Base","ASIA","Water Consumption|Electricity|Dry Cooling","km3/yr",0.00521258,0.020604504,0.03801072,0.065838979,0.098485002]
["GCAM","Base","ASIA","Water Consumption|Electricity|Fossil","km3/yr",9.16429744,14.404886547,18.734973778,21.9292252,24.185341091]
["GCAM","Base","ASIA","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",9.16429744,14.404886547,18.734973778,21.9292252,24.185341091]
["GCAM","Base","ASIA","Water Consumption|Electricity|Gas","km3/yr",0.74142331,1.07083297,1.46273514,1.809813557,2.08976556]
["GCAM","Base","ASIA","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.74142331,1.07083297,1.46273514,1.809813557,2.08976556]
["GCAM","Base","ASIA","Water Consumption|Electricity|Geothermal","km3/yr",0.08456858,0.328524785,0.515546701,0.663623731,0.71669473]
["GCAM","Base","ASIA","Water Consumption|Electricity|Hydro","km3/yr",16.738859,17.6708315,18.6061545,20.1046819,22.1666172]
["GCAM","Base","ASIA","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.08456858,0.330464445,0.549587884,0.799751982,1.013201733]
["GCAM","Base","ASIA","Water Consumption|Electricity|Nuclear","km3/yr",0.2198275,0.596806722,1.128998408,1.69305695,2.219231673]
["GCAM","Base","ASIA","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Oil","km3/yr",0.29462684,0.352354569,0.35331592,0.340381321,0.333074798]
["GCAM","Base","ASIA","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.29462684,0.352354569,0.35331592,0.340381321,0.333074798]
["GCAM","Base","ASIA","Water Consumption|Electricity|Once Through","km3/yr",0.90970356,0.855891445,0.780507471,0.631584757,0.477383792]
["GCAM","Base","ASIA","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Consumption|Electricity|Solar","km3/yr",4.001e-05,0.00291156,0.037030233,0.141738012,0.304223798]
["GCAM","Base","ASIA","Water Consumption|Electricity|Solar|CSP","km3/yr",0,0.0019397,0.034041183,0.136128251,0.296507003]
["GCAM","Base","ASIA","Water Consumption|Electricity|Solar|PV","km3/yr",4.001e-05,0.00097193,0.002989014,0.005609765,0.007716733]
["GCAM","Base","ASIA","Water Consumption|Electricity|Wet Tower","km3/yr",8.14968488,14.143687652,19.417595221,23.730183464,27.005547457]
["GCAM","Base","ASIA","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity","km3/yr",151.50085792,151.217227504,146.602340007,129.394068982,110.008593391]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Biomass","km3/yr",0.47724167,0.389156141,0.599895583,0.8464618269999999,1.042915271]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.47724167,0.389156141,0.599895583,0.8464618269999999,1.042915271]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Coal","km3/yr",131.5587926,131.271764691,124.476933047,106.00724069,85.51315506]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",131.5587926,131.271764691,124.476933047,106.00724069,85.51315506]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Cooling Pond","km3/yr",9.3785521,8.254357778,6.851264317,4.685442307,2.519894144]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.00521258,0.020604504,0.03801072,0.065838979,0.098485002]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Fossil","km3/yr",145.24236091,144.200382481,138.187943802,119.551879542,98.722428443]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",145.24236091,144.200382481,138.187943802,119.551879542,98.722428443]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Gas","km3/yr",10.75554219,11.156609187,12.048585796,12.086810756,11.916634722]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",10.75554219,11.156609187,12.048585796,12.086810756,11.916634722]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Geothermal","km3/yr",0.08456858,0.328524785,0.515546701,0.663623731,0.71669473]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.08456858,0.330464445,0.549587884,0.799751982,1.013201733]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Nuclear","km3/yr",5.69664674,6.29625249,7.26192369,8.190365867,9.222331154]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Oil","km3/yr",2.92802612,1.772008598,1.662424963,1.457828092,1.292638653]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",2.92802612,1.772008598,1.662424963,1.457828092,1.292638653]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Once Through","km3/yr",130.1612239,122.337018695,111.570399648,90.407166965,68.562872707]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Sea Cooling","km3/yr",123.71549432,228.62988869,315.14645761,387.26668518,443.92292129]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Solar","km3/yr",4.001e-05,0.00291156,0.037030233,0.141738012,0.304223798]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.0019397,0.034041183,0.136128251,0.296507003]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Solar|PV","km3/yr",4.001e-05,0.00097193,0.002989014,0.005609765,0.007716733]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Wet Tower","km3/yr",11.95582932,20.604274579,28.139676285,34.23001096,38.819624746]
["GCAM","Base","ASIA","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",2.55479135,2.404026232,1.68059111,1.432405544,1.121922842]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0.085045662,2.089606006,1.680569627,1.677904022,1.653029276]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",3.243178605,7.5390957,6.277755422,5.774089263,5.012925292]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Nuclear","GW/yr",0.592085588,0.133848195,0.186490783,0.25631807,0.318418774]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",5.007981355,19.83179953,13.90424943,11.99306507,10.17320301]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.007528518,0.058795531,0.141512016,0.22917279]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Solar|PV","GW/yr",0,0.352680746,0.514307617,0.712369197,0.932418189]
["GCAM","Base","Brazil","Capacity Additions|Electricity|Wind","GW/yr",0.566410874,0.989418513,1.234262913,1.666739737,2.034323556]
["GCAM","Base","Brazil","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity|Electricity|Biomass|w/o CCS","GW",4.494149543,7.226939054,9.494371512,10.690013,10.65745894]
["GCAM","Base","Brazil","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity|Electricity|Coal|w/o CCS","GW",1.617861333,4.361721525,7.497611856,10.47813213,13.46300656]
["GCAM","Base","Brazil","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity|Electricity|Gas|w/o CCS","GW",6.479540049,16.26774956,27.94740297,38.17581019,47.02449899]
["GCAM","Base","Brazil","Capacity|Electricity|Hydro","GW",57.54693049,59.4467434,61.34655632,63.97331621,67.32741946]
["GCAM","Base","Brazil","Capacity|Electricity|Nuclear","GW",1.842081713,1.764676701,1.827653757,1.879879785,2.067644033]
["GCAM","Base","Brazil","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Brazil","Capacity|Electricity|Oil|w/o CCS","GW",18.33900939,52.47304668,69.89666572,82.01420599,92.00738838]
["GCAM","Base","Brazil","Capacity|Electricity|Solar|CSP","GW",0,0.008592331,0.0943404,0.337338716,0.746445575]
["GCAM","Base","Brazil","Capacity|Electricity|Solar|PV","GW",0,1.45792618,4.610640855,9.662629059,16.17570713]
["GCAM","Base","Brazil","Capacity|Electricity|Wind","GW",0.591703208,1.855473815,4.082987283,6.652143582,9.17727258]
["GCAM","Base","Brazil","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Concentration|CH4","ppb",1882.23,2022.81,2228.22,2444.67,2623.87]
["GCAM","Base","Brazil","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","Brazil","Concentration|N2O","ppb",327.014,335.859,345.667,356.386,367.857]
["GCAM","Base","Brazil","Emissions|CO2","Mt CO2/yr",1403.90333,1104.254563,1381.668899,1668.273876,1875.01834]
["GCAM","Base","Brazil","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",78.18736358,271.1148143,459.8130704,608.5382592,733.8668752]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",78.18736358,271.1148143,459.8130704,608.5382592,733.8668752]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",-2.83E-6,-3.56e-05,-2.5e-05,8.93e-05,-1.96e-05]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",26.78359933,60.1862998,95.97069401,127.3399262,157.1906762]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",28.8653244,73.67663684,125.2328285,168.6940305,205.0608862]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",22.53844267,137.2519119,238.6095674,312.5041932,371.6152645]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",464.4809344,895.4693236,1220.967938,1509.587298,1809.727024]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",412.3465832,580.4590845,665.1966027,721.8631627,763.2310734]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",157.0652649,242.2331087,280.2006837,303.0655889,317.5776606]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",22.27673547,45.73337685,56.366841,63.24103206,68.69154029]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",233.0045828,292.4925989,328.629078,355.5565418,376.9618725]
["GCAM","Base","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",130.3217148,586.1251621,1015.584694,1396.262374,1780.362831]
["GCAM","Base","Brazil","Emissions|CO2|Land Use","Mt CO2/yr",939.422396,208.7852391,160.7009603,158.6865788,65.29131649]
["GCAM","Base","Brazil","Final Energy","EJ/yr",10.06055115,12.97365899,15.22332813,16.92477846,18.26689339]
["GCAM","Base","Brazil","Final Energy|Electricity","EJ/yr",1.51586032,2.240144984,3.059848049,3.802325984,4.494071212]
["GCAM","Base","Brazil","Final Energy|Gases","EJ/yr",0.577272294,0.751054885,1.013080169,1.285350614,1.579401622]
["GCAM","Base","Brazil","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Final Energy|Hydrogen","EJ/yr",0,0.008646733,0.029513589,0.059147592,0.093798098]
["GCAM","Base","Brazil","Final Energy|Industry","EJ/yr",5.45580669,6.95577019,8.10474955,8.87730837,9.374959761]
["GCAM","Base","Brazil","Final Energy|Liquids","EJ/yr",4.920385169,7.267461127,8.354705681,9.081169092,9.615903733]
["GCAM","Base","Brazil","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Final Energy|Residential and Commercial","EJ/yr",1.363749674,1.924688978,2.470489104,2.939749539,3.371628408]
["GCAM","Base","Brazil","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Final Energy|Solids","EJ/yr",2.74250217,2.50988636,2.60934134,2.56906798,2.38265885]
["GCAM","Base","Brazil","Final Energy|Solids|Biomass","EJ/yr",2.57393137,2.1859544,2.16838805,2.04677505,1.80652366]
["GCAM","Base","Brazil","Final Energy|Solids|Biomass|Traditional","EJ/yr",0.3045312,0.1964649,0.1568393,0.1277172,0.10105987]
["GCAM","Base","Brazil","Final Energy|Solids|Coal","EJ/yr",0.473102,0.52039686,0.59779259,0.65001013,0.67719506]
["GCAM","Base","Brazil","Final Energy|Transportation","EJ/yr",3.240994789,4.093199821,4.648089474,5.107720553,5.520305216]
["GCAM","Base","Brazil","Forcing","W/m2",1.86272,2.25795,2.76499,3.33767,3.94881]
["GCAM","Base","Brazil","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","Brazil","GDP|MER","billion US$2010/yr",1196.020433,1710.995083,2295.413092,2849.700217,3412.239267]
["GCAM","Base","Brazil","GDP|PPP","billion US$2010/yr",2150.863468,3076.968182,4127.956367,5124.758675,6136.400834]
["GCAM","Base","Brazil","Land Cover|Cropland|Energy Crops","million ha",0,0.934008602,1.323171138,1.813831594,2.722050075]
["GCAM","Base","Brazil","Population","million",194.946,210.743,222.819,229.841,231.868]
["GCAM","Base","Brazil","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","Brazil","Price|Primary Energy|Coal","US$2010/GJ",2.09954199,2.13469085,2.18851234,2.25799287,2.34346513]
["GCAM","Base","Brazil","Price|Primary Energy|Gas","US$2010/GJ",5.6525,5.7436183,5.8860936,6.236807,6.7080317]
["GCAM","Base","Brazil","Price|Primary Energy|Oil","US$2010/GJ",11.1178538,11.5519012,12.192604,12.6689644,12.835051]
["GCAM","Base","Brazil","Price|Secondary Energy|Electricity","US$2010/GJ",43.530387,39.273893,37.538737,36.38272,35.402738]
["GCAM","Base","Brazil","Primary Energy","EJ/yr",11.37737984,17.15483302,21.38602028,25.00714526,28.17757564]
["GCAM","Base","Brazil","Primary Energy|Biomass","EJ/yr",2.8166712,2.9539349,3.5515293,4.1185472,4.22976987]
["GCAM","Base","Brazil","Primary Energy|Biomass|Electricity","EJ/yr",0.113382,0.182327,0.2395316,0.2696962,0.2688749]
["GCAM","Base","Brazil","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Biomass|Gases","EJ/yr",0,0.000222414,0.000764298,0.00192575,0.00394957]
["GCAM","Base","Brazil","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.000692657,2.21061E-3,0.00412174,5.80344E-3]
["GCAM","Base","Brazil","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Biomass|Liquids","EJ/yr",0,0.251829,0.6598861,1.2352227,1.5824866]
["GCAM","Base","Brazil","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Biomass|Traditional","EJ/yr",0.3045312,0.1964649,0.1568393,0.1277172,0.10105987]
["GCAM","Base","Brazil","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Biomass|w/o CCS","EJ/yr",2.8166712,2.9539349,3.5515293,4.1185472,4.22976987]
["GCAM","Base","Brazil","Primary Energy|Coal","EJ/yr",0.606886,1.04965,2.11751,3.7437,6.05873]
["GCAM","Base","Brazil","Primary Energy|Coal|Electricity","EJ/yr",0.0408167,0.110041,0.18915575,0.2643507,0.3396555]
["GCAM","Base","Brazil","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.00294186,0.0104691,0.0225602,0.0389743]
["GCAM","Base","Brazil","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Coal|w/o CCS","EJ/yr",0.606886,1.04965,2.11751,3.7437,6.05873]
["GCAM","Base","Brazil","Primary Energy|Fossil","EJ/yr",6.23204,11.159064,14.566903,17.57877,20.66167]
["GCAM","Base","Brazil","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Fossil|w/o CCS","EJ/yr",6.23204,11.159064,14.566903,17.57877,20.66167]
["GCAM","Base","Brazil","Primary Energy|Gas","EJ/yr",0.963435,1.86285,3.31857,4.99632,6.74321]
["GCAM","Base","Brazil","Primary Energy|Gas|Electricity","EJ/yr",0.1313097,0.374831,0.6652164,0.9225808,1.1465498]
["GCAM","Base","Brazil","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.00864059,0.0287434,0.0549485,0.082013]
["GCAM","Base","Brazil","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Gas|w/o CCS","EJ/yr",0.963435,1.86285,3.31857,4.99632,6.74321]
["GCAM","Base","Brazil","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Hydro","EJ/yr",1.45184,1.49977,1.5477,1.61397,1.69859]
["GCAM","Base","Brazil","Primary Energy|Non-Biomass Renewables","EJ/yr",1.45967718,1.536944683,1.64118053,1.78252518,1.955908018]
["GCAM","Base","Brazil","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Oil","EJ/yr",4.661719,8.246564,9.130823,8.83875,7.85973]
["GCAM","Base","Brazil","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Oil|w/o CCS","EJ/yr",4.661719,8.246564,9.130823,8.83875,7.85973]
["GCAM","Base","Brazil","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Primary Energy|Solar","EJ/yr",0,0.010843613,0.034250429,0.072055043,0.121293109]
["GCAM","Base","Brazil","Primary Energy|Wind","EJ/yr",0.00783718,0.02633107,0.059230101,0.096500137,0.136024909]
["GCAM","Base","Brazil","Resource|Cumulative Extraction|Coal","EJ",0.4171095,1.116077,1.9841675,3.0337185,4.2968235]
["GCAM","Base","Brazil","Resource|Cumulative Extraction|Gas","EJ",2.613885,5.76191,10.202935,18.095915,28.203665]
["GCAM","Base","Brazil","Resource|Cumulative Extraction|Oil","EJ",23.71825,43.941185,74.615345,107.93054,137.28115]
["GCAM","Base","Brazil","Secondary Energy|Electricity","EJ/yr",1.85530218,2.733165003,3.695927832,4.547184502,5.319959178]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Biomass","EJ/yr",0.113382,0.182327,0.2395316,0.2696962,0.2688749]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.113382,0.182327,0.2395316,0.2696962,0.2688749]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Coal","EJ/yr",0.0408167,0.110041,0.18915575,0.2643507,0.3396555]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",0.0408167,0.110041,0.18915575,0.2643507,0.3396555]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Fossil","EJ/yr",0.2299603,0.95536201,1.73405219,2.381156645,2.941142789]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",0.2299603,0.95536201,1.73405219,2.381156645,2.941142789]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Gas","EJ/yr",0.1313097,0.37483101,0.66521644,0.922580945,1.146550289]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",0.1313097,0.37483101,0.66521644,0.922580945,1.146550289]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Geothermal","EJ/yr",0,0.00836155,0.02760751,0.05386944,0.080317301]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Hydro","EJ/yr",1.45184,1.49977,1.5477,1.61397,1.69859]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",1.45967718,1.545390233,1.670470842,1.842976157,2.051256789]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Nuclear","EJ/yr",0.0522827,0.05008576,0.0518732,0.0533555,0.0586847]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Oil","EJ/yr",0.0578339,0.47049,0.87968,1.194225,1.454937]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.0578339,0.47049,0.87968,1.194225,1.454937]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Solar","EJ/yr",0,0.010927613,0.035933231,0.07863658,0.136324579]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,8.4e-05,1.682802E-3,0.006581537,0.01503147]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Solar|PV","EJ/yr",0,0.010843613,0.034250429,0.072055043,0.121293109]
["GCAM","Base","Brazil","Secondary Energy|Electricity|Wind","EJ/yr",0.00783718,0.02633107,0.059230101,0.096500137,0.136024909]
["GCAM","Base","Brazil","Secondary Energy|Gases","EJ/yr",0.963435,1.65455634,2.4699891,3.20291836,3.8779533]
["GCAM","Base","Brazil","Secondary Energy|Gases|Biomass","EJ/yr",0,1.66E-4,0.000575,0.00146556,3.0393E-3]
["GCAM","Base","Brazil","Secondary Energy|Gases|Coal","EJ/yr",0,0.00385034,0.0150541,0.0454828,0.121984]
["GCAM","Base","Brazil","Secondary Energy|Gases|Natural Gas","EJ/yr",0.963435,1.65054,2.45436,3.15597,3.75293]
["GCAM","Base","Brazil","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen","EJ/yr",0,0.00864626,0.029513586,0.059147556,0.093798014]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.000312,1.01688E-3,0.00193722,0.00278565]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.000312,1.01688E-3,0.00193722,0.00278565]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.00188279,0.00683634,0.0150476,0.0265025]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.00188279,0.00683634,0.0150476,0.0265025]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.000732,2.373076E-3,0.004675776,0.007432324]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.00540047,0.01827535,0.0355329,0.0540374]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.00540047,0.01827535,0.0355329,0.0540374]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,3.19E-4,1.01194E-3,0.00195406,0.00304014]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Liquids","EJ/yr",5.0771895,8.2223638,10.01479194,11.25536451,12.20135867]
["GCAM","Base","Brazil","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.1250778,0.3302111,0.6246146,0.8124876]
["GCAM","Base","Brazil","Secondary Energy|Liquids|Coal","EJ/yr",0,0.104441,0.480868,1.1384408,2.1236965]
["GCAM","Base","Brazil","Secondary Energy|Liquids|Gas","EJ/yr",0,0.106981,0.482247,1.057951,1.7491893]
["GCAM","Base","Brazil","Secondary Energy|Liquids|Oil","EJ/yr",4.48847,7.885171,8.720331,8.431148,7.510298]
["GCAM","Base","Brazil","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Temperature|Global Mean","?C",0.824511,1.01712,1.27001,1.56514,1.88832]
["GCAM","Base","Brazil","Water Consumption|Electricity","km3/yr",7.0493781,7.464882204,7.855503365,8.313721865,8.839514943]
["GCAM","Base","Brazil","Water Consumption|Electricity|Biomass","km3/yr",0.05586702,0.092760345,0.120640826,0.134414155,0.132125386]
["GCAM","Base","Brazil","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.05586702,0.092760345,0.120640826,0.134414155,0.132125386]
["GCAM","Base","Brazil","Water Consumption|Electricity|Coal","km3/yr",0.02435055,0.069225366,0.118342162,0.164317567,0.20968508]
["GCAM","Base","Brazil","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.02435055,0.069225366,0.118342162,0.164317567,0.20968508]
["GCAM","Base","Brazil","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Dry Cooling","km3/yr",0,0.00063063,0.002228324,0.004687081,0.007523769]
["GCAM","Base","Brazil","Water Consumption|Electricity|Fossil","km3/yr",0.1054862,0.248769428,0.359472651,0.454897123,0.542578127]
["GCAM","Base","Brazil","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",0.1054862,0.248769428,0.359472651,0.454897123,0.542578127]
["GCAM","Base","Brazil","Water Consumption|Electricity|Gas","km3/yr",0.04007264,0.088328875,0.145975666,0.195597477,0.238121409]
["GCAM","Base","Brazil","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.04007264,0.088328875,0.145975666,0.195597477,0.238121409]
["GCAM","Base","Brazil","Water Consumption|Electricity|Geothermal","km3/yr",0,0.01009842,0.033343724,0.065062281,0.09700535]
["GCAM","Base","Brazil","Water Consumption|Electricity|Hydro","km3/yr",6.85591,7.08224,7.30856,7.62153,8.02112]
["GCAM","Base","Brazil","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,0.01014555,0.034287824,0.068755176,0.105439124]
["GCAM","Base","Brazil","Water Consumption|Electricity|Nuclear","km3/yr",0.03211488,0.030952141,0.032494591,0.034032191,0.038110996]
["GCAM","Base","Brazil","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Oil","km3/yr",0.04106301,0.091215187,0.095154823,0.094982079,0.094771638]
["GCAM","Base","Brazil","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.04106301,0.091215187,0.095154823,0.094982079,0.094771638]
["GCAM","Base","Brazil","Water Consumption|Electricity|Once Through","km3/yr",0.0127618,0.019695183,0.025143847,0.028808868,0.031330518]
["GCAM","Base","Brazil","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Consumption|Electricity|Solar","km3/yr",0,6.19E-5,0.000991573,0.003786115,0.008575084]
["GCAM","Base","Brazil","Water Consumption|Electricity|Solar|CSP","km3/yr",0,4.71E-5,0.0009441,0.003692895,0.008433774]
["GCAM","Base","Brazil","Water Consumption|Electricity|Solar|PV","km3/yr",0,1.47E-5,4.75e-05,9.32e-05,0.00014131]
["GCAM","Base","Brazil","Water Consumption|Electricity|Wet Tower","km3/yr",0.1807063,0.362301651,0.519523721,0.658602696,0.779399346]
["GCAM","Base","Brazil","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity","km3/yr",1.9367324,3.072563917,4.020212544,4.727315393,5.28092054]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Biomass","km3/yr",0.6053813,0.8701005,1.07387933,1.15505262,1.11019694]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.6053813,0.8701005,1.07387933,1.15505262,1.11019694]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Coal","km3/yr",0.2307498,0.526104,0.85714608,1.16476246,1.47106044]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",0.2307498,0.526104,0.85714608,1.16476246,1.47106044]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0.00063063,0.002228324,0.004687081,0.007523769]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Fossil","km3/yr",0.9742703,1.85663257,2.57938385,3.18220432,3.73516986]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",0.9742703,1.85663257,2.57938385,3.18220432,3.73516986]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Gas","km3/yr",0.419313,0.73983227,1.12344399,1.43938874,1.70548685]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",0.419313,0.73983227,1.12344399,1.43938874,1.70548685]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0.01009842,0.033343724,0.065062281,0.09700535]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0,0.01014555,0.034287824,0.068755176,0.105439124]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Nuclear","km3/yr",0.3570808,0.335670557,0.332614067,0.321210057,0.329973306]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Oil","km3/yr",0.3242075,0.5906963,0.59879378,0.57805312,0.55862257]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",0.3242075,0.5906963,0.59879378,0.57805312,0.55862257]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Once Through","km3/yr",1.660172,2.537816092,3.273393492,3.800083092,4.201160991]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Sea Cooling","km3/yr",0.7115015,0.737223872,0.739182122,0.676982652,0.602601072]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Solar","km3/yr",0,6.19E-5,0.000991573,0.003786115,0.008575084]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,4.71E-5,0.0009441,0.003692895,0.008433774]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Solar|PV","km3/yr",0,1.47E-5,4.75e-05,9.32e-05,0.00014131]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Wet Tower","km3/yr",0.2765604,0.534102455,0.744543255,0.922452,1.07209447]
["GCAM","Base","Brazil","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","China","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",1.284244712,1.819211576,2.238974228,2.065871742,1.383615075]
["GCAM","Base","China","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","China","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",184.7860778,139.4674737,103.7964307,69.83165113,39.21432688]
["GCAM","Base","China","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","China","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",14.01944254,7.980923532,6.674364552,4.498242342,2.524384814]
["GCAM","Base","China","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","China","Capacity Additions|Electricity|Nuclear","GW/yr",2.637240684,11.31410029,14.79605601,14.47239557,10.95863704]
["GCAM","Base","China","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","China","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",0,2.144882357,1.571643201,1.055206748,0.605576167]
["GCAM","Base","China","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.084798121,0.690690902,1.191102936,1.136222968]
["GCAM","Base","China","Capacity Additions|Electricity|Solar|PV","GW/yr",0.49379915,10.27902714,15.48150209,15.21548231,11.53602391]
["GCAM","Base","China","Capacity Additions|Electricity|Wind","GW/yr",11.57728356,15.39024184,21.88980778,21.95995053,16.53159037]
["GCAM","Base","China","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","China","Capacity|Electricity|Biomass|w/o CCS","GW",1.627564529,3.314612665,6.176956494,8.639301116,9.459157788]
["GCAM","Base","China","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","China","Capacity|Electricity|Coal|w/o CCS","GW",470.4028729,699.9024924,843.2122019,885.9938642,872.0704116]
["GCAM","Base","China","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","China","Capacity|Electricity|Gas|w/o CCS","GW",17.96924943,28.62886859,39.80240836,45.24554477,47.08508371]
["GCAM","Base","China","Capacity|Electricity|Hydro","GW",103.0718861,106.4267821,109.7816781,115.3063166,123.001094]
["GCAM","Base","China","Capacity|Electricity|Nuclear","GW",9.370842494,27.68846186,53.67650375,79.91656801,102.2355262]
["GCAM","Base","China","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","China","Capacity|Electricity|Oil|w/o CCS","GW",15.34313166,13.13072362,13.76931523,12.57551687,11.22976915]
["GCAM","Base","China","Capacity|Electricity|Solar|CSP","GW",0,0.115911564,1.121972072,3.294411364,5.57722723]
["GCAM","Base","China","Capacity|Electricity|Solar|PV","GW",0.537241565,17.48050932,51.90398535,93.61770776,122.1758168]
["GCAM","Base","China","Capacity|Electricity|Wind","GW",12.12854244,36.31370927,75.26864543,107.3780008,117.8356495]
["GCAM","Base","China","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Concentration|CH4","ppb",1882.23,2022.81,2228.22,2444.67,2623.87]
["GCAM","Base","China","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","China","Concentration|N2O","ppb",327.014,335.859,345.667,356.386,367.857]
["GCAM","Base","China","Emissions|CO2","Mt CO2/yr",11920.99689,16143.37761,18896.43367,19622.36922,19296.12757]
["GCAM","Base","China","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",6800.858323,9646.377405,11219.92448,11394.81696,10872.95058]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",7168.101894,10176.96457,11865.01436,12083.66082,11562.40996]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",3.19e-05,3.74e-05,2.09E-5,-5.69e-05,1.88032E-4]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",6705.0588,9497.673827,11017.7874,11169.66999,10641.01248]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",75.88861007,124.0783334,171.7062141,193.0647396,199.2886659]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",19.91088,24.62516217,30.4301802,32.07695087,32.63436594]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",367.2435714,530.5871603,645.089881,688.8438617,689.4593776]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",12148.04996,16520.42558,19192.37069,19826.34086,19455.36779]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",4879.717783,6141.588852,6873.05134,6971.796054,6731.702488]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",3716.18668,4438.292769,4716.605129,4645.879487,4387.65661]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",501.3294556,821.6373676,1069.967104,1136.985113,1115.347421]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",662.2016477,881.6587157,1086.479106,1188.931455,1228.698457]
["GCAM","Base","China","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",14069.19053,20025.21409,23539.24318,24249.35647,23596.60106]
["GCAM","Base","China","Emissions|CO2|Land Use","Mt CO2/yr",-227.0530714,-377.0479691,-295.9370207,-203.9716353,-159.2402186]
["GCAM","Base","China","Final Energy","EJ/yr",74.05172204,97.9243162,114.7439076,120.8482845,120.5615481]
["GCAM","Base","China","Final Energy|Electricity","EJ/yr",13.0187695,19.35258861,24.27858637,26.96577058,27.96368458]
["GCAM","Base","China","Final Energy|Gases","EJ/yr",3.058436448,6.036521449,8.35421036,9.169638514,9.219700373]
["GCAM","Base","China","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Final Energy|Heat","EJ/yr",3.0529687,4.4048133,5.3412084,5.6816913,5.6656475]
["GCAM","Base","China","Final Energy|Hydrogen","EJ/yr",0,0.02601825,0.069624243,0.119333205,0.170236149]
["GCAM","Base","China","Final Energy|Industry","EJ/yr",45.998256,60.65781561,68.08808074,69.70058391,68.1559513]
["GCAM","Base","China","Final Energy|Liquids","EJ/yr",17.85210339,26.09427359,33.28790519,36.82971189,38.37747563]
["GCAM","Base","China","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Final Energy|Residential and Commercial","EJ/yr",18.6975098,24.7181659,31.1749096,34.1312401,34.7118345]
["GCAM","Base","China","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Final Energy|Solids","EJ/yr",29.004764,37.048001,40.194033,39.776859,37.4740999]
["GCAM","Base","China","Final Energy|Solids|Biomass","EJ/yr",8.065063,4.962571,3.218818,2.305706,1.69105]
["GCAM","Base","China","Final Energy|Solids|Biomass|Traditional","EJ/yr",8.06468,4.9621,3.21834,2.30528,1.690704]
["GCAM","Base","China","Final Energy|Solids|Coal","EJ/yr",29.004381,37.04753,40.193555,39.776433,37.4737539]
["GCAM","Base","China","Final Energy|Transportation","EJ/yr",7.832288837,10.77724469,13.67392322,15.21691248,15.96659233]
["GCAM","Base","China","Forcing","W/m2",1.86272,2.25795,2.76499,3.33767,3.94881]
["GCAM","Base","China","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","China","GDP|MER","billion US$2010/yr",4460.930279,9839.414093,16201.02775,20894.78345,24377.24736]
["GCAM","Base","China","GDP|PPP","billion US$2010/yr",10277.9768,22669.9956,37327.14411,48141.55034,56165.14207]
["GCAM","Base","China","Land Cover|Cropland|Energy Crops","million ha",0,2.01147916,2.691669492,3.61663393,5.341100844]
["GCAM","Base","China","Population","million",1348.93,1387.49,1389.58,1349.14,1273.18]
["GCAM","Base","China","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","China","Price|Primary Energy|Coal","US$2010/GJ",2.09954199,2.13469085,2.18851234,2.25799287,2.34346513]
["GCAM","Base","China","Price|Primary Energy|Gas","US$2010/GJ",5.6525,5.7436183,5.8860936,6.236807,6.7080317]
["GCAM","Base","China","Price|Primary Energy|Oil","US$2010/GJ",11.0792876,11.5198596,12.1793933,12.6772655,12.8490692]
["GCAM","Base","China","Price|Secondary Energy|Electricity","US$2010/GJ",27.8773225,29.0996837,30.015744,30.3810893,30.629767]
["GCAM","Base","China","Primary Energy","EJ/yr",105.3268288,141.8785603,167.7247376,177.090011,176.952934]
["GCAM","Base","China","Primary Energy|Biomass","EJ/yr",8.669498,6.59265,6.19155,6.62573,6.371594]
["GCAM","Base","China","Primary Energy|Biomass|Electricity","EJ/yr",0.0410615,0.0836237,0.1558372,0.2179592,0.2386432]
["GCAM","Base","China","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Biomass|Gases","EJ/yr",0.39296,0.797275,1.10095,1.31814,1.37244]
["GCAM","Base","China","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.00226189,0.00566597,0.00907606,0.0115064]
["GCAM","Base","China","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Biomass|Liquids","EJ/yr",0,0.448988,1.246569,2.200884,2.4807066]
["GCAM","Base","China","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Biomass|Traditional","EJ/yr",8.06468,4.9621,3.21834,2.30528,1.690704]
["GCAM","Base","China","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Biomass|w/o CCS","EJ/yr",8.669498,6.59265,6.19155,6.62573,6.371594]
["GCAM","Base","China","Primary Energy|Coal","EJ/yr",66.2219,90.9317,106.421,112.333,113.583]
["GCAM","Base","China","Primary Energy|Coal|Electricity","EJ/yr",11.8677,17.6577,21.273232,22.352562,22.00129]
["GCAM","Base","China","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.00960671,0.0268332,0.0496774,0.0772736]
["GCAM","Base","China","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Coal|w/o CCS","EJ/yr",66.2219,90.9317,106.421,112.333,113.583]
["GCAM","Base","China","Primary Energy|Fossil","EJ/yr",89.145268,125.446861,149.95072,158.36793,158.75293]
["GCAM","Base","China","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Fossil|w/o CCS","EJ/yr",89.145268,125.446861,149.95072,158.36793,158.75293]
["GCAM","Base","China","Primary Energy|Gas","EJ/yr",3.64044,7.58809,12.7062,16.5977,19.2797]
["GCAM","Base","China","Primary Energy|Gas|Electricity","EJ/yr",0.3003612,0.607117,0.89776,1.062598,1.1370576]
["GCAM","Base","China","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.0242331,0.0635722,0.1035054,0.1383455]
["GCAM","Base","China","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Gas|w/o CCS","EJ/yr",3.64044,7.58809,12.7062,16.5977,19.2797]
["GCAM","Base","China","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Hydro","EJ/yr",2.60038,2.68502,2.76966,2.90904,3.10317]
["GCAM","Base","China","Primary Energy|Non-Biomass Renewables","EJ/yr",2.76441249,3.313533299,4.202538669,5.091121469,5.68304146]
["GCAM","Base","China","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Oil","EJ/yr",19.282928,26.927071,30.82352,29.43723,25.89023]
["GCAM","Base","China","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Oil|w/o CCS","EJ/yr",19.282928,26.927071,30.82352,29.43723,25.89023]
["GCAM","Base","China","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Primary Energy|Solar","EJ/yr",0.00338849,0.113178188,0.340989548,0.624396058,0.83332089]
["GCAM","Base","China","Primary Energy|Wind","EJ/yr",0.160644,0.515335111,1.091889121,1.557685411,1.74655057]
["GCAM","Base","China","Resource|Cumulative Extraction|Coal","EJ",323.336,760.083,1307.7885,1974.534,2781.64]
["GCAM","Base","China","Resource|Cumulative Extraction|Gas","EJ",16.6237,50.2064,93.36635,168.2299,264.26495]
["GCAM","Base","China","Resource|Cumulative Extraction|Oil","EJ",43.9655,127.05658,217.668,308.345335,376.92721]
["GCAM","Base","China","Secondary Energy|Electricity","EJ/yr",15.2884713,22.62588163,28.28594625,31.28133043,32.30586418]
["GCAM","Base","China","Secondary Energy|Electricity|Biomass","EJ/yr",0.0410615,0.0836237,0.1558372,0.2179592,0.2386432]
["GCAM","Base","China","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.0410615,0.0836237,0.1558372,0.2179592,0.2386432]
["GCAM","Base","China","Secondary Energy|Electricity|Coal","EJ/yr",11.8677,17.6577,21.273232,22.352562,22.00129]
["GCAM","Base","China","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",11.8677,17.6577,21.273232,22.352562,22.00129]
["GCAM","Base","China","Secondary Energy|Electricity|Fossil","EJ/yr",12.21644731,18.33940956,22.27077377,23.52684484,23.2573561]
["GCAM","Base","China","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",12.21644731,18.33940956,22.27077377,23.52684484,23.2573561]
["GCAM","Base","China","Secondary Energy|Electricity|Gas","EJ/yr",0.300361207,0.60711736,0.897765272,1.062641242,1.137179698]
["GCAM","Base","China","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",0.300361207,0.60711736,0.897765272,1.062641242,1.137179698]
["GCAM","Base","China","Secondary Energy|Electricity|Geothermal","EJ/yr",0.000583,0.1023169,0.1134115,0.1134114,0.11341142]
["GCAM","Base","China","Secondary Energy|Electricity|Hydro","EJ/yr",2.60038,2.68502,2.76966,2.90904,3.10317]
["GCAM","Base","China","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",2.76499549,3.416983369,4.335867279,5.268302389,5.90817528]
["GCAM","Base","China","Secondary Energy|Electricity|Nuclear","EJ/yr",0.265967,0.785865,1.523468,2.268224,2.9016896]
["GCAM","Base","China","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Oil","EJ/yr",0.0483861,0.0745922,0.0997765,0.1116416,0.1188864]
["GCAM","Base","China","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.0483861,0.0745922,0.0997765,0.1116416,0.1188864]
["GCAM","Base","China","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Electricity|Solar","EJ/yr",0.00338849,0.114311358,0.360906658,0.688165578,0.94504329]
["GCAM","Base","China","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,1.13317E-3,0.01991711,0.06376952,0.1117224]
["GCAM","Base","China","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.00338849,0.113178188,0.340989548,0.624396058,0.83332089]
["GCAM","Base","China","Secondary Energy|Electricity|Wind","EJ/yr",0.160644,0.515335111,1.091889121,1.557685411,1.74655057]
["GCAM","Base","China","Secondary Energy|Gases","EJ/yr",4.104359,7.815827,10.786987,11.917718,12.06024]
["GCAM","Base","China","Secondary Energy|Gases|Biomass","EJ/yr",0.292598,0.593652,0.828717,1.00315,1.05613]
["GCAM","Base","China","Secondary Energy|Gases|Coal","EJ/yr",0.171321,0.373325,0.6179,0.946898,1.40273]
["GCAM","Base","China","Secondary Energy|Gases|Natural Gas","EJ/yr",3.64044,6.84885,9.34037,9.96767,9.60138]
["GCAM","Base","China","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Hydrogen","EJ/yr",0,0.026017991,0.069624275,0.119333174,0.170235841]
["GCAM","Base","China","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.00102011,2.60634E-3,0.00426575,0.00552306]
["GCAM","Base","China","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.00102011,2.60634E-3,0.00426575,0.00552306]
["GCAM","Base","China","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.00614829,0.0175221,0.0331348,0.052546]
["GCAM","Base","China","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.00614829,0.0175221,0.0331348,0.052546]
["GCAM","Base","China","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.002407221,0.005898455,0.009811104,0.013920051]
["GCAM","Base","China","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.01540092,0.0410037,0.0678187,0.0922191]
["GCAM","Base","China","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.01540092,0.0410037,0.0678187,0.0922191]
["GCAM","Base","China","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,1.04145E-3,0.00259368,0.00430282,6.02763E-3]
["GCAM","Base","China","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Liquids","EJ/yr",18.1592898,26.48908246,33.75243025,37.30192241,38.84334772]
["GCAM","Base","China","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.223002,0.6238967,1.1122249,1.2724856]
["GCAM","Base","China","Secondary Energy|Liquids|Coal","EJ/yr",0,0.410222,1.984811,4.23881,6.95084]
["GCAM","Base","China","Secondary Energy|Liquids|Gas","EJ/yr",0,0.420198,1.990813,3.967724,5.838912]
["GCAM","Base","China","Secondary Energy|Liquids|Oil","EJ/yr",18.1086,25.35734,29.08479,27.88378,24.681303]
["GCAM","Base","China","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","China","Temperature|Global Mean","?C",0.824511,1.01712,1.27001,1.56514,1.88832]
["GCAM","Base","China","Water Consumption|Electricity","km3/yr",19.07305913,22.92327656,25.57202049,27.10499049,28.08137355]
["GCAM","Base","China","Water Consumption|Electricity|Biomass","km3/yr",0.01911557,0.036153529,0.064013813,0.087025139,0.0931842]
["GCAM","Base","China","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.01911557,0.036153529,0.064013813,0.087025139,0.0931842]
["GCAM","Base","China","Water Consumption|Electricity|Coal","km3/yr",6.466333,9.4609236,11.20113973,11.59863987,11.27309491]
["GCAM","Base","China","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",6.466333,9.4609236,11.20113973,11.59863987,11.27309491]
["GCAM","Base","China","Water Consumption|Electricity|Cooling Pond","km3/yr",0.42873492,0.37502959,0.31138493,0.21278087,0.11430757]
["GCAM","Base","China","Water Consumption|Electricity|Dry Cooling","km3/yr",4.34e-05,0.00773293,0.0104894,0.014997156,0.019925429]
["GCAM","Base","China","Water Consumption|Electricity|Fossil","km3/yr",6.61390936,9.629471636,11.40863021,11.81440873,11.48335269]
["GCAM","Base","China","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",6.61390936,9.629471636,11.40863021,11.81440873,11.48335269]
["GCAM","Base","China","Water Consumption|Electricity|Gas","km3/yr",0.11585872,0.144767251,0.184597387,0.196829687,0.195199029]
["GCAM","Base","China","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.11585872,0.144767251,0.184597387,0.196829687,0.195199029]
["GCAM","Base","China","Water Consumption|Electricity|Geothermal","km3/yr",0.0007044,0.123576051,0.136975776,0.136975809,0.136975809]
["GCAM","Base","China","Water Consumption|Electricity|Hydro","km3/yr",12.2796,12.6793,13.079,13.7371,14.6538]
["GCAM","Base","China","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.0007044,0.124211051,0.148151014,0.172757822,0.199664538]
["GCAM","Base","China","Water Consumption|Electricity|Nuclear","km3/yr",0.159711,0.453583572,0.870684611,1.29113032,1.648436637]
["GCAM","Base","China","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Oil","km3/yr",0.03171764,0.023780785,0.022893095,0.018939176,0.01505875]
["GCAM","Base","China","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.03171764,0.023780785,0.022893095,0.018939176,0.01505875]
["GCAM","Base","China","Water Consumption|Electricity|Once Through","km3/yr",0.57118488,0.520102217,0.451453051,0.331949106,0.208612266]
["GCAM","Base","China","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Consumption|Electricity|Solar","km3/yr",1.88E-5,1.19177E-3,0.012716082,0.038350487,0.065624213]
["GCAM","Base","China","Water Consumption|Electricity|Solar|CSP","km3/yr",0,0.000635,0.011175238,0.035782013,0.062688729]
["GCAM","Base","China","Water Consumption|Electricity|Solar|PV","km3/yr",1.88E-5,0.00055677,1.540844E-3,0.002568474,0.002935484]
["GCAM","Base","China","Water Consumption|Electricity|Wet Tower","km3/yr",5.79347713,9.340555051,11.71815227,12.80559488,13.0817928]
["GCAM","Base","China","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity","km3/yr",100.5427523,97.32844993,89.62927653,71.93374122,52.45814385]
["GCAM","Base","China","Water Withdrawal|Electricity|Biomass","km3/yr",0.28748394,0.19981935,0.24524339,0.26289229,0.24538411]
["GCAM","Base","China","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.28748394,0.19981935,0.24524339,0.26289229,0.24538411]
["GCAM","Base","China","Water Withdrawal|Electricity|Coal","km3/yr",95.71186,92.52736,84.1396773,66.1806151,46.6364445]
["GCAM","Base","China","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",95.71186,92.52736,84.1396773,66.1806151,46.6364445]
["GCAM","Base","China","Water Withdrawal|Electricity|Cooling Pond","km3/yr",9.27144371,8.16122552,6.774026,4.63269067,2.49156356]
["GCAM","Base","China","Water Withdrawal|Electricity|Dry Cooling","km3/yr",4.34e-05,0.00773293,0.0104894,0.014997156,0.019925429]
["GCAM","Base","China","Water Withdrawal|Electricity|Fossil","km3/yr",97.76072515,94.03875476,85.55943278,67.27351344,47.39612252]
["GCAM","Base","China","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",97.76072515,94.03875476,85.55943278,67.27351344,47.39612252]
["GCAM","Base","China","Water Withdrawal|Electricity|Gas","km3/yr",1.70125026,1.32009368,1.24738418,0.96892514,0.682627175]
["GCAM","Base","China","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",1.70125026,1.32009368,1.24738418,0.96892514,0.682627175]
["GCAM","Base","China","Water Withdrawal|Electricity|Geothermal","km3/yr",0.0007044,0.123576051,0.136975776,0.136975809,0.136975809]
["GCAM","Base","China","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.0007044,0.124211051,0.148151014,0.172757822,0.199664538]
["GCAM","Base","China","Water Withdrawal|Electricity|Nuclear","km3/yr",2.49382,2.965108,3.6749085,4.2220092,4.6140372]
["GCAM","Base","China","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Oil","km3/yr",0.34761489,0.191301075,0.172371304,0.123973196,0.077050843]
["GCAM","Base","China","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",0.34761489,0.191301075,0.172371304,0.123973196,0.077050843]
["GCAM","Base","China","Water Withdrawal|Electricity|Once Through","km3/yr",82.7673611,75.48151047,65.68579406,48.52827222,30.77594921]
["GCAM","Base","China","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","China","Water Withdrawal|Electricity|Sea Cooling","km3/yr",21.8101881,77.8377083,121.8861507,152.6636541,171.5740393]
["GCAM","Base","China","Water Withdrawal|Electricity|Solar","km3/yr",1.88E-5,1.19177E-3,0.012716082,0.038350487,0.065624213]
["GCAM","Base","China","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.000635,0.011175238,0.035782013,0.062688729]
["GCAM","Base","China","Water Withdrawal|Electricity|Solar|PV","km3/yr",1.88E-5,0.00055677,1.540844E-3,0.002568474,0.002935484]
["GCAM","Base","China","Water Withdrawal|Electricity|Wet Tower","km3/yr",8.50388528,13.67742424,17.15742623,18.7552127,19.16777017]
["GCAM","Base","China","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","EU","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",4.922956026,1.720331526,2.198328259,3.545342704,2.408473808]
["GCAM","Base","EU","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","EU","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0,15.254726701,16.876704675,22.72313122,15.680898334]
["GCAM","Base","EU","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","EU","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",55.68292364,15.654266943,19.000651117,26.357850649,15.897168163]
["GCAM","Base","EU","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","EU","Capacity Additions|Electricity|Nuclear","GW/yr",0,9.998294436,12.007373159,18.663873522,13.947370373]
["GCAM","Base","EU","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","EU","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",0.455149353,4.947641109,5.367410579,7.480062469,5.043200787]
["GCAM","Base","EU","Capacity Additions|Electricity|Solar|CSP","GW/yr",0.254813751,0.138501825,1.023188232,3.107247981,3.490249218]
["GCAM","Base","EU","Capacity Additions|Electricity|Solar|PV","GW/yr",11.944687028,2.200923548,2.722009608,4.413668981,1.810720763]
["GCAM","Base","EU","Capacity Additions|Electricity|Wind","GW/yr",21.367573867,8.084110364,16.057960049,34.623471722,28.835354327]
["GCAM","Base","EU","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","EU","Capacity|Electricity|Biomass|w/o CCS","GW",11.627104733,10.686707255,11.960792031,14.405888112,15.148665014]
["GCAM","Base","EU","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","EU","Capacity|Electricity|Coal|w/o CCS","GW",120.11268867,148.98607938,162.17524815,175.15798217,181.8457081]
["GCAM","Base","EU","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","EU","Capacity|Electricity|Gas|w/o CCS","GW",125.762699793,151.79090243,167.90166637,185.14517536,192.08674217]
["GCAM","Base","EU","Capacity|Electricity|Hydro","GW",52.770008878,51.300180749,50.333824835,50.252211754,51.056173895]
["GCAM","Base","EU","Capacity|Electricity|Nuclear","GW",116.25761033,132.42329749,137.11726282,141.93968794,144.94365171]
["GCAM","Base","EU","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","EU","Capacity|Electricity|Oil|w/o CCS","GW",75.9093417,65.17877981,62.70687072,58.8774694,54.39756151]
["GCAM","Base","EU","Capacity|Electricity|Solar|CSP","GW",0.254812728,0.546526449,2.021008851,6.705919648,13.175827689]
["GCAM","Base","EU","Capacity|Electricity|Solar|PV","GW",12.776855024,18.655102742,24.570784311,20.101951993,21.828257099]
["GCAM","Base","EU","Capacity|Electricity|Wind","GW",40.513343787,57.371525738,82.847196162,101.548590571,140.55609987]
["GCAM","Base","EU","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Concentration|CH4","ppb",3764.46,4045.62,4456.44,4889.34,5247.74]
["GCAM","Base","EU","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","EU","Concentration|N2O","ppb",654.028,671.718,691.334,712.772,735.714]
["GCAM","Base","EU","Emissions|CO2","Mt CO2/yr",4932.7574192,5569.555322,5778.861845,6220.288455,6606.002657]
["GCAM","Base","EU","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",2352.9680359,2815.6645255,3015.8205026,3169.1323002,3180.1235314]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",2376.7632375,2889.9903254,3096.8589937,3253.3430264,3265.5931496]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",-1.03516E-4,-6.673e-05,-5.858e-05,0.000348721,-5.6e-06]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",1694.4127933,2036.2642465,2148.8901882,2212.4090281,2190.370285]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",556.69013347,676.32102334,745.07516809,810.38326962,829.1829634]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",101.86465814,103.0761796,121.82441366,146.30520083,160.33013786]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",23.79520166,74.32579992,81.03849108,84.21072624,85.46961814]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",5142.464487,5782.768622,6069.763265,6453.268967,6770.637029]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",2660.1049028,2717.4304078,2722.3223649,2694.6419463,2657.6055082]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",816.8194914,825.5948212,845.0724459,843.3796702,834.7351476]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",619.40553459,642.4852646,670.6731883,677.8688017,673.690803]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",1223.879877,1249.3503222,1206.5767301,1173.3934745,1149.1795568]
["GCAM","Base","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",4835.327286,5880.999998,6363.230623,6927.72487,7292.914924]
["GCAM","Base","EU","Emissions|CO2|Land Use","Mt CO2/yr",-209.70706709,-213.213299572,-290.90142006,-232.98051183,-164.6343722]
["GCAM","Base","EU","Final Energy","EJ/yr",56.183029982,59.442028118,61.47739744,62.92654373,63.92847812]
["GCAM","Base","EU","Final Energy|Electricity","EJ/yr",10.4643943,12.438201619,13.895305842,15.408249503,16.750378634]
["GCAM","Base","EU","Final Energy|Gases","EJ/yr",12.901639612,13.273261941,14.128349782,14.309113845,14.070280746]
["GCAM","Base","EU","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Final Energy|Heat","EJ/yr",0.7893372,0.8350838,0.8964585,0.9077904,0.8920002]
["GCAM","Base","EU","Final Energy|Hydrogen","EJ/yr",0,0.162408054,0.40333919,0.707583712,1.074666504]
["GCAM","Base","EU","Final Energy|Industry","EJ/yr",20.23133419,21.462149977,22.515417192,23.190951125,23.66933946]
["GCAM","Base","EU","Final Energy|Liquids","EJ/yr",25.78699207,26.618577698,26.303338445,26.085561073,26.090379247]
["GCAM","Base","EU","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Final Energy|Residential and Commercial","EJ/yr",18.8185977,20.40981804,21.79882406,22.82487945,23.463377448]
["GCAM","Base","EU","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Final Energy|Solids","EJ/yr",6.2406668,6.114495,5.85060569,5.5082452,5.050772788]
["GCAM","Base","EU","Final Energy|Solids|Biomass","EJ/yr",3.1935695,3.06521168,2.74276207,2.38135572,1.949053448]
["GCAM","Base","EU","Final Energy|Solids|Biomass|Traditional","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Final Energy|Solids|Coal","EJ/yr",3.0470973,3.04928332,3.10784362,3.12688948,3.10171934]
["GCAM","Base","EU","Final Energy|Transportation","EJ/yr",17.133098092,17.570060101,17.163156199,16.910713165,16.79576121]
["GCAM","Base","EU","Forcing","W/m2",3.72544,4.5159,5.52998,6.67534,7.89762]
["GCAM","Base","EU","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","EU","GDP|MER","billion US$2010/yr",15679.657478,18376.733414,21501.489232,25221.548022,29189.679382]
["GCAM","Base","EU","GDP|PPP","billion US$2010/yr",14926.836712,17585.247377,20664.872137,24282.311263,28095.331963]
["GCAM","Base","EU","Land Cover|Cropland|Energy Crops","million ha",0,5.722453056,7.432204955,9.94011524,14.022906711]
["GCAM","Base","EU","Population","million",501.054,515.583,525.997,533.269,537.658]
["GCAM","Base","EU","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","EU","Price|Primary Energy|Coal","US$2010/GJ",4.19908398,4.2693817,4.37702468,4.51598574,4.68693026]
["GCAM","Base","EU","Price|Primary Energy|Gas","US$2010/GJ",11.305,11.4872366,11.7721872,12.473614,13.4160634]
["GCAM","Base","EU","Price|Primary Energy|Oil","US$2010/GJ",22.1512754,23.0335499,24.3562349,25.3561783,25.7008839]
["GCAM","Base","EU","Price|Secondary Energy|Electricity","US$2010/GJ",65.9141578,62.6777624,62.6658437,62.5677486,62.6236276]
["GCAM","Base","EU","Primary Energy","EJ/yr",70.32904048,76.39726659,79.48807248,83.6090879,86.931838]
["GCAM","Base","EU","Primary Energy|Biomass","EJ/yr",5.024706,5.002595,5.182597,6.43369,6.907923]
["GCAM","Base","EU","Primary Energy|Biomass|Electricity","EJ/yr",0.2933379,0.2696128,0.30175643,0.36344327,0.38218264]
["GCAM","Base","EU","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Biomass|Gases","EJ/yr",0.616366,0.7172007,0.7789762,0.9051158,0.9699716]
["GCAM","Base","EU","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.01338,0.03099348,0.05054956,0.068142494]
["GCAM","Base","EU","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Biomass|Liquids","EJ/yr",0,0.0642757,0.4172771,1.76275221,2.61757802]
["GCAM","Base","EU","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Biomass|Traditional","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Biomass|w/o CCS","EJ/yr",5.024706,5.002595,5.182597,6.43369,6.907923]
["GCAM","Base","EU","Primary Energy|Coal","EJ/yr",11.74841,14.00418,15.76471,20.61049,26.0561]
["GCAM","Base","EU","Primary Energy|Coal|Electricity","EJ/yr",3.030299,3.75874,4.0914869,4.4190257,4.587749]
["GCAM","Base","EU","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.056827625,0.1467805,0.27668031,0.45762623]
["GCAM","Base","EU","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Coal|w/o CCS","EJ/yr",11.74841,14.00418,15.76471,20.61049,26.0561]
["GCAM","Base","EU","Primary Energy|Fossil","EJ/yr",57.900724,63.496345,66.331965,69.938662,73.083211]
["GCAM","Base","EU","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Fossil|w/o CCS","EJ/yr",57.900724,63.496345,66.331965,69.938662,73.083211]
["GCAM","Base","EU","Primary Energy|Gas","EJ/yr",18.46987,20.42431,22.79639,26.42539,28.96084]
["GCAM","Base","EU","Primary Energy|Gas|Electricity","EJ/yr",2.404335,3.1702357,3.6645976,4.243241,4.5653645]
["GCAM","Base","EU","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.157210902,0.38198354,0.6396374,0.915716]
["GCAM","Base","EU","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Gas|w/o CCS","EJ/yr",18.46987,20.42431,22.79639,26.42539,28.96084]
["GCAM","Base","EU","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Hydro","EJ/yr",1.331324,1.294242,1.269862,1.267803,1.288086]
["GCAM","Base","EU","Primary Energy|Non-Biomass Renewables","EJ/yr",1.94851428,2.226818159,2.628918811,2.872721802,3.518161438]
["GCAM","Base","EU","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Oil","EJ/yr",27.682444,29.067855,27.770865,22.902782,18.066271]
["GCAM","Base","EU","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Oil|w/o CCS","EJ/yr",27.682444,29.067855,27.770865,22.902782,18.066271]
["GCAM","Base","EU","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Primary Energy|Solar","EJ/yr",0.08058618,0.118405751,0.157228813,0.131798153,0.14676417]
["GCAM","Base","EU","Primary Energy|Wind","EJ/yr",0.5366041,0.814170408,1.201827998,1.473120649,2.083311268]
["GCAM","Base","EU","Resource|Cumulative Extraction|Coal","EJ",32.68475,204.84905,424.95735,696.4925,1028.8682]
["GCAM","Base","EU","Resource|Cumulative Extraction|Gas","EJ",32.689735,155.824985,320.011135,464.080835,612.915385]
["GCAM","Base","EU","Resource|Cumulative Extraction|Oil","EJ",21.02488,59.066625,125.779385,184.959285,236.38069]
["GCAM","Base","EU","Secondary Energy|Electricity","EJ/yr",11.75923197,13.560956542,15.178822367,16.859904514,18.336879288]
["GCAM","Base","EU","Secondary Energy|Electricity|Biomass","EJ/yr",0.3155654,0.2696128,0.30175643,0.36344327,0.38218264]
["GCAM","Base","EU","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.3155654,0.2696128,0.30175643,0.36344327,0.38218264]
["GCAM","Base","EU","Secondary Energy|Electricity|Coal","EJ/yr",3.349102,3.75874,4.0914869,4.4190257,4.587749]
["GCAM","Base","EU","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",3.349102,3.75874,4.0914869,4.4190257,4.587749]
["GCAM","Base","EU","Secondary Energy|Electricity|Fossil","EJ/yr",6.1728249,7.210155238,8.131084544,9.167836867,9.746747115]
["GCAM","Base","EU","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",6.1728249,7.210155238,8.131084544,9.167836867,9.746747115]
["GCAM","Base","EU","Secondary Energy|Electricity|Gas","EJ/yr",2.56441,3.170258338,3.664817444,4.243471167,4.566912015]
["GCAM","Base","EU","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",2.56441,3.170258338,3.664817444,4.243471167,4.566912015]
["GCAM","Base","EU","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0201663,0.09053641,0.19215968,0.29432052,0.2999701]
["GCAM","Base","EU","Secondary Energy|Electricity|Hydro","EJ/yr",1.331324,1.294242,1.269862,1.267803,1.288086]
["GCAM","Base","EU","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",1.97117167,2.322697499,2.854264397,3.300035372,4.094100828]
["GCAM","Base","EU","Secondary Energy|Electricity|Nuclear","EJ/yr",3.29967,3.758491,3.891717,4.028589,4.1138487]
["GCAM","Base","EU","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Oil","EJ/yr",0.2593129,0.2811569,0.3747802,0.50534,0.5920861]
["GCAM","Base","EU","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.2593129,0.2811569,0.3747802,0.50534,0.5920861]
["GCAM","Base","EU","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Electricity|Solar","EJ/yr",0.08307727,0.123748681,0.190414719,0.264791203,0.42273346]
["GCAM","Base","EU","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0.00249109,0.00534293,0.033185906,0.13299305,0.27596929]
["GCAM","Base","EU","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.08058618,0.118405751,0.157228813,0.131798153,0.14676417]
["GCAM","Base","EU","Secondary Energy|Electricity|Wind","EJ/yr",0.5366041,0.814170408,1.201827998,1.473120649,2.083311268]
["GCAM","Base","EU","Secondary Energy|Gases","EJ/yr",18.9494401,20.8440075,22.5366591,23.5265921,23.6307171]
["GCAM","Base","EU","Secondary Energy|Gases|Biomass","EJ/yr",0.4589467,0.5340287,0.5863581,0.6888251,0.7464191]
["GCAM","Base","EU","Secondary Energy|Gases|Coal","EJ/yr",0.0262334,0.0849788,0.183081,0.392207,0.811238]
["GCAM","Base","EU","Secondary Energy|Gases|Natural Gas","EJ/yr",18.46426,20.225,21.76722,22.44556,22.07306]
["GCAM","Base","EU","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Hydrogen","EJ/yr",0,0.162407781,0.403339505,0.70758411,1.074666706]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.00603439,0.0142573,0.0237586,0.0327081]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.00603439,0.0142573,0.0237586,0.0327081]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.0363693,0.09584765,0.18454576,0.31118584]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.0363693,0.09584765,0.18454576,0.31118584]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.014964331,0.034962885,0.05995244,0.089647176]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.0988792,0.24408377,0.41536301,0.60542929]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.0988792,0.24408377,0.41536301,0.60542929]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,0.00616056,0.0141879,0.0239643,0.0356963]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Liquids","EJ/yr",26.50663295,27.371743093,27.188318187,27.14082278,27.243836605]
["GCAM","Base","EU","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.03192425,0.20963972,0.89788119,1.34733761]
["GCAM","Base","EU","Secondary Energy|Liquids|Coal","EJ/yr",0.0207611,0.053094,0.464483,2.42047291,4.766237722]
["GCAM","Base","EU","Secondary Energy|Liquids|Gas","EJ/yr",0.00339045,0.03700465,0.44905742,2.163858132,3.871645145]
["GCAM","Base","EU","Secondary Energy|Liquids|Oil","EJ/yr",25.92373,27.242656,26.0502733,21.5990608,17.2098403]
["GCAM","Base","EU","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","EU","Temperature|Global Mean","?C",1.649022,2.03424,2.54002,3.13028,3.77664]
["GCAM","Base","EU","Water Consumption|Electricity","km3/yr",10.9716476,11.531540214,11.798823812,12.155040025,12.350702833]
["GCAM","Base","EU","Water Consumption|Electricity|Biomass","km3/yr",0.13879812,0.122561267,0.131452291,0.149449627,0.150206487]
["GCAM","Base","EU","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.13879812,0.122561267,0.131452291,0.149449627,0.150206487]
["GCAM","Base","EU","Water Consumption|Electricity|Coal","km3/yr",1.689445,2.101740605,2.27513444,2.422512837,2.479527188]
["GCAM","Base","EU","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",1.689445,2.101740605,2.27513444,2.422512837,2.479527188]
["GCAM","Base","EU","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Dry Cooling","km3/yr",1.75728E-3,7.28847E-3,0.017715216,0.035579558,0.050694353]
["GCAM","Base","EU","Water Consumption|Electricity|Fossil","km3/yr",2.64141235,3.076379845,3.258184248,3.386337715,3.387105174]
["GCAM","Base","EU","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",2.64141235,3.076379845,3.258184248,3.386337715,3.387105174]
["GCAM","Base","EU","Water Consumption|Electricity|Gas","km3/yr",0.7943658,0.846800913,0.869922753,0.872240321,0.834957655]
["GCAM","Base","EU","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.7943658,0.846800913,0.869922753,0.872240321,0.834957655]
["GCAM","Base","EU","Water Consumption|Electricity|Geothermal","km3/yr",0.02435638,0.10934769,0.232086136,0.35547365,0.362297161]
["GCAM","Base","EU","Water Consumption|Electricity|Hydro","km3/yr",6.2868,6.111685,5.996552,5.986857,6.082629]
["GCAM","Base","EU","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.02575413,0.112345359,0.250705904,0.430097466,0.517146502]
["GCAM","Base","EU","Water Consumption|Electricity|Nuclear","km3/yr",1.8784356,2.107928666,2.161112031,2.20169364,2.213037669]
["GCAM","Base","EU","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Oil","km3/yr",0.15760155,0.127838327,0.113127055,0.091584557,0.072620331]
["GCAM","Base","EU","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.15760155,0.127838327,0.113127055,0.091584557,0.072620331]
["GCAM","Base","EU","Water Consumption|Electricity|Once Through","km3/yr",0.57138347,0.493988838,0.415230666,0.293759619,0.172957896]
["GCAM","Base","EU","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Consumption|Electricity|Solar","km3/yr",1.84515E-3,0.003637746,0.019437106,0.075228393,0.155427342]
["GCAM","Base","EU","Water Consumption|Electricity|Solar|CSP","km3/yr",0.00139775,0.002997669,0.018619768,0.074623816,0.154849341]
["GCAM","Base","EU","Water Consumption|Electricity|Solar|PV","km3/yr",0.0004474,0.00064007,0.00081738,0.0006046,0.000578]
["GCAM","Base","EU","Water Consumption|Electricity|Wet Tower","km3/yr",4.11125945,4.917937829,5.368508592,5.838239271,6.043843583]
["GCAM","Base","EU","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity","km3/yr",89.33603233,79.63880053,68.79848044,51.75712844,34.432899709]
["GCAM","Base","EU","Water Withdrawal|Electricity|Biomass","km3/yr",2.6867709,1.66711394,1.352839794,0.975983375,0.632154389]
["GCAM","Base","EU","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",2.6867709,1.66711394,1.352839794,0.975983375,0.632154389]
["GCAM","Base","EU","Water Withdrawal|Electricity|Coal","km3/yr",31.032675,28.6536431,24.92625249,18.95160247,12.78307911]
["GCAM","Base","EU","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",31.032675,28.6536431,24.92625249,18.95160247,12.78307911]
["GCAM","Base","EU","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Dry Cooling","km3/yr",1.75728E-3,7.28847E-3,0.017715216,0.035579558,0.050694353]
["GCAM","Base","EU","Water Withdrawal|Electricity|Fossil","km3/yr",48.0623779,42.65623225,36.85527851,27.607946035,18.20891927]
["GCAM","Base","EU","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",48.0623779,42.65623225,36.85527851,27.607946035,18.20891927]
["GCAM","Base","EU","Water Withdrawal|Electricity|Gas","km3/yr",14.8391979,12.669870345,10.827958194,7.893673607,4.966816502]
["GCAM","Base","EU","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",14.8391979,12.669870345,10.827958194,7.893673607,4.966816502]
["GCAM","Base","EU","Water Withdrawal|Electricity|Geothermal","km3/yr",0.02435638,0.10934769,0.232086136,0.35547365,0.362297161]
["GCAM","Base","EU","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.02575413,0.112345359,0.250705904,0.430097466,0.517146502]
["GCAM","Base","EU","Water Withdrawal|Electricity|Nuclear","km3/yr",38.560682,35.2024689,30.3388389,22.742497,15.07410155]
["GCAM","Base","EU","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Oil","km3/yr",2.190505,1.332718806,1.101067822,0.762669953,0.459023658]
["GCAM","Base","EU","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",2.190505,1.332718806,1.101067822,0.762669953,0.459023658]
["GCAM","Base","EU","Water Withdrawal|Electricity|Once Through","km3/yr",82.987522,72.13328017,60.7021852,43.066397033,25.496125508]
["GCAM","Base","EU","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","EU","Water Withdrawal|Electricity|Sea Cooling","km3/yr",18.3396739,38.30227852,51.72646809,70.65813697,86.63521697]
["GCAM","Base","EU","Water Withdrawal|Electricity|Solar","km3/yr",1.84515E-3,0.003637746,0.019437106,0.075228393,0.155427342]
["GCAM","Base","EU","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.00139775,0.002997669,0.018619768,0.074623816,0.154849341]
["GCAM","Base","EU","Water Withdrawal|Electricity|Solar|PV","km3/yr",0.0004474,0.00064007,0.00081738,0.0006046,0.000578]
["GCAM","Base","EU","Water Withdrawal|Electricity|Wet Tower","km3/yr",6.34630565,7.497591809,8.077762686,8.654547285,8.88550185]
["GCAM","Base","EU","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","India","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.019120965,0.847020508,1.903073234,2.816299309,2.981098784]
["GCAM","Base","India","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","India","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",25.83657962,54.33850956,80.2538267,89.86731553,81.45152564]
["GCAM","Base","India","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","India","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",22.88641622,15.25399453,23.90535746,25.52661685,21.3681863]
["GCAM","Base","India","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","India","Capacity Additions|Electricity|Nuclear","GW/yr",1.134196192,2.309561383,3.562677469,4.388167843,4.72475897]
["GCAM","Base","India","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","India","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",3.654106418,26.08627949,33.80326421,33.14287291,26.4066784]
["GCAM","Base","India","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.053906646,0.831210697,2.327196094,3.548802813]
["GCAM","Base","India","Capacity Additions|Electricity|Solar|PV","GW/yr",0.002283105,4.218367738,12.07643011,19.34066939,23.39553685]
["GCAM","Base","India","Capacity Additions|Electricity|Wind","GW/yr",3.617083122,4.643896852,10.3443904,14.84971833,15.8626406]
["GCAM","Base","India","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","India","Capacity|Electricity|Biomass|w/o CCS","GW",0.293521293,1.299820047,3.923932173,7.845311707,11.32837471]
["GCAM","Base","India","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","India","Capacity|Electricity|Coal|w/o CCS","GW",93.18001649,193.79043,327.0516632,481.4680445,629.6458809]
["GCAM","Base","India","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","India","Capacity|Electricity|Gas|w/o CCS","GW",25.97313784,53.00848237,92.77265665,136.8948186,175.4281773]
["GCAM","Base","India","Capacity|Electricity|Hydro","GW",16.32760972,19.17570396,22.0237982,25.95616914,30.97277714]
["GCAM","Base","India","Capacity|Electricity|Nuclear","GW",3.331554062,7.736798157,13.79707142,21.2193014,29.88994588]
["GCAM","Base","India","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","India","Capacity|Electricity|Oil|w/o CCS","GW",30.18375824,72.06474347,109.7433092,143.16019790000001,172.9187278]
["GCAM","Base","India","Capacity|Electricity|Solar|CSP","GW",0,0.073648549,1.21044731,5.118757164,11.62199916]
["GCAM","Base","India","Capacity|Electricity|Solar|PV","GW",0.013127854,7.91888001,34.45191032,84.31658752,149.9715067]
["GCAM","Base","India","Capacity|Electricity|Wind","GW",5.411766749,13.31366023,30.72161732,53.20715835,75.78343494]
["GCAM","Base","India","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Concentration|CH4","ppb",1882.23,2022.81,2228.22,2444.67,2623.87]
["GCAM","Base","India","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","India","Concentration|N2O","ppb",327.014,335.859,345.667,356.386,367.857]
["GCAM","Base","India","Emissions|CO2","Mt CO2/yr",2819.023243,4544.363175,7280.606801,10028.01453,12492.69678]
["GCAM","Base","India","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",1869.597237,3314.198014,5160.447073,7088.360826,8811.958863]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",1869.597237,3314.198014,5160.447073,7088.360826,8811.958863]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",-1.34E-5,-1.83e-06,-2.03E-6,-1.4E-5,-1.08455E-4]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",1688.361033,2889.244651,4368.216104,5947.696111,7379.091075]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",113.5305864,238.5310633,414.1646211,602.1725897,761.2398031]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",67.70563067,186.4222751,378.0659362,538.4885273,671.6081356]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",2773.908308,4815.895003,7444.707543,10124.65307,12574.89681]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",853.5536752,1427.905452,2077.475799,2644.113312,3096.450999]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",542.2956341,953.2724996,1412.000182,1812.142195,2120.205343]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",126.7174542,220.9364569,335.2764006,425.9465768,494.3600366]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",184.540587,253.6964955,330.1992162,406.0245402,481.8856193]
["GCAM","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",3789.952053,6702.187538,10527.67844,14568.89698,18290.38497]
["GCAM","Base","India","Emissions|CO2|Land Use","Mt CO2/yr",45.11493474,-271.5318278,-164.1007423,-96.6385398,-82.2000249]
["GCAM","Base","India","Final Energy","EJ/yr",19.82526573,29.87689088,42.98647001,56.31849343,68.31224401]
["GCAM","Base","India","Final Energy|Electricity","EJ/yr",2.47525409,5.58645252,10.10359962,15.52879943,21.07238804]
["GCAM","Base","India","Final Energy|Gases","EJ/yr",1.11677259,2.229769446,3.605172201,5.018922895,6.234128851]
["GCAM","Base","India","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Final Energy|Hydrogen","EJ/yr",0,0.00461913,0.01657586,0.037046028,0.065760639]
["GCAM","Base","India","Final Energy|Industry","EJ/yr",8.94318938,16.64164973,25.95788965,34.83471927,42.16356497]
["GCAM","Base","India","Final Energy|Liquids","EJ/yr",5.69962519,8.92292571,13.24472524,17.45144112,21.4742585]
["GCAM","Base","India","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Final Energy|Residential and Commercial","EJ/yr",8.24110835,9.58870202,12.24519379,15.53629109,19.00100728]
["GCAM","Base","India","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Final Energy|Solids","EJ/yr",4.9580323,8.8617479,12.9097048,16.0300707,17.8681197]
["GCAM","Base","India","Final Energy|Solids|Biomass","EJ/yr",7.06662986,6.61579807,6.34681809,5.98198396,5.31659998]
["GCAM","Base","India","Final Energy|Solids|Biomass|Traditional","EJ/yr",5.57558156,4.27137617,3.10669229,2.25221326,1.59758828]
["GCAM","Base","India","Final Energy|Solids|Coal","EJ/yr",3.466984,6.517326,9.669579,12.3003,14.149108]
["GCAM","Base","India","Final Energy|Transportation","EJ/yr",2.640968,3.646539126,4.783386569,5.94748307,7.147671759]
["GCAM","Base","India","Forcing","W/m2",1.86272,2.25795,2.76499,3.33767,3.94881]
["GCAM","Base","India","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","India","GDP|MER","billion US$2010/yr",1359.472148,2594.435612,4542.919593,7089.509179,10248.0131]
["GCAM","Base","India","GDP|PPP","billion US$2010/yr",4021.664064,7674.999803,13439.11054,20972.56964,30316.22682]
["GCAM","Base","India","Land Cover|Cropland|Energy Crops","million ha",0,0.333655961,0.452979406,0.605759009,0.89506114]
["GCAM","Base","India","Population","million",1224.61,1388.09,1528.6,1645.88,1733.8]
["GCAM","Base","India","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","India","Price|Primary Energy|Coal","US$2010/GJ",2.09954199,2.13469085,2.18851234,2.25799287,2.34346513]
["GCAM","Base","India","Price|Primary Energy|Gas","US$2010/GJ",5.6525,5.7436183,5.8860936,6.236807,6.7080317]
["GCAM","Base","India","Price|Primary Energy|Oil","US$2010/GJ",11.0729245,11.5144978,12.1771646,12.6786867,12.8514594]
["GCAM","Base","India","Price|Secondary Energy|Electricity","US$2010/GJ",37.73286,36.183752,35.526124,34.709903,34.051952]
["GCAM","Base","India","Primary Energy","EJ/yr",30.10578216,47.28988195,70.34994364,93.76094865,114.3243182]
["GCAM","Base","India","Primary Energy|Biomass","EJ/yr",7.13170156,7.67792617,8.78304229,10.07912326,10.08344828]
["GCAM","Base","India","Primary Energy|Biomass|Electricity","EJ/yr",0.00740519,0.0327929,0.0989961,0.1979278,0.2858013]
["GCAM","Base","India","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Biomass|Gases","EJ/yr",0,0.000615448,0.00238586,0.00662043,0.0140875]
["GCAM","Base","India","Primary Energy|Biomass|Hydrogen","EJ/yr",0,3.79117E-4,0.00126908,0.00263514,0.00414693]
["GCAM","Base","India","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Biomass|Liquids","EJ/yr",0.0156704,0.9397252,2.0975534,3.45829025,3.883438193]
["GCAM","Base","India","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Biomass|Traditional","EJ/yr",5.57558156,4.27137617,3.10669229,2.25221326,1.59758828]
["GCAM","Base","India","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Biomass|w/o CCS","EJ/yr",7.13170156,7.67792617,8.78304229,10.07912326,10.08344828]
["GCAM","Base","India","Primary Energy|Coal","EJ/yr",11.9019,21.468,34.2239,48.0538,61.3489]
["GCAM","Base","India","Primary Energy|Coal|Electricity","EJ/yr",2.35082,4.8891,8.251121,12.146861,15.88521]
["GCAM","Base","India","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.00161019,0.00601015,0.0144233,0.0278496]
["GCAM","Base","India","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Coal|w/o CCS","EJ/yr",11.9019,21.468,34.2239,48.0538,61.3489]
["GCAM","Base","India","Primary Energy|Fossil","EJ/yr",20.98332,36.624886,57.325566,78.24479,97.57897]
["GCAM","Base","India","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Fossil|w/o CCS","EJ/yr",20.98332,36.624886,57.325566,78.24479,97.57897]
["GCAM","Base","India","Primary Energy|Gas","EJ/yr",2.20582,5.00158,9.81475,15.2098,19.9087]
["GCAM","Base","India","Primary Energy|Gas|Electricity","EJ/yr",0.4240401,1.121134,2.126143,3.25718,4.252509]
["GCAM","Base","India","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Gas|Hydrogen","EJ/yr",0,4.66308E-3,0.01634083,0.0348578,0.0583013]
["GCAM","Base","India","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Gas|w/o CCS","EJ/yr",2.20582,5.00158,9.81475,15.2098,19.9087]
["GCAM","Base","India","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Hydro","EJ/yr",0.411926,0.48378,0.555634,0.654843,0.781406]
["GCAM","Base","India","Primary Energy|Non-Biomass Renewables","EJ/yr",0.4836883,0.725372102,1.232136146,1.996930086,2.931362194]
["GCAM","Base","India","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Oil","EJ/yr",6.8756,10.155306,13.286916,14.98119,16.32137]
["GCAM","Base","India","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Oil|w/o CCS","EJ/yr",6.8756,10.155306,13.286916,14.98119,16.32137]
["GCAM","Base","India","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Primary Energy|Solar","EJ/yr",8.28e-05,0.052655287,0.230837161,0.570234251,1.026700184]
["GCAM","Base","India","Primary Energy|Wind","EJ/yr",0.0716795,0.188936815,0.445664985,0.771852835,1.12325601]
["GCAM","Base","India","Resource|Cumulative Extraction|Coal","EJ",48.70795,115.597,199.3718,301.26265,424.50915]
["GCAM","Base","India","Resource|Cumulative Extraction|Gas","EJ",8.8821,38.26802,115.09862,251.03362,373.37367]
["GCAM","Base","India","Resource|Cumulative Extraction|Oil","EJ",9.2704,67.9635,162.594935,203.148825,235.158745]
["GCAM","Base","India","Secondary Energy|Electricity","EJ/yr",3.45569859,7.661797288,13.57507689,20.4276732,27.13275153]
["GCAM","Base","India","Secondary Energy|Electricity|Biomass","EJ/yr",0.00740519,0.0327929,0.0989961,0.1979278,0.2858013]
["GCAM","Base","India","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.00740519,0.0327929,0.0989961,0.1979278,0.2858013]
["GCAM","Base","India","Secondary Energy|Electricity|Coal","EJ/yr",2.35082,4.8891,8.251121,12.146861,15.88521]
["GCAM","Base","India","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",2.35082,4.8891,8.251121,12.146861,15.88521]
["GCAM","Base","India","Secondary Energy|Electricity|Fossil","EJ/yr",2.8700476,6.638257186,11.77491101,17.47425243,22.77707493]
["GCAM","Base","India","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",2.8700476,6.638257186,11.77491101,17.47425243,22.77707493]
["GCAM","Base","India","Secondary Energy|Electricity|Gas","EJ/yr",0.4240401,1.121134186,2.12614601,3.25720643,4.252655929]
["GCAM","Base","India","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",0.4240401,1.121134186,2.12614601,3.25720643,4.252655929]
["GCAM","Base","India","Secondary Energy|Electricity|Geothermal","EJ/yr",0,0.0450662,0.05541535,0.05541538,0.055415304]
["GCAM","Base","India","Secondary Energy|Electricity|Hydro","EJ/yr",0.411926,0.48378,0.555634,0.654843,0.781406]
["GCAM","Base","India","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",0.4836883,0.771158302,1.309575776,2.153238266,3.221526898]
["GCAM","Base","India","Secondary Energy|Electricity|Nuclear","EJ/yr",0.0945575,0.2195889,0.391594,0.6022547,0.8483484]
["GCAM","Base","India","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Oil","EJ/yr",0.0951875,0.628023,1.397644,2.070185,2.639209]
["GCAM","Base","India","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.0951875,0.628023,1.397644,2.070185,2.639209]
["GCAM","Base","India","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Electricity|Solar","EJ/yr",8.28e-05,0.053375287,0.252861441,0.671127051,1.261449584]
["GCAM","Base","India","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,0.00072,0.02202428,0.1008928,0.2347494]
["GCAM","Base","India","Secondary Energy|Electricity|Solar|PV","EJ/yr",8.28e-05,0.052655287,0.230837161,0.570234251,1.026700184]
["GCAM","Base","India","Secondary Energy|Electricity|Wind","EJ/yr",0.0716795,0.188936815,0.445664985,0.771852835,1.12325601]
["GCAM","Base","India","Secondary Energy|Gases","EJ/yr",2.20701959,4.5811162,7.7157033,11.02120538,13.8497107]
["GCAM","Base","India","Secondary Energy|Gases|Biomass","EJ/yr",0,0.000458,1.7959E-3,0.00503838,0.0108407]
["GCAM","Base","India","Secondary Energy|Gases|Coal","EJ/yr",0.00119959,0.0134082,0.0523074,0.166467,0.45267]
["GCAM","Base","India","Secondary Energy|Gases|Natural Gas","EJ/yr",2.20582,4.56725,7.6616,10.8497,13.3862]
["GCAM","Base","India","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Hydrogen","EJ/yr",0,0.00461923,0.016576267,0.037046117,0.065760667]
["GCAM","Base","India","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.000171,0.000584,0.00123852,0.00199053]
["GCAM","Base","India","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.000171,0.000584,0.00123852,0.00199053]
["GCAM","Base","India","Secondary Energy|Hydrogen|Coal","EJ/yr",0,1.03052E-3,0.00392463,0.00962036,0.0189378]
["GCAM","Base","India","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,1.03052E-3,0.00392463,0.00962036,0.0189378]
["GCAM","Base","India","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.000324,0.001087697,0.002383057,0.004232557]
["GCAM","Base","India","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.00291871,0.01039894,0.0225549,0.0384274]
["GCAM","Base","India","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.00291871,0.01039894,0.0225549,0.0384274]
["GCAM","Base","India","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,1.75E-4,0.000581,1.24928E-3,0.00217238]
["GCAM","Base","India","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Liquids","EJ/yr",6.17067808,10.21993179,15.8750516,21.1979048,26.14683912]
["GCAM","Base","India","Secondary Energy|Liquids|Biomass","EJ/yr",0.00761808,0.46301079,1.0452426,1.7430508,1.990669119]
["GCAM","Base","India","Secondary Energy|Liquids|Coal","EJ/yr",0,0.2365,1.266828,2.78489,4.692654]
["GCAM","Base","India","Secondary Energy|Liquids|Gas","EJ/yr",0,0.242251,1.269121,2.602575,3.924615]
["GCAM","Base","India","Secondary Energy|Liquids|Oil","EJ/yr",6.16306,9.27817,12.29386,14.067389,15.538901]
["GCAM","Base","India","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","India","Temperature|Global Mean","?C",0.824511,1.01712,1.27001,1.56514,1.88832]
["GCAM","Base","India","Water Consumption|Electricity","km3/yr",3.23949147,5.561139357,8.339332939,11.63444707,14.954628]
["GCAM","Base","India","Water Consumption|Electricity|Biomass","km3/yr",0.00289226,0.01639428,0.047220992,0.092199873,0.130275834]
["GCAM","Base","India","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.00289226,0.01639428,0.047220992,0.092199873,0.130275834]
["GCAM","Base","India","Water Consumption|Electricity|Coal","km3/yr",1.042577,2.67280212,4.7379603,7.11379611,9.36524611]
["GCAM","Base","India","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",1.042577,2.67280212,4.7379603,7.11379611,9.36524611]
["GCAM","Base","India","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Dry Cooling","km3/yr",0,0.00342893,0.006388816,0.014494903,0.028252374]
["GCAM","Base","India","Water Consumption|Electricity|Fossil","km3/yr",1.2472152,3.079516997,5.350556579,7.948977854,10.39661576]
["GCAM","Base","India","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",1.2472152,3.079516997,5.350556579,7.948977854,10.39661576]
["GCAM","Base","India","Water Consumption|Electricity|Gas","km3/yr",0.15583001,0.280298407,0.466442229,0.670271744,0.846635823]
["GCAM","Base","India","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.15583001,0.280298407,0.466442229,0.670271744,0.846635823]
["GCAM","Base","India","Water Consumption|Electricity|Geothermal","km3/yr",0,0.05442993,0.066929367,0.066929368,0.066929368]
["GCAM","Base","India","Water Consumption|Electricity|Hydro","km3/yr",1.94521,2.28452,2.62383,3.09231,3.68997]
["GCAM","Base","India","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,0.05483393,0.079287268,0.123541466,0.198649743]
["GCAM","Base","India","Water Consumption|Electricity|Nuclear","km3/yr",0.04417355,0.12565355,0.2375171,0.37528247,0.53559899]
["GCAM","Base","India","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Oil","km3/yr",0.04880819,0.12641647,0.14615405,0.16491,0.184733825]
["GCAM","Base","India","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.04880819,0.12641647,0.14615405,0.16491,0.184733825]
["GCAM","Base","India","Water Consumption|Electricity|Once Through","km3/yr",0.26057445,0.225091907,0.192916489,0.141113524,0.089256993]
["GCAM","Base","India","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Consumption|Electricity|Solar","km3/yr",4.6e-07,6.246E-4,0.013278901,0.058747509,0.135238054]
["GCAM","Base","India","Water Consumption|Electricity|Solar|CSP","km3/yr",0,0.000404,0.012357901,0.056612098,0.131720375]
["GCAM","Base","India","Water Consumption|Electricity|Solar|PV","km3/yr",4.6e-07,2.206E-4,0.000921,0.002135411,0.003517679]
["GCAM","Base","India","Water Consumption|Electricity|Wet Tower","km3/yr",1.03370656,3.04787792,5.515276634,8.384393236,11.14363096]
["GCAM","Base","India","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity","km3/yr",38.31519551,36.26770025,35.32554923,32.20389105,28.91206586]
["GCAM","Base","India","Water Withdrawal|Electricity|Biomass","km3/yr",0.09182807,0.037321679,0.093627386,0.175775258,0.244141821]
["GCAM","Base","India","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.09182807,0.037321679,0.093627386,0.175775258,0.244141821]
["GCAM","Base","India","Water Withdrawal|Electricity|Coal","km3/yr",30.58262,30.023557,29.3487557,26.874624,24.1763704]
["GCAM","Base","India","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",30.58262,30.023557,29.3487557,26.874624,24.1763704]
["GCAM","Base","India","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0.00342893,0.006388816,0.014494903,0.028252374]
["GCAM","Base","India","Water Withdrawal|Electricity|Fossil","km3/yr",36.71353658,34.67157304,33.63653088,30.43947011,27.00979632]
["GCAM","Base","India","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",36.71353658,34.67157304,33.63653088,30.43947011,27.00979632]
["GCAM","Base","India","Water Withdrawal|Electricity|Gas","km3/yr",4.93444898,4.36855855,3.98876818,3.25433107,2.50416973]
["GCAM","Base","India","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",4.93444898,4.36855855,3.98876818,3.25433107,2.50416973]
["GCAM","Base","India","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0.05442993,0.066929367,0.066929368,0.066929368]
["GCAM","Base","India","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0,0.05483393,0.079287268,0.123541466,0.198649743]
["GCAM","Base","India","Water Withdrawal|Electricity|Nuclear","km3/yr",1.5098304,1.503751,1.5151827,1.4629688,1.4559603]
["GCAM","Base","India","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Oil","km3/yr",1.1964676,0.27945749,0.299007,0.31051504,0.329256186]
["GCAM","Base","India","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",1.1964676,0.27945749,0.299007,0.31051504,0.329256186]
["GCAM","Base","India","Water Withdrawal|Electricity|Once Through","km3/yr",36.7847373,31.82097741,27.33234761,20.10669526,12.88484476]
["GCAM","Base","India","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","India","Water Withdrawal|Electricity|Sea Cooling","km3/yr",15.7649079,25.87819107,39.52321641,55.02189928,69.87687791]
["GCAM","Base","India","Water Withdrawal|Electricity|Solar","km3/yr",4.6e-07,6.246E-4,0.013278901,0.058747509,0.135238054]
["GCAM","Base","India","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.000404,0.012357901,0.056612098,0.131720375]
["GCAM","Base","India","Water Withdrawal|Electricity|Solar|PV","km3/yr",4.6e-07,2.206E-4,0.000921,0.002135411,0.003517679]
["GCAM","Base","India","Water Withdrawal|Electricity|Wet Tower","km3/yr",1.53045775,4.443073309,7.985891813,12.08056547,15.99545105]
["GCAM","Base","India","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Japan","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.193779332,0.185928463,0.180731267,0.258531321,0.201942225]
["GCAM","Base","Japan","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Japan","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0.134544647,3.80467224,3.590505097,5.010761273,4.028362387]
["GCAM","Base","Japan","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Japan","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",16.58252283,5.409192304,5.314738109,6.889826738,4.939449645]
["GCAM","Base","Japan","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","Japan","Capacity Additions|Electricity|Nuclear","GW/yr",0,0,1.179081121,2.44551539,1.948693063]
["GCAM","Base","Japan","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","Japan","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",0,2.167095066,1.866924784,2.404368024,1.816507801]
["GCAM","Base","Japan","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.075182894,0.21307732,0.498626965,0.55694748]
["GCAM","Base","Japan","Capacity Additions|Electricity|Solar|PV","GW/yr",1.316211631,0.18578339,0.175605974,0.257847539,0.239037291]
["GCAM","Base","Japan","Capacity Additions|Electricity|Wind","GW/yr",0.600131218,0.378193951,0.693182188,1.433807257,1.475604712]
["GCAM","Base","Japan","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Japan","Capacity|Electricity|Biomass|w/o CCS","GW",3.346742612,3.434178399,3.126939847,2.629649448,1.975760242]
["GCAM","Base","Japan","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Japan","Capacity|Electricity|Coal|w/o CCS","GW",43.44954972,56.07638889,55.7952142,54.61062754,53.43432902]
["GCAM","Base","Japan","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Japan","Capacity|Electricity|Gas|w/o CCS","GW",52.65928621,69.48515982,71.20631976,71.44660071,70.35878044]
["GCAM","Base","Japan","Capacity|Electricity|Hydro","GW",11.73115646,11.65330892,11.57542174,11.6619102,11.91273465]
["GCAM","Base","Japan","Capacity|Electricity|Nuclear","GW",36.55892384,32.20087096,28.34156731,24.22536501,20.07571594]
["GCAM","Base","Japan","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Japan","Capacity|Electricity|Oil|w/o CCS","GW",111.2465119,98.10570063,86.88620545,66.56380803,46.12339866]
["GCAM","Base","Japan","Capacity|Electricity|Solar|CSP","GW",0,0.24876741,0.565947189,1.373168763,2.255861225]
["GCAM","Base","Japan","Capacity|Electricity|Solar|PV","GW",2.168378995,3.021446918,3.544796582,2.156337678,2.335116216]
["GCAM","Base","Japan","Capacity|Electricity|Wind","GW",1.076864536,2.219338745,3.25356942,4.615346436,6.406425079]
["GCAM","Base","Japan","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Concentration|CH4","ppb",1882.23,2022.81,2228.22,2444.67,2623.87]
["GCAM","Base","Japan","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","Japan","Concentration|N2O","ppb",327.014,335.859,345.667,356.386,367.857]
["GCAM","Base","Japan","Emissions|CO2","Mt CO2/yr",1600.48746,1804.388801,1779.769007,1780.670479,1782.196951]
["GCAM","Base","Japan","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",860.046555,1101.809163,1099.250649,1066.473994,1020.653299]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",860.046555,1101.809163,1099.250649,1066.473994,1020.653299]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",3.6e-05,-1.34E-5,-1.21e-06,-3.39e-05,1.51e-05]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",516.5322067,680.4358081,676.2545418,655.8990673,631.7311067]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",235.0401117,314.081012,321.1958057,319.807631,311.568215]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",108.4741973,107.2923512,101.8002958,90.76732416,77.35395273]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",1627.49398,1819.470097,1795.721636,1791.303872,1789.547485]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",744.7191409,692.4117748,667.3202372,632.1352659,598.7705808]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",335.8506361,314.2550012,310.1685674,296.6417458,280.6752171]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",152.2788657,133.7543603,134.9530903,126.9228256,117.1239701]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",256.5896392,244.4024133,222.1985795,208.5706945,200.9713935]
["GCAM","Base","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",1742.821391,2228.867505,2227.652041,2225.642595,2211.430194]
["GCAM","Base","Japan","Emissions|CO2|Land Use","Mt CO2/yr",-27.00652024,-15.08129588,-15.95262972,-10.63339342,-7.350533736]
["GCAM","Base","Japan","Final Energy","EJ/yr",14.99276395,14.91798786,14.59112348,14.02755413,13.45351257]
["GCAM","Base","Japan","Final Energy|Electricity","EJ/yr",3.619541873,4.239577322,4.210751673,4.136052344,4.036583471]
["GCAM","Base","Japan","Final Energy|Gases","EJ/yr",1.5515831,1.530762854,1.606945909,1.559774686,1.473529247]
["GCAM","Base","Japan","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Final Energy|Hydrogen","EJ/yr",0,0.002777329,0.00992303,0.017902505,0.025907611]
["GCAM","Base","Japan","Final Energy|Industry","EJ/yr",6.5987764,6.591469803,6.500329505,6.26855412,6.007113593]
["GCAM","Base","Japan","Final Energy|Liquids","EJ/yr",7.68514858,7.08972335,6.740106466,6.37815899,6.09859734]
["GCAM","Base","Japan","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Final Energy|Residential and Commercial","EJ/yr",4.7541862,4.8408788,4.8882396,4.7210526,4.4877925]
["GCAM","Base","Japan","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Final Energy|Solids","EJ/yr",2.1364904,2.055147,2.0233964,1.9356656,1.8188949]
["GCAM","Base","Japan","Final Energy|Solids|Biomass","EJ/yr",0.11516,0.107541,0.101825,0.0911721,0.0770147]
["GCAM","Base","Japan","Final Energy|Solids|Biomass|Traditional","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Final Energy|Solids|Coal","EJ/yr",2.0213304,1.947606,1.9215714,1.8444935,1.7418802]
["GCAM","Base","Japan","Final Energy|Transportation","EJ/yr",3.639801353,3.485639252,3.202554373,3.037947405,2.958606476]
["GCAM","Base","Japan","Forcing","W/m2",1.86272,2.25795,2.76499,3.33767,3.94881]
["GCAM","Base","Japan","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","Japan","GDP|MER","billion US$2010/yr",5067.742045,5615.639606,6192.229641,6562.460978,6913.341929]
["GCAM","Base","Japan","GDP|PPP","billion US$2010/yr",4321.394025,4788.600371,5280.273529,5595.979315,5895.184529]
["GCAM","Base","Japan","Land Cover|Cropland|Energy Crops","million ha",0,0.118843179,0.156694149,0.217978936,0.326936431]
["GCAM","Base","Japan","Population","million",126.536,124.813,120.41,114.754,108.609]
["GCAM","Base","Japan","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","Japan","Price|Primary Energy|Coal","US$2010/GJ",2.09954199,2.13469085,2.18851234,2.25799287,2.34346513]
["GCAM","Base","Japan","Price|Primary Energy|Gas","US$2010/GJ",5.6525,5.7436183,5.8860936,6.236807,6.7080317]
["GCAM","Base","Japan","Price|Primary Energy|Oil","US$2010/GJ",11.0729245,11.5144978,12.1771646,12.6786867,12.8514594]
["GCAM","Base","Japan","Price|Secondary Energy|Electricity","US$2010/GJ",29.8672286,26.8317069,27.5759958,27.8772256,27.973415]
["GCAM","Base","Japan","Primary Energy","EJ/yr",19.53362462,20.34143151,19.97821828,20.06461756,20.06935123]
["GCAM","Base","Japan","Primary Energy|Biomass","EJ/yr",0.300876,0.323111,0.310209,0.779707,1.09231]
["GCAM","Base","Japan","Primary Energy|Biomass|Electricity","EJ/yr",0.0844343,0.0866402,0.07888894,0.0663429,0.04984606]
["GCAM","Base","Japan","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Biomass|Gases","EJ/yr",7.30833E-3,0.00998819,0.0112041,0.0135628,0.0156816]
["GCAM","Base","Japan","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.000227299,0.000755876,0.00126488,0.00162136]
["GCAM","Base","Japan","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Biomass|Liquids","EJ/yr",0,0,2.74325E-3,0.50172592,0.86220718]
["GCAM","Base","Japan","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Biomass|Traditional","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Biomass|w/o CCS","EJ/yr",0.300876,0.323111,0.310209,0.779707,1.09231]
["GCAM","Base","Japan","Primary Energy|Coal","EJ/yr",4.60141,5.36138,5.34579,6.31088,7.39118]
["GCAM","Base","Japan","Primary Energy|Coal|Electricity","EJ/yr",1.09618,1.41474,1.4076463,1.3777606,1.348084]
["GCAM","Base","Japan","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.000965387,0.00357972,0.00692326,0.0108886]
["GCAM","Base","Japan","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Coal|w/o CCS","EJ/yr",4.60141,5.36138,5.34579,6.31088,7.39118]
["GCAM","Base","Japan","Primary Energy|Fossil","EJ/yr",17.16315,18.057379,17.796261,17.744848,17.714395]
["GCAM","Base","Japan","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Fossil|w/o CCS","EJ/yr",17.16315,18.057379,17.796261,17.744848,17.714395]
["GCAM","Base","Japan","Primary Energy|Gas","EJ/yr",3.80767,4.56805,4.73125,5.44106,5.95273]
["GCAM","Base","Japan","Primary Energy|Gas|Electricity","EJ/yr",1.096252,1.548717,1.61654,1.666075,1.683276]
["GCAM","Base","Japan","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.00269493,0.00945897,0.01635091,0.02235026]
["GCAM","Base","Japan","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Gas|w/o CCS","EJ/yr",3.80767,4.56805,4.73125,5.44106,5.95273]
["GCAM","Base","Japan","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Hydro","EJ/yr",0.295963,0.293999,0.292034,0.294216,0.300544]
["GCAM","Base","Japan","Primary Energy|Non-Biomass Renewables","EJ/yr",0.3239026,0.344717533,0.362103979,0.375828169,0.411959548]
["GCAM","Base","Japan","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Oil","EJ/yr",8.75407,8.127949,7.719221,5.992908,4.370485]
["GCAM","Base","Japan","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Oil|w/o CCS","EJ/yr",8.75407,8.127949,7.719221,5.992908,4.370485]
["GCAM","Base","Japan","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Primary Energy|Solar","EJ/yr",0.0136764,0.019223261,0.022871655,0.014659584,0.016459785]
["GCAM","Base","Japan","Primary Energy|Wind","EJ/yr",0.0142632,0.031495272,0.047198324,0.066952585,0.094955763]
["GCAM","Base","Japan","Resource|Cumulative Extraction|Coal","EJ",0,17.62135,40.47035,68.92615,104.02905]
["GCAM","Base","Japan","Resource|Cumulative Extraction|Gas","EJ",0.67179,2.17638,4.45916,14.28393,27.74993]
["GCAM","Base","Japan","Resource|Cumulative Extraction|Oil","EJ",0.150154,2.4258977,6.8692222,13.7332722,23.0734672]
["GCAM","Base","Japan","Secondary Energy|Electricity","EJ/yr",3.998701115,4.667371625,4.62911639,4.533272623,4.41111308]
["GCAM","Base","Japan","Secondary Energy|Electricity|Biomass","EJ/yr",0.0844343,0.0866402,0.07888894,0.0663429,0.04984606]
["GCAM","Base","Japan","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.0844343,0.0866402,0.07888894,0.0663429,0.04984606]
["GCAM","Base","Japan","Secondary Energy|Electricity|Coal","EJ/yr",1.09618,1.41474,1.4076463,1.3777606,1.348084]
["GCAM","Base","Japan","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",1.09618,1.41474,1.4076463,1.3777606,1.348084]
["GCAM","Base","Japan","Secondary Energy|Electricity|Fossil","EJ/yr",2.543259025,3.305989132,3.354046041,3.348262624,3.300937032]
["GCAM","Base","Japan","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",2.543259025,3.305989132,3.354046041,3.348262624,3.300937032]
["GCAM","Base","Japan","Secondary Energy|Electricity|Gas","EJ/yr",1.096252025,1.548717032,1.616540041,1.666075024,1.683276032]
["GCAM","Base","Japan","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",1.096252025,1.548717032,1.616540041,1.666075024,1.683276032]
["GCAM","Base","Japan","Secondary Energy|Electricity|Geothermal","EJ/yr",0.00947519,0.01365477,0.02228952,0.03373887,0.03923304]
["GCAM","Base","Japan","Secondary Energy|Electricity|Hydro","EJ/yr",0.295963,0.293999,0.292034,0.294216,0.300544]
["GCAM","Base","Japan","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",0.33337779,0.360804293,0.391779709,0.431093099,0.490532988]
["GCAM","Base","Japan","Secondary Energy|Electricity|Nuclear","EJ/yr",1.03763,0.913938,0.8044017,0.687574,0.569797]
["GCAM","Base","Japan","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Oil","EJ/yr",0.350827,0.3425321,0.3298597,0.304427,0.269577]
["GCAM","Base","Japan","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.350827,0.3425321,0.3298597,0.304427,0.269577]
["GCAM","Base","Japan","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Electricity|Solar","EJ/yr",0.0136764,0.021655251,0.030257865,0.036185644,0.055800185]
["GCAM","Base","Japan","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,0.00243199,0.00738621,0.02152606,0.0393404]
["GCAM","Base","Japan","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.0136764,0.019223261,0.022871655,0.014659584,0.016459785]
["GCAM","Base","Japan","Secondary Energy|Electricity|Wind","EJ/yr",0.0142632,0.031495272,0.047198324,0.066952585,0.094955763]
["GCAM","Base","Japan","Secondary Energy|Gases","EJ/yr",3.8131118,4.55338722,4.70198662,4.6729026,4.5406174]
["GCAM","Base","Japan","Secondary Energy|Gases|Biomass","EJ/yr",0.0054418,0.00743722,0.00843362,0.0103217,0.0120674]
["GCAM","Base","Japan","Secondary Energy|Gases|Coal","EJ/yr",0,0.01058,0.028613,0.0662409,0.14256]
["GCAM","Base","Japan","Secondary Energy|Gases|Natural Gas","EJ/yr",3.80767,4.53537,4.66494,4.59634,4.38599]
["GCAM","Base","Japan","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Hydrogen","EJ/yr",0,0.00277836,0.009923,0.017902344,0.025907018]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,1.03E-4,3.48E-4,0.000594,0.000778]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,1.03E-4,3.48E-4,0.000594,0.000778]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.000618,0.00233755,4.61781E-3,0.00740425]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.000618,0.00233755,4.61781E-3,0.00740425]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.000259,0.000856,0.001491164,2.124768E-3]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.00169336,0.00603545,0.01059937,0.014751]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.00169336,0.00603545,0.01059937,0.014751]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,1.05E-4,0.000346,0.0006,0.000849]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Liquids","EJ/yr",8.43984,7.83619,7.448359629,7.009650027,6.636767422]
["GCAM","Base","Japan","Secondary Energy|Liquids|Biomass","EJ/yr",0,0,0.001384589,0.256608817,0.444610382]
["GCAM","Base","Japan","Secondary Energy|Liquids|Coal","EJ/yr",0,0,0.00249384,0.52826667,1.11201456]
["GCAM","Base","Japan","Secondary Energy|Liquids|Gas","EJ/yr",0,0,2.45598E-3,0.46162491,0.89057851]
["GCAM","Base","Japan","Secondary Energy|Liquids|Oil","EJ/yr",8.43984,7.83619,7.44202522,5.76314963,4.18956397]
["GCAM","Base","Japan","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","Japan","Temperature|Global Mean","?C",0.824511,1.01712,1.27001,1.56514,1.88832]
["GCAM","Base","Japan","Water Consumption|Electricity","km3/yr",1.53925889,1.548589141,1.544738315,1.562169717,1.593444731]
["GCAM","Base","Japan","Water Consumption|Electricity|Biomass","km3/yr",0.00411235,0.004066454,0.003618433,0.00289823,0.002028346]
["GCAM","Base","Japan","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.00411235,0.004066454,0.003618433,0.00289823,0.002028346]
["GCAM","Base","Japan","Water Consumption|Electricity|Coal","km3/yr",0.06260226,0.075672359,0.073184865,0.068367379,0.063438775]
["GCAM","Base","Japan","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.06260226,0.075672359,0.073184865,0.068367379,0.063438775]
["GCAM","Base","Japan","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Dry Cooling","km3/yr",0.000705,1.266526E-3,0.002418335,0.004723945,0.006963741]
["GCAM","Base","Japan","Water Consumption|Electricity|Fossil","km3/yr",0.11720722,0.130465244,0.124313396,0.112153327,0.099477515]
["GCAM","Base","Japan","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",0.11720722,0.130465244,0.124313396,0.112153327,0.099477515]
["GCAM","Base","Japan","Water Consumption|Electricity|Gas","km3/yr",0.03109399,0.034861019,0.033820643,0.031163217,0.028041829]
["GCAM","Base","Japan","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.03109399,0.034861019,0.033820643,0.031163217,0.028041829]
["GCAM","Base","Japan","Water Consumption|Electricity|Geothermal","km3/yr",0.0114435,0.016491884,0.026920743,0.040749029,0.047384771]
["GCAM","Base","Japan","Water Consumption|Electricity|Hydro","km3/yr",1.3976,1.38833,1.37905,1.38935,1.41924]
["GCAM","Base","Japan","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.0114435,0.017856547,0.031065084,0.052827395,0.069458839]
["GCAM","Base","Japan","Water Consumption|Electricity|Nuclear","km3/yr",0.00881982,0.00776846,6.57779E-3,0.0048879,3.19601E-3]
["GCAM","Base","Japan","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Oil","km3/yr",0.02351097,0.019931866,0.017307888,0.012622731,0.007996911]
["GCAM","Base","Japan","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.02351097,0.019931866,0.017307888,0.012622731,0.007996911]
["GCAM","Base","Japan","Water Consumption|Electricity|Once Through","km3/yr",0.02491664,0.023193195,0.020324907,0.015821014,0.011273725]
["GCAM","Base","Japan","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Consumption|Electricity|Solar","km3/yr",7.6e-05,0.001467099,0.004257953,0.012131231,0.022118089]
["GCAM","Base","Japan","Water Consumption|Electricity|Solar|CSP","km3/yr",0,0.001364663,0.004144341,0.012078366,0.022074068]
["GCAM","Base","Japan","Water Consumption|Electricity|Solar|PV","km3/yr",7.6e-05,0.000102436,1.13612E-4,5.29e-05,4.4e-05]
["GCAM","Base","Japan","Water Consumption|Electricity|Wet Tower","km3/yr",0.11596125,0.135696984,0.142831461,0.152221893,0.155923244]
["GCAM","Base","Japan","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity","km3/yr",3.77421685,3.537757604,3.125073404,2.482612908,1.830242866]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Biomass","km3/yr",0.08816065,0.081178422,0.0699149,0.052197602,0.032978012]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.08816065,0.081178422,0.0699149,0.052197602,0.032978012]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Coal","km3/yr",1.2035036,1.24342609,1.12650105,0.93800414,0.749243239]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",1.2035036,1.24342609,1.12650105,0.93800414,0.749243239]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.000705,1.266526E-3,0.002418335,0.004723945,0.006963741]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Fossil","km3/yr",2.2218567,2.159110199,1.940599338,1.572442576,1.201400834]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",2.2218567,2.159110199,1.940599338,1.572442576,1.201400834]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Gas","km3/yr",0.6437439,0.616874121,0.558299206,0.453931471,0.346113455]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",0.6437439,0.616874121,0.558299206,0.453931471,0.346113455]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Geothermal","km3/yr",0.0114435,0.016491884,0.026920743,0.040749029,0.047384771]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.0114435,0.017856547,0.031065084,0.052827395,0.069458839]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Nuclear","km3/yr",1.45268,1.27951,1.08338047,0.80509247,0.52636116]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Oil","km3/yr",0.3746092,0.298809988,0.255799082,0.180506965,0.10604414]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",0.3746092,0.298809988,0.255799082,0.180506965,0.10604414]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Once Through","km3/yr",3.6085259,3.346668403,2.928554901,2.280020202,1.627578092]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Sea Cooling","km3/yr",116.67573,124.6515926,118.0752726,108.5463146,98.479768]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Solar","km3/yr",7.6e-05,0.001467099,0.004257953,0.012131231,0.022118089]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.001364663,0.004144341,0.012078366,0.022074068]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Solar|PV","km3/yr",7.6e-05,0.000102436,1.13612E-4,5.29e-05,4.4e-05]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Wet Tower","km3/yr",0.16490995,0.189720239,0.193986556,0.197815896,0.195657012]
["GCAM","Base","Japan","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","LAM","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",3.059305159,3.45215266,2.935993508,2.845038527,2.56077031]
["GCAM","Base","LAM","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","LAM","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",1.874937136,5.374328901,5.801236326,6.005163621,6.043422953]
["GCAM","Base","LAM","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","LAM","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",28.363263465,25.462311326,28.625637001,26.937942257,23.363444135]
["GCAM","Base","LAM","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","LAM","Capacity Additions|Electricity|Nuclear","GW/yr",0.62988366,0.315936778,0.588572919,1.385241875,2.595338767]
["GCAM","Base","LAM","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","LAM","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",30.644527528,39.277330034,33.623716705,30.111093357,26.542493662]
["GCAM","Base","LAM","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.03797094,0.398032689,1.013937256,1.684424998]
["GCAM","Base","LAM","Capacity Additions|Electricity|Solar|PV","GW/yr",0.021182141,3.195657028,4.301257293,5.369972095,6.513050958]
["GCAM","Base","LAM","Capacity Additions|Electricity|Wind","GW/yr",1.09291875,3.992235822,7.220400909,10.288879858,12.714860288]
["GCAM","Base","LAM","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","LAM","Capacity|Electricity|Biomass|w/o CCS","GW",6.053818651,10.292280648,14.226369863,17.353338644,18.98568343]
["GCAM","Base","LAM","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","LAM","Capacity|Electricity|Coal|w/o CCS","GW",10.088133404,21.185372273,30.759155409,40.472150866,50.369256959]
["GCAM","Base","LAM","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","LAM","Capacity|Electricity|Gas|w/o CCS","GW",62.143960074,119.284284632,164.649430814,205.22402334,239.24154617]
["GCAM","Base","LAM","Capacity|Electricity|Hydro","GW",104.335089264,110.042907305,115.766695205,123.681189757,133.786941909]
["GCAM","Base","LAM","Capacity|Electricity|Nuclear","GW",3.497332854,3.796845581,4.302515291,5.598447276,9.517817732]
["GCAM","Base","LAM","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","LAM","Capacity|Electricity|Oil|w/o CCS","GW",212.502730212,294.97387471,308.215981743,303.336907026,300.134867296]
["GCAM","Base","LAM","Capacity|Electricity|Solar|CSP","GW",0,0.064309504,0.614098374,2.365880961,5.417017017]
["GCAM","Base","LAM","Capacity|Electricity|Solar|PV","GW",0.026319128,8.710316939,22.556592467,43.683168953,67.403081279]
["GCAM","Base","LAM","Capacity|Electricity|Wind","GW",1.21192107,8.884230932,21.14275645,39.304514438,55.906386417]
["GCAM","Base","LAM","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Concentration|CH4","ppb",13175.61,14159.67,15597.54,17112.69,18367.09]
["GCAM","Base","LAM","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","LAM","Concentration|N2O","ppb",2289.098,2351.013,2419.669,2494.702,2574.999]
["GCAM","Base","LAM","Emissions|CO2","Mt CO2/yr",3454.66585559,3405.3145795,4263.6349538,5184.1111276,5962.5243196]
["GCAM","Base","LAM","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",678.17781703,1326.91992368,1826.46001583,2231.85615219,2587.930538]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",678.17781703,1326.91992368,1826.46001583,2231.85615219,2587.930538]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",3.204e-06,-1.1978e-05,-3.63474e-05,9.7664e-05,-2.0903E-5]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",147.764282599,284.784060287,393.133497918,493.851025769,590.91412579]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",279.33051623,543.18341343,742.67492651,912.91679271,1049.58470856]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",251.08301489,498.951634249,690.564442596,824.764941977,947.07571456]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",2091.96890735,3180.4943696,4084.3723452,4946.2506059,5853.2690505]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",1313.9766858,1655.9518684,1920.21522481,2139.9839627,2328.3906991]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",518.23511499,684.60749563,817.75976543,922.81637189,1006.77405364]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",109.457545801,148.982152542,183.901602477,212.082973,237.75678169]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",686.2840249,822.36222018,918.5538569,1005.08461794,1083.8598637]
["GCAM","Base","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",1456.17008946,2851.4617194,3990.5303167,5037.7995672,6112.453046]
["GCAM","Base","LAM","Emissions|CO2|Land Use","Mt CO2/yr",1362.696948693,224.820209745,179.262607956,237.86052178,109.255270035]
["GCAM","Base","LAM","Final Energy","EJ/yr",27.646858608,35.01625048,41.857603453,48.097420559,53.830932475]
["GCAM","Base","LAM","Final Energy|Electricity","EJ/yr",4.107527449,6.683949703,9.133332393,11.590470774,14.030392124]
["GCAM","Base","LAM","Final Energy|Gases","EJ/yr",4.259633815,5.269648712,6.707916044,8.131369907,9.50784249]
["GCAM","Base","LAM","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Final Energy|Hydrogen","EJ/yr",0,0.046547558,0.145548054,0.291159515,0.477835881]
["GCAM","Base","LAM","Final Energy|Industry","EJ/yr",12.80485798,16.694378481,20.330762068,23.42036407,26.006563778]
["GCAM","Base","LAM","Final Energy|Liquids","EJ/yr",14.280515814,18.428385092,21.21450961,23.509731933,25.532775665]
["GCAM","Base","LAM","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Final Energy|Residential and Commercial","EJ/yr",5.259623065,6.760437256,8.455883101,10.133863269,11.822138479]
["GCAM","Base","LAM","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Final Energy|Solids","EJ/yr",3.583351141,3.514885766,3.776328982,3.860974432,3.728024262]
["GCAM","Base","LAM","Final Energy|Solids|Biomass","EJ/yr",4.289363363,3.741251353,3.655479694,3.441162662,3.046550604]
["GCAM","Base","LAM","Final Energy|Solids|Biomass|Traditional","EJ/yr",1.415830392,1.072833648,0.879968368,0.713714,0.554062052]
["GCAM","Base","LAM","Final Energy|Solids|Coal","EJ/yr",0.70981817,0.846468061,1.000817656,1.13352577,1.23553571]
["GCAM","Base","LAM","Final Energy|Transportation","EJ/yr",9.582377566,11.561434742,13.070958282,14.543193222,16.002230217]
["GCAM","Base","LAM","Forcing","W/m2",13.03904,15.80565,19.35493,23.36369,27.64167]
["GCAM","Base","LAM","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","LAM","GDP|MER","billion US$2010/yr",3557.2717763,5162.6391861,7087.1925845,9208.3159268,11608.1590262]
["GCAM","Base","LAM","GDP|PPP","billion US$2010/yr",6392.0393532,9318.2070083,12811.6912247,16658.1267669,20995.871879]
["GCAM","Base","LAM","Land Cover|Cropland|Energy Crops","million ha",0,4.199253448,5.84600866,8.021990689,11.967234345]
["GCAM","Base","LAM","Population","million",586.223,645.157,692.822,725.667,743.177]
["GCAM","Base","LAM","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","LAM","Price|Primary Energy|Coal","US$2010/GJ",14.69679393,14.94283595,15.31958638,15.80595009,16.40425591]
["GCAM","Base","LAM","Price|Primary Energy|Gas","US$2010/GJ",39.5675,40.2053281,41.2026552,43.657649,46.9562219]
["GCAM","Base","LAM","Price|Primary Energy|Oil","US$2010/GJ",77.8526254,80.8859184,85.3573043,88.6771629,89.8358931]
["GCAM","Base","LAM","Price|Secondary Energy|Electricity","US$2010/GJ",282.9519083,241.8234785,237.0763152,235.3590211,234.5261979]
["GCAM","Base","LAM","Primary Energy","EJ/yr",36.480085783,49.676721736,61.238825091,72.3545892,82.756561573]
["GCAM","Base","LAM","Primary Energy|Biomass","EJ/yr",4.738232992,5.039547348,6.392252368,8.028911,8.631354052]
["GCAM","Base","LAM","Primary Energy|Biomass|Electricity","EJ/yr",0.15273088,0.25966189,0.358914008,0.43780391,0.47898601]
["GCAM","Base","LAM","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Biomass|Gases","EJ/yr",0.003148125,0.006688175,0.011492164,0.020191777,0.03264191]
["GCAM","Base","LAM","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.003743065,0.0109339,0.020329,0.029573884]
["GCAM","Base","LAM","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Biomass|Liquids","EJ/yr",0,0.473048195,1.56608142,3.15238616,4.023626069]
["GCAM","Base","LAM","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Biomass|Traditional","EJ/yr",1.415830392,1.072833648,0.879968368,0.713714,0.554062052]
["GCAM","Base","LAM","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Biomass|w/o CCS","EJ/yr",4.738232992,5.039547348,6.392252368,8.028911,8.631354052]
["GCAM","Base","LAM","Primary Energy|Coal","EJ/yr",1.44790175,2.7505813,5.758438,10.569981,16.922253]
["GCAM","Base","LAM","Primary Energy|Coal|Electricity","EJ/yr",0.2545115,0.53448152,0.77601631,1.0210638,1.27075591]
["GCAM","Base","LAM","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.015897823,0.051781262,0.11127001,0.19861023]
["GCAM","Base","LAM","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Coal|w/o CCS","EJ/yr",1.44790175,2.7505813,5.758438,10.569981,16.922253]
["GCAM","Base","LAM","Primary Energy|Fossil","EJ/yr",25.99393915,37.5145204,47.1407472,56.361214,65.922999]
["GCAM","Base","LAM","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Fossil|w/o CCS","EJ/yr",25.99393915,37.5145204,47.1407472,56.361214,65.922999]
["GCAM","Base","LAM","Primary Energy|Gas","EJ/yr",7.841462,11.925507,17.113106,22.90563,28.32277]
["GCAM","Base","LAM","Primary Energy|Gas|Electricity","EJ/yr",1.1594933,2.6191296,3.7854286,4.8643124,5.7826742]
["GCAM","Base","LAM","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.046271996,0.1413514,0.27038851,0.41882769]
["GCAM","Base","LAM","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Gas|w/o CCS","EJ/yr",7.841462,11.925507,17.113106,22.90563,28.32277]
["GCAM","Base","LAM","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Hydro","EJ/yr",2.6322491,2.7762505,2.9206548,3.120328,3.375284]
["GCAM","Base","LAM","Primary Energy|Non-Biomass Renewables","EJ/yr",2.64846714,2.961153593,3.382748175,3.996842806,4.687542231]
["GCAM","Base","LAM","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Oil","EJ/yr",16.7045754,22.8384321,24.2692032,22.885603,20.677976]
["GCAM","Base","LAM","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Oil|w/o CCS","EJ/yr",16.7045754,22.8384321,24.2692032,22.885603,20.677976]
["GCAM","Base","LAM","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Primary Energy|Solar","EJ/yr",1.66E-4,0.058824718,0.155383885,0.306341423,0.483618182]
["GCAM","Base","LAM","Primary Energy|Wind","EJ/yr",0.01605204,0.126078375,0.30670949,0.570173383,0.828640049]
["GCAM","Base","LAM","Resource|Cumulative Extraction|Coal","EJ",11.4751085,21.190257,32.9896156,47.025807,63.6809479]
["GCAM","Base","LAM","Resource|Cumulative Extraction|Gas","EJ",38.2318,101.33149,188.286765,351.336645,566.882495]
["GCAM","Base","LAM","Resource|Cumulative Extraction|Oil","EJ",119.795575,301.69054,574.39779,858.46937,1092.151825]
["GCAM","Base","LAM","Secondary Energy|Electricity","EJ/yr",5.02022503,8.113334661,10.974310547,13.792803651,16.53011186]
["GCAM","Base","LAM","Secondary Energy|Electricity|Biomass","EJ/yr",0.15273058,0.25966189,0.358914008,0.43780391,0.47898601]
["GCAM","Base","LAM","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.15273058,0.25966189,0.358914008,0.43780391,0.47898601]
["GCAM","Base","LAM","Secondary Energy|Electricity|Coal","EJ/yr",0.2545115,0.53448152,0.77601631,1.0210638,1.27075591]
["GCAM","Base","LAM","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",0.2545115,0.53448152,0.77601631,1.0210638,1.27075591]
["GCAM","Base","LAM","Secondary Energy|Electricity|Fossil","EJ/yr",2.08415341,4.687830628,6.910620861,8.866943901,10.626851178]
["GCAM","Base","LAM","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",2.08415341,4.687830628,6.910620861,8.866943901,10.626851178]
["GCAM","Base","LAM","Secondary Energy|Electricity|Gas","EJ/yr",1.1594933,2.619135618,3.786064281,4.866677581,5.785241738]
["GCAM","Base","LAM","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",1.1594933,2.619135618,3.786064281,4.866677581,5.785241738]
["GCAM","Base","LAM","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0356112,0.09629626,0.18857116,0.283898554,0.351764462]
["GCAM","Base","LAM","Secondary Energy|Electricity|Hydro","EJ/yr",2.6322491,2.7762505,2.9206548,3.120328,3.375284]
["GCAM","Base","LAM","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",2.68407834,3.058078553,3.582659968,4.32915847,5.154136162]
["GCAM","Base","LAM","Secondary Energy|Electricity|Nuclear","EJ/yr",0.0992627,0.10776359,0.12211571,0.15889737,0.27013851]
["GCAM","Base","LAM","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Oil","EJ/yr",0.67014861,1.53421349,2.34854027,2.97920252,3.57085353]
["GCAM","Base","LAM","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.67014861,1.53421349,2.34854027,2.97920252,3.57085353]
["GCAM","Base","LAM","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Electricity|Solar","EJ/yr",1.66E-4,0.059453418,0.166724518,0.354758533,0.598447651]
["GCAM","Base","LAM","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,0.0006287,0.011340633,0.04841711,0.114829469]
["GCAM","Base","LAM","Secondary Energy|Electricity|Solar|PV","EJ/yr",1.66E-4,0.058824718,0.155383885,0.306341423,0.483618182]
["GCAM","Base","LAM","Secondary Energy|Electricity|Wind","EJ/yr",0.01605204,0.126078375,0.30670949,0.570173383,0.828640049]
["GCAM","Base","LAM","Secondary Energy|Gases","EJ/yr",7.67753639,11.33071477,14.65977013,17.69608321,20.41807648]
["GCAM","Base","LAM","Secondary Energy|Gases|Biomass","EJ/yr",2.34439E-3,0.00497988,0.00865049,0.01536631,0.02511888]
["GCAM","Base","LAM","Secondary Energy|Gases|Coal","EJ/yr",0,0.02635889,0.08931664,0.2511889,0.6419776]
["GCAM","Base","LAM","Secondary Energy|Gases|Natural Gas","EJ/yr",7.675192,11.299376,14.561803,17.429528,19.75098]
["GCAM","Base","LAM","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Hydrogen","EJ/yr",0,0.04654746,0.145548524,0.291158213,0.477835657]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.001687,0.00503029,0.00955361,0.01419486]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.001687,0.00503029,0.00955361,0.01419486]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.01017412,0.03381275,0.07421704,0.135055]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.01017412,0.03381275,0.07421704,0.135055]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.0040142,0.011780734,0.022869353,0.037171387]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.02894774,0.08991991,0.17488067,0.27592136]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.02894774,0.08991991,0.17488067,0.27592136]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,0.0017244,5.00484E-3,9.63754E-3,0.01549305]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Liquids","EJ/yr",16.02738066,21.899742952,26.019002035,29.247896457,32.121896663]
["GCAM","Base","LAM","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.234952413,0.784484969,1.595942037,2.065685845]
["GCAM","Base","LAM","Secondary Energy|Liquids|Coal","EJ/yr",0,0.20396351,1.250146422,3.131097126,5.651079465]
["GCAM","Base","LAM","Secondary Energy|Liquids|Gas","EJ/yr",0,0.20892315,1.25150627,2.900879027,4.67713944]
["GCAM","Base","LAM","Secondary Energy|Liquids|Oil","EJ/yr",15.399817,21.24760595,22.72574859,21.60331382,19.70614145]
["GCAM","Base","LAM","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","LAM","Temperature|Global Mean","?C",5.771577,7.11984,8.89007,10.95598,13.21824]
["GCAM","Base","LAM","Water Consumption|Electricity","km3/yr",13.65636673,15.071273313,16.244959394,17.640937658,19.285599248]
["GCAM","Base","LAM","Water Consumption|Electricity|Biomass","km3/yr",0.07525451,0.13310717,0.18141209,0.218199342,0.234651159]
["GCAM","Base","LAM","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.07525451,0.13310717,0.18141209,0.218199342,0.234651159]
["GCAM","Base","LAM","Water Consumption|Electricity|Coal","km3/yr",0.15183714,0.333845507,0.484199339,0.634396781,0.784965842]
["GCAM","Base","LAM","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.15183714,0.333845507,0.484199339,0.634396781,0.784965842]
["GCAM","Base","LAM","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Dry Cooling","km3/yr",0.00265062,7.234028E-3,0.01520399,0.026110689,0.03798906]
["GCAM","Base","LAM","Water Consumption|Electricity|Fossil","km3/yr",1.04707299,1.644090803,1.95966434,2.214267015,2.444542776]
["GCAM","Base","LAM","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",1.04707299,1.644090803,1.95966434,2.214267015,2.444542776]
["GCAM","Base","LAM","Water Consumption|Electricity|Gas","km3/yr",0.41952083,0.689417609,0.901700605,1.08094997,1.227018365]
["GCAM","Base","LAM","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.41952083,0.689417609,0.901700605,1.08094997,1.227018365]
["GCAM","Base","LAM","Water Consumption|Electricity|Geothermal","km3/yr",0.04300982,0.116305028,0.22775154,0.342886326,0.42485323]
["GCAM","Base","LAM","Water Consumption|Electricity|Hydro","km3/yr",12.430055,13.11006,13.791956,14.734894,15.938828]
["GCAM","Base","LAM","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.04300982,0.116657998,0.234115795,0.370052958,0.489285742]
["GCAM","Base","LAM","Water Consumption|Electricity|Nuclear","km3/yr",0.06097348,0.067134901,0.077301187,0.102656214,0.177193491]
["GCAM","Base","LAM","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Oil","km3/yr",0.47571502,0.620827687,0.573764396,0.498920264,0.432558569]
["GCAM","Base","LAM","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.47571502,0.620827687,0.573764396,0.498920264,0.432558569]
["GCAM","Base","LAM","Water Consumption|Electricity|Once Through","km3/yr",0.0730224,0.096168103,0.10972449,0.118728032,0.127157044]
["GCAM","Base","LAM","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Consumption|Electricity|Solar","km3/yr",9.2e-07,0.00057545,0.006874237,0.028034761,0.065530592]
["GCAM","Base","LAM","Water Consumption|Electricity|Solar|CSP","km3/yr",0,3.5293E-4,0.006364255,0.027166632,0.064432512]
["GCAM","Base","LAM","Water Consumption|Electricity|Solar|PV","km3/yr",9.2e-07,0.00022239,5.0997E-4,0.00086817,1.09815E-3]
["GCAM","Base","LAM","Water Consumption|Electricity|Wet Tower","km3/yr",1.15063779,1.857588741,2.327564932,2.760336808,3.180527064]
["GCAM","Base","LAM","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity","km3/yr",11.19357407,15.060342686,17.425410195,19.226508022,21.094198662]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Biomass","km3/yr",0.81549816,1.20425732,1.568521308,1.83472677,1.946927307]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.81549816,1.20425732,1.568521308,1.83472677,1.946927307]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Coal","km3/yr",1.43884108,2.61951554,3.603557357,4.567061915,5.543876856]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",1.43884108,2.61951554,3.603557357,4.567061915,5.543876856]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.00265062,7.234028E-3,0.01520399,0.026110689,0.03798906]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Fossil","km3/yr",9.65711827,13.03547402,14.866884582,16.109061148,17.198311817]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",9.65711827,13.03547402,14.866884582,16.109061148,17.198311817]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Gas","km3/yr",4.45480129,6.107051,7.36980545,8.28248311,8.969107775]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",4.45480129,6.107051,7.36980545,8.28248311,8.969107775]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Geothermal","km3/yr",0.04300982,0.116305028,0.22775154,0.342886326,0.42485323]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.04300982,0.116657998,0.234115795,0.370052958,0.489285742]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Nuclear","km3/yr",0.6779469,0.703730907,0.755378528,0.911799017,1.458575716]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Oil","km3/yr",3.7634759,4.30890748,3.893521775,3.259516123,2.685327186]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",3.7634759,4.30890748,3.893521775,3.259516123,2.685327186]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Once Through","km3/yr",9.48729121,12.390783779,14.15225634,15.411730343,16.73838404]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Sea Cooling","km3/yr",4.06280198,3.816213231,3.572243184,3.059842791,2.573953524]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Solar","km3/yr",9.2e-07,0.00057545,0.006874237,0.028034761,0.065530592]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,3.5293E-4,0.006364255,0.027166632,0.064432512]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Solar|PV","km3/yr",9.2e-07,0.00022239,5.0997E-4,0.00086817,1.09815E-3]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Wet Tower","km3/yr",1.70363132,2.662102438,3.257439883,3.787798861,4.316727482]
["GCAM","Base","LAM","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","MAF","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.012556959,0.537288021,1.177172001,2.218013541,3.56877299]
["GCAM","Base","MAF","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","MAF","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",1.917990154,12.338190639,13.15678875,15.627955155,19.896700398]
["GCAM","Base","MAF","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","MAF","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",59.165150497,37.472676865,51.295335537,60.922332696,68.562325197]
["GCAM","Base","MAF","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","MAF","Capacity Additions|Electricity|Nuclear","GW/yr",0.102233074,0.4555669,2.675848731,5.59915976,9.143747252]
["GCAM","Base","MAF","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","MAF","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",128.366894657,50.822206049,57.105418251,67.512281833,81.052437215]
["GCAM","Base","MAF","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.013079778,0.235727988,0.913512157,2.323730884]
["GCAM","Base","MAF","Capacity Additions|Electricity|Solar|PV","GW/yr",0.040525114,4.853801054,11.483565608,21.461061961,29.641551242]
["GCAM","Base","MAF","Capacity Additions|Electricity|Wind","GW/yr",0.459036989,3.842271127,9.955512196,20.047452878,34.312239243]
["GCAM","Base","MAF","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","MAF","Capacity|Electricity|Biomass|w/o CCS","GW",0.11972032,0.922218655,2.569019929,5.798662242,10.852711187]
["GCAM","Base","MAF","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","MAF","Capacity|Electricity|Coal|w/o CCS","GW",42.034409087,62.098546108,80.319908591,100.346029147,128.383014648]
["GCAM","Base","MAF","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","MAF","Capacity|Electricity|Gas|w/o CCS","GW",168.072539814,253.757723726,321.965355755,399.154590086,493.339952102]
["GCAM","Base","MAF","Capacity|Electricity|Hydro","GW",17.589964644,23.636300578,29.687270104,38.291619102,49.44946252]
["GCAM","Base","MAF","Capacity|Electricity|Nuclear","GW",1.534620046,2.345818183,6.153238626,15.642757484,31.834464319]
["GCAM","Base","MAF","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","MAF","Capacity|Electricity|Oil|w/o CCS","GW",418.523864792,458.49304766,471.173424469,492.140261147,555.461872556]
["GCAM","Base","MAF","Capacity|Electricity|Solar|CSP","GW",0,0.019604835,0.331890545,1.7707713,5.611246188]
["GCAM","Base","MAF","Capacity|Electricity|Solar|PV","GW",0.054794521,13.233925674,44.86302879,112.04627232,219.17970422]
["GCAM","Base","MAF","Capacity|Electricity|Wind","GW",0.710170991,7.277711328,23.191983281,56.927755172,110.835916804]
["GCAM","Base","MAF","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Concentration|CH4","ppb",11293.38,12136.86,13369.32,14668.02,15743.22]
["GCAM","Base","MAF","Concentration|CO2","ppm",0,0,0,0,0]
["GCAM","Base","MAF","Concentration|N2O","ppb",1962.084,2015.154,2074.002,2138.316,2207.142]
["GCAM","Base","MAF","Emissions|CO2","Mt CO2/yr",5549.1424775,5473.51443219,7043.3348197,9188.6628604,11762.9758775]
["GCAM","Base","MAF","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",2005.10596852,2834.00520747,3616.75332564,4452.9657418,5556.9729335]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",2005.10596852,2834.00520747,3616.75332564,4452.9657418,5556.9729335]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",9.5982e-07,6.8044e-06,-8.038E-6,-3.7233e-05,-0.00014085]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",618.74392144,861.253054017,1058.4199015,1249.78216565,1513.43775406]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",748.082478252,1151.566399627,1454.933193244,1781.604019421,2165.921088285]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",638.279567013,821.17599569,1103.240601908,1421.110707177,1876.498530035]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",3966.78921029,5280.8446004,6889.1331262,8834.3436029,11513.1278568]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",1793.86435264,2221.17533294,2817.84764557,3492.9555596,4331.4249388]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",771.60352704,961.75943399,1238.32821959,1561.55079324,1986.4320159]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Other Sector","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",245.246114573,292.319583537,403.27796179,536.50636352,716.14966899]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",777.01471088,967.09631594,1176.24146383,1394.89840232,1628.84325417]
["GCAM","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",4178.03085973,5893.6648408,7687.8813737,9793.8849231,12737.5658363]
["GCAM","Base","MAF","Emissions|CO2|Land Use","Mt CO2/yr",1582.353267266,192.669831232,154.201692405,354.31925582,249.848021616]
["GCAM","Base","MAF","Final Energy","EJ/yr",44.920991905,58.04392411,75.146506953,95.500248597,120.590989404]
["GCAM","Base","MAF","Final Energy|Electricity","EJ/yr",4.53228389,8.054882536,11.84752249,16.822179578,23.625706502]
["GCAM","Base","MAF","Final Energy|Gases","EJ/yr",8.411787678,10.476979951,13.478224099,16.640587949,20.010919288]
["GCAM","Base","MAF","Final Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Final Energy|Hydrogen","EJ/yr",0,0.033613634,0.140562639,0.387205016,0.927420555]
["GCAM","Base","MAF","Final Energy|Industry","EJ/yr",16.296187847,22.956053655,32.449270264,44.833831876,61.280619643]
["GCAM","Base","MAF","Final Energy|Liquids","EJ/yr",16.982188317,21.394385651,27.518179549,35.009455596,45.150889348]
["GCAM","Base","MAF","Final Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Final Energy|Residential and Commercial","EJ/yr",17.835450079,21.633769573,26.242810287,31.012285912,36.182651272]
["GCAM","Base","MAF","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Final Energy|Solids","EJ/yr",4.75738422,7.152142836,10.934735377,15.597771297,20.679250132]
["GCAM","Base","MAF","Final Energy|Solids|Biomass","EJ/yr",13.784981687,16.5736794,20.27215222,24.37775227,28.16989155]
["GCAM","Base","MAF","Final Energy|Solids|Biomass|Traditional","EJ/yr",10.2373478,10.9319195,11.2272828,11.04304917,10.19680358]
["GCAM","Base","MAF","Final Energy|Solids|Coal","EJ/yr",1.209750333,1.510382936,1.889865957,2.263068197,2.706162164]
["GCAM","Base","MAF","Final Energy|Transportation","EJ/yr",10.789353979,13.45410088,16.454426403,19.654130817,23.127718489]
["GCAM","Base","MAF","Forcing","W/m2",11.17632,13.5477,16.58994,20.02602,23.69286]
["GCAM","Base","MAF","Forcing|Kyoto Gases","W/m2",0,0,0,0,0]
["GCAM","Base","MAF","GDP|MER","billion US$2010/yr",2770.1561986,4407.6743214,6893.146667,10229.8028401,14774.99966]
["GCAM","Base","MAF","GDP|PPP","billion US$2010/yr",5813.4746017,9282.2781215,14626.4731555,21883.390508,31896.465167]
["GCAM","Base","MAF","Land Cover|Cropland|Energy Crops","million ha",0,4.482346157,6.212456891,8.79404836,13.130696888]
["GCAM","Base","MAF","Population","million",1237.419,1529.167,1828.654,2121.691,2390.765]
["GCAM","Base","MAF","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["GCAM","Base","MAF","Price|Primary Energy|Coal","US$2010/GJ",12.59721318,12.80810957,13.13103528,13.54791846,14.06075202]
["GCAM","Base","MAF","Price|Primary Energy|Gas","US$2010/GJ",33.915,34.4617098,35.3165616,37.420842,40.2481902]
["GCAM","Base","MAF","Price|Primary Energy|Oil","US$2010/GJ",66.4370948,69.0865669,73.0625677,76.0717326,77.1083688]
["GCAM","Base","MAF","Price|Secondary Energy|Electricity","US$2010/GJ",254.8436408,209.4644664,206.5874731,204.9884616,204.3272483]
["GCAM","Base","MAF","Primary Energy","EJ/yr",59.885634341,78.164465434,102.967779305,134.004171551,172.74769684]
["GCAM","Base","MAF","Primary Energy|Biomass","EJ/yr",13.7989867,17.3285435,23.1304868,30.82047417,37.53067258]
["GCAM","Base","MAF","Primary Energy|Biomass|Electricity","EJ/yr",0.0030204,0.023266699,0.064813237,0.14629329,0.27380088]
["GCAM","Base","MAF","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Biomass|Gases","EJ/yr",7.30856E-4,0.004260999,0.010406837,0.023044102,0.045555286]
["GCAM","Base","MAF","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.002716353,0.010598798,0.02712817,0.057645771]
["GCAM","Base","MAF","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Biomass|Liquids","EJ/yr",0,0.6619543,2.6160733,5.9248623,8.43087698]
["GCAM","Base","MAF","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Biomass|Modern","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Biomass|Traditional","EJ/yr",10.2373478,10.9319195,11.2272828,11.04304917,10.19680358]
["GCAM","Base","MAF","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Biomass|w/o CCS","EJ/yr",13.7989867,17.3285435,23.1304868,30.82047417,37.53067258]
["GCAM","Base","MAF","Primary Energy|Coal","EJ/yr",4.6012303,6.696784,11.853262,20.88267,34.34168]
["GCAM","Base","MAF","Primary Energy|Coal|Electricity","EJ/yr",1.0604777,1.5666718,2.02637491,2.5316099,3.2389494]
["GCAM","Base","MAF","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.01153684,0.05019458,0.1484855,0.38713356]
["GCAM","Base","MAF","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Coal|w/o CCS","EJ/yr",4.6012303,6.696784,11.853262,20.88267,34.34168]
["GCAM","Base","MAF","Primary Energy|Fossil","EJ/yr",43.958647,57.8355072,75.7185026,97.4177885,126.776308]
["GCAM","Base","MAF","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Fossil|w/o CCS","EJ/yr",43.958647,57.8355072,75.7185026,97.4177885,126.776308]
["GCAM","Base","MAF","Primary Energy|Gas","EJ/yr",16.7746767,23.502341,32.419343,43.595234,56.151498]
["GCAM","Base","MAF","Primary Energy|Gas|Electricity","EJ/yr",2.68173937,5.002077662,6.890234367,9.113270023,11.75003839]
["GCAM","Base","MAF","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.033548492,0.13716995,0.3615902,0.81819032]
["GCAM","Base","MAF","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Gas|w/o CCS","EJ/yr",16.7746767,23.502341,32.419343,43.595234,56.151498]
["GCAM","Base","MAF","Primary Energy|Geothermal","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Hydro","EJ/yr",0.4437737,0.5963155,0.7489742,0.9660516,1.2475506]
["GCAM","Base","MAF","Primary Energy|Non-Biomass Renewables","EJ/yr",0.4535256,0.790804616,1.397318986,2.576419468,4.446940593]
["GCAM","Base","MAF","Primary Energy|Nuclear","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Oil","EJ/yr",22.58274,27.6363822,31.4458976,32.9398845,36.28313]
["GCAM","Base","MAF","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Oil|w/o CCS","EJ/yr",22.58274,27.6363822,31.4458976,32.9398845,36.28313]
["GCAM","Base","MAF","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Secondary Energy Trade","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Primary Energy|Solar","EJ/yr",3.456E-4,0.0912097,0.311907938,0.784542449,1.556588703]
["GCAM","Base","MAF","Primary Energy|Wind","EJ/yr",0.0094063,0.103279416,0.336436848,0.825825419,1.64280129]
["GCAM","Base","MAF","Resource|Cumulative Extraction|Coal","EJ",29.439444,94.8675427,177.56237055,278.78111755,401.98781855]
["GCAM","Base","MAF","Resource|Cumulative Extraction|Gas","EJ",121.167375,369.332827,711.4561575,1204.9872285,1827.529745]
["GCAM","Base","MAF","Resource|Cumulative Extraction|Oil","EJ",375.365986,1014.104694,1633.76591495,2420.62151445,3303.99700045]
["GCAM","Base","MAF","Secondary Energy|Electricity","EJ/yr",5.567472138,9.790836872,14.309926929,20.216198308,28.277126811]
["GCAM","Base","MAF","Secondary Energy|Electricity|Biomass","EJ/yr",0.0030204,0.02326647,0.064813237,0.14629329,0.27380088]
["GCAM","Base","MAF","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.0030204,0.02326647,0.064813237,0.14629329,0.27380088]
["GCAM","Base","MAF","Secondary Energy|Electricity|Coal","EJ/yr",1.0604777,1.5666718,2.02637491,2.5316099,3.2389494]
["GCAM","Base","MAF","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",1.0604777,1.5666718,2.02637491,2.5316099,3.2389494]
["GCAM","Base","MAF","Secondary Energy|Electricity|Fossil","EJ/yr",5.062074338,8.825564666,12.466609569,16.702866333,22.133812347]
["GCAM","Base","MAF","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",5.062074338,8.825564666,12.466609569,16.702866333,22.133812347]
["GCAM","Base","MAF","Secondary Energy|Electricity|Gas","EJ/yr",2.68173977834,5.002149311,6.891413397,9.116759497,11.758399244]
["GCAM","Base","MAF","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",2.68173977834,5.002149311,6.891413397,9.116759497,11.758399244]
["GCAM","Base","MAF","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0052956,0.08442951,0.20017177,0.30993306,0.399449609]
["GCAM","Base","MAF","Secondary Energy|Electricity|Hydro","EJ/yr",0.4437737,0.5963155,0.7489742,0.9660516,1.2475506]
["GCAM","Base","MAF","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",0.4588212,0.875425786,1.603860443,2.923059685,4.965975084]
["GCAM","Base","MAF","Secondary Energy|Electricity|Nuclear","EJ/yr",0.0435562,0.06657995,0.17464368,0.443979,0.9035385]
["GCAM","Base","MAF","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Oil","EJ/yr",1.31985686,2.256743555,3.548821262,5.054496936,7.136463703]
["GCAM","Base","MAF","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",1.31985686,2.256743555,3.548821262,5.054496936,7.136463703]
["GCAM","Base","MAF","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Electricity|Solar","EJ/yr",3.456E-4,0.09140136,0.318277625,0.821249606,1.676173585]
["GCAM","Base","MAF","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,0.00019166,0.006369687,0.036707157,0.119584882]
["GCAM","Base","MAF","Secondary Energy|Electricity|Solar|PV","EJ/yr",3.456E-4,0.0912097,0.311907938,0.784542449,1.556588703]
["GCAM","Base","MAF","Secondary Energy|Electricity|Wind","EJ/yr",0.0094063,0.103279416,0.336436848,0.825825419,1.64280129]
["GCAM","Base","MAF","Secondary Energy|Gases","EJ/yr",16.61979992,22.73438004,28.83301733,35.24946813,42.67934664]
["GCAM","Base","MAF","Secondary Energy|Gases|Biomass","EJ/yr",5.44E-4,0.00317263,0.00783311,0.01753763,0.03505604]
["GCAM","Base","MAF","Secondary Energy|Gases|Coal","EJ/yr",0.0738831,0.09190821,0.21483622,0.5489295,1.4062676]
["GCAM","Base","MAF","Secondary Energy|Gases|Natural Gas","EJ/yr",16.54537282,22.6392992,28.610348,34.683001,41.238023]
["GCAM","Base","MAF","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Hydrogen","EJ/yr",0,0.033613324,0.140561766,0.387204733,0.92742028]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0.0012249,0.0048748,0.0127505,0.0276697]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.0012249,0.0048748,0.0127505,0.0276697]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.00738343,0.03277728,0.09903974,0.26325099]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,0.00738343,0.03277728,0.09903974,0.26325099]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0.002765355,0.010805846,0.028725353,0.06736114]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.020989239,0.08725123,0.23382867,0.53894089]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.020989239,0.08725123,0.23382867,0.53894089]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,1.2504E-3,0.00485261,0.01286047,0.03019756]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Liquids","EJ/yr",21.42290883,27.107625792,35.193782411,44.89659368,58.206301079]
["GCAM","Base","MAF","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.3287777,1.3115549,3.0038738,4.33349103]
["GCAM","Base","MAF","Secondary Energy|Liquids|Coal","EJ/yr",0.0960599,0.3556036,2.0694069,5.5222539,10.56456812]
["GCAM","Base","MAF","Secondary Energy|Liquids|Gas","EJ/yr",0.13866093,0.411547492,2.107263611,5.11027638,8.666385225]
["GCAM","Base","MAF","Secondary Energy|Liquids|Oil","EJ/yr",21.188188,26.011697,29.705557,31.2601896,34.6418567]
["GCAM","Base","MAF","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Base","MAF","Temperature|Global Mean","?C",4.947066,6.10272,7.62006,9.39084,11.32992]
["GCAM","Base","MAF","Water Consumption|Electricity","km3/yr",4.005812119,5.220386086,6.510359003,8.263574766,10.700053254]
["GCAM","Base","MAF","Water Consumption|Electricity|Biomass","km3/yr",1.40204E-3,0.00908179,0.024642832,0.055420343,0.10475234]
["GCAM","Base","MAF","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",1.40204E-3,0.00908179,0.024642832,0.055420343,0.10475234]
["GCAM","Base","MAF","Water Consumption|Electricity|Coal","km3/yr",0.56939031,0.845277396,1.090587251,1.354064362,1.721329555]
["GCAM","Base","MAF","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.56939031,0.845277396,1.090587251,1.354064362,1.721329555]
["GCAM","Base","MAF","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Dry Cooling","km3/yr",0.000394,0.006305252,0.015557042,0.026846068,0.042027521]
["GCAM","Base","MAF","Water Consumption|Electricity|Fossil","km3/yr",1.874338182,2.264288704,2.630701271,3.048840881,3.703833851]
["GCAM","Base","MAF","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",1.874338182,2.264288704,2.630701271,3.048840881,3.703833851]
["GCAM","Base","MAF","Water Consumption|Electricity|Gas","km3/yr",0.75980355,0.920398324,1.093179547,1.299048673,1.603995977]
["GCAM","Base","MAF","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.75980355,0.920398324,1.093179547,1.299048673,1.603995977]
["GCAM","Base","MAF","Water Consumption|Electricity|Geothermal","km3/yr",0.00639575,0.101972274,0.241762922,0.374330067,0.482446105]
["GCAM","Base","MAF","Water Consumption|Electricity|Hydro","km3/yr",2.095594,2.8159343,3.5368187,4.5619078,5.8912099]
["GCAM","Base","MAF","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.00639575,0.102079912,0.245337366,0.39492737,0.549545734]
["GCAM","Base","MAF","Water Consumption|Electricity|Nuclear","km3/yr",0.02808023,0.028703881,0.071907116,0.200219032,0.446760099]
["GCAM","Base","MAF","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Oil","km3/yr",0.5451443,0.498612984,0.446934473,0.395727846,0.378508319]
["GCAM","Base","MAF","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.5451443,0.498612984,0.446934473,0.395727846,0.378508319]
["GCAM","Base","MAF","Water Consumption|Electricity|Once Through","km3/yr",0.067706989,0.07897942,0.092936768,0.111577474,0.142789361]
["GCAM","Base","MAF","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Consumption|Electricity|Solar","km3/yr",1.92e-06,0.00040509,0.004526162,0.022856643,0.071050959]
["GCAM","Base","MAF","Water Consumption|Electricity|Solar|CSP","km3/yr",0,1.0759E-4,3.574444E-3,0.020597303,0.067099629]
["GCAM","Base","MAF","Water Consumption|Electricity|Solar|PV","km3/yr",1.92e-06,0.00029745,0.00095175,0.00225934,0.00395133]
["GCAM","Base","MAF","Water Consumption|Electricity|Wet Tower","km3/yr",1.84211521,2.318869615,2.864094775,3.560984084,4.620075142]
["GCAM","Base","MAF","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity","km3/yr",11.66634786,13.745976353,16.387366087,19.997768699,26.016533975]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Biomass","km3/yr",0.01131116,0.061039472,0.169677825,0.388721377,0.750049558]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.01131116,0.061039472,0.169677825,0.388721377,0.750049558]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Coal","km3/yr",3.92861822,5.5055218,6.94170981,8.474821169,10.678018831]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",3.92861822,5.5055218,6.94170981,8.474821169,10.678018831]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.000394,0.006305252,0.015557042,0.026846068,0.042027521]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Fossil","km3/yr",11.43350163,13.356971576,15.447072237,17.817085023,21.665403837]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",11.43350163,13.356971576,15.447072237,17.817085023,21.665403837]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Gas","km3/yr",4.92556648,5.615797873,6.509416193,7.587867466,9.312546513]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",4.92556648,5.615797873,6.509416193,7.587867466,9.312546513]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Geothermal","km3/yr",0.00639575,0.101972274,0.241762922,0.374330067,0.482446105]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.00639575,0.102079912,0.245337366,0.39492737,0.549545734]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Nuclear","km3/yr",0.2151374,0.225587894,0.524326941,1.394775589,3.047583516]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Oil","km3/yr",2.57931693,2.235651903,1.995946234,1.754396388,1.674838493]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",2.57931693,2.235651903,1.995946234,1.754396388,1.674838493]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Once Through","km3/yr",8.88732299,10.356895477,12.303789031,15.006444145,19.58421328]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Sea Cooling","km3/yr",68.46560572,73.139734937,74.021732856,73.732668469,74.579527399]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Solar","km3/yr",1.92e-06,0.00040509,0.004526162,0.022856643,0.071050959]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,1.0759E-4,3.574444E-3,0.020597303,0.067099629]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Solar|PV","km3/yr",1.92e-06,0.00029745,0.00095175,0.00225934,0.00395133]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Wet Tower","km3/yr",2.77862895,3.382478125,4.067068296,4.962219146,6.386341844]
["GCAM","Base","MAF","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",4.359005422,3.386775986,4.118721421,6.166113172,4.717440782]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0.134544647,59.410403746,59.641594918,79.157791129,61.632870845]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",140.707025578,47.166457489,50.359280335,64.111926163,43.413476279]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Nuclear","GW/yr",3.956690414,18.891635168,23.949896026,37.187049933,29.531544865]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",0.362991502,9.439867454,9.478186199,13.268268646,9.82442098]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Solar|CSP","GW/yr",0.360127084,0.323717697,1.833800422,5.360833416,6.320598547]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Solar|PV","GW/yr",14.552601792,4.979660228,7.131278538,11.723976089,8.630377663]
["GCAM","Base","OECD90","Capacity Additions|Electricity|Wind","GW/yr",45.582221227,18.515802328,33.381835727,63.334605788,59.043910577]
["GCAM","Base","OECD90","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity|Electricity|Biomass|w/o CCS","GW",19.456531421,18.478675561,21.272664178,25.648172722,27.220502754]
["GCAM","Base","OECD90","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity|Electricity|Coal|w/o CCS","GW",448.635091626,551.882380439,595.822906368,634.720665347,662.661721951]
["GCAM","Base","OECD90","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity|Electricity|Gas|w/o CCS","GW",363.636004914,439.044449527,478.574722258,509.84323216,520.781482154]
["GCAM","Base","OECD90","Capacity|Electricity|Hydro","GW",174.818857826,176.652119796,179.034278278,182.247114411,186.290945259]
["GCAM","Base","OECD90","Capacity|Electricity|Nuclear","GW",262.539249687,283.27928218,287.037527502,290.935939094,293.041479989]
["GCAM","Base","OECD90","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","OECD90","Capacity|Electricity|Oil|w/o CCS","GW",232.912227268,199.078471438,182.91736032,154.34790636,125.209621541]
["GCAM","Base","OECD90","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Final Energy|Gases","EJ/yr",30.579440989,32.72097307,35.625490442,36.702374861,36.80264809]
["GCAM","Base","OECD90","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Secondary Energy|Electricity|Nuclear","EJ/yr",7.451494,8.0401459,8.14681392,8.2574602,8.3172205]
["GCAM","Base","OECD90","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Base","OECD90","Water Consumption|Electricity|Wet Tower","km3/yr",8.08969138,10.543296861,12.157573321,13.993917254,15.366114965]
["GCAM","Base","REF","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["GCAM","Base","REF","Capacity|Electricity|Hydro","GW",53.896546801,57.414839389,60.969146373,66.107012619,72.828557048]
["GCAM","Base","REF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",435.35301563,488.9725429,553.86272161,577.45759835,571.68329879]
["GCAM","Base","REF","Primary Energy|Coal|w/o CCS","EJ/yr",13.53404,16.51287,18.44432,21.38248,24.71306]
["GCAM","Base","REF","Primary Energy|Oil|w/o CCS","EJ/yr",14.339827,15.9441368,16.1339332,14.0141615,11.5704628]
["GCAM","Base","REF","Secondary Energy|Gases|Biomass","EJ/yr",0.02021827,0.03160251,0.0414647,0.05537576,0.0684639]
["GCAM","Base","REF","Water Consumption|Electricity|Once Through","km3/yr",0.57719052,0.460977834,0.41263685,0.319393731,0.225953719]
["GCAM","Base","REF","Water Withdrawal|Electricity|Fossil","km3/yr",61.71708068,48.644998933,44.228857614,34.705672667,25.098347087]
["GCAM","Base","Russia","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","Base","Russia","Final Energy|Industry","EJ/yr",12.45176892,12.65370483,12.93461786,12.95258189,12.82206794]
["GCAM","Base","Russia","Primary Energy|Coal","EJ/yr",4.18338,4.84595,5.2481,6.37406,7.83386]
["GCAM","Base","Russia","Primary Energy|Hydro","EJ/yr",0.599339,0.673909,0.74848,0.827183,0.910019]
["GCAM","Base","Russia","Secondary Energy|Electricity|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","Russia","Water Consumption|Electricity|Hydro","km3/yr",2.83021,3.18235,3.53449,3.90614,4.29731]
["GCAM","Base","Russia","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Base","USA","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Base","USA","Emissions|CO2|Land Use","Mt CO2/yr",158.3648113,-619.3884708,-521.8502747,-293.1807507,-188.8320905]
["GCAM","Base","USA","Final Energy|Transportation","EJ/yr",26.07165009,27.55613872,27.55922815,27.64169655,27.83706889]
["GCAM","Base","USA","Primary Energy|Gas","EJ/yr",22.9697,25.8202,29.473,34.1493,37.5278]
["GCAM","Base","USA","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Base","USA","Secondary Energy|Liquids|Coal","EJ/yr",0,0.118681,0.74983,3.359162,6.4897155]
["GCAM","Base","USA","Water Consumption|Electricity|Solar|CSP","km3/yr",0.00177533,0.002193697,0.008083199,0.027358902,0.059526651]
["GCAM","Base","World","Capacity|Electricity|Coal|w/o CCS","GW",1225.962043,1765.57627,2151.250815,2444.617738,2665.153643]
["GCAM","Base","World","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",19500.57755,22934.03421,25958.00596,28003.41707,29561.81375]
["GCAM","Base","World","Final Energy|Residential and Commercial","EJ/yr",119.1471277,140.8092755,164.0189301,182.1533443,196.8231324]
["GCAM","Base","World","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Base","World","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.11483726,0.55641452,1.484407953,2.939901799,4.872304667]
["GCAM","Base","World","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.247995415,0.716520942,1.36835695,2.249014262]
["GCAM","Base","World","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",283.9825129,276.2289573,253.7014791,208.5126859,161.5322807]
["GCAM","Base","World","Water Withdrawal|Electricity|Cooling Pond","km3/yr",20.5683682,18.13100162,15.08613605,10.37655509,5.665009157]
["GCAM","FullTech","ASIA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,2619.998561931,4886.821023922,5975.974840761]
["GCAM","FullTech","ASIA","Final Energy|Liquids","EJ/yr",41.26959203,54.352608223,63.61815379,63.072589281,58.78892235]
["GCAM","FullTech","ASIA","GDP|PPP","billion US$2010/yr",20244.6583581,39941.5036559,65243.9946536,89757.1025621,114181.862476]
["GCAM","FullTech","ASIA","Resource|Cumulative Extraction|Oil","EJ",82.458981,297.96574045,531.18090315,697.5433482,792.84266455]
["GCAM","FullTech","ASIA","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.002067343,0.000743979,7.1027e-05,5.3502E-6]
["GCAM","FullTech","ASIA","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","ASIA","Water Withdrawal|Electricity","km3/yr",151.500858499,122.388568731,69.221818171,53.841999997,66.982422379]
["GCAM","FullTech","Brazil","Capacity|Electricity|Nuclear","GW",1.842081713,1.781327865,2.474417244,4.127945487,6.396534472]
["GCAM","FullTech","Brazil","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",78.18736358,131.1591816,1.590908795,-219.3635651,-365.4331274]
["GCAM","FullTech","Brazil","Final Energy|Solids|Biomass|Traditional","EJ/yr",0.3045312,0.3007878,0.2746053,0.2549277,0.2237154]
["GCAM","FullTech","Brazil","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","Brazil","Secondary Energy|Electricity|Gas","EJ/yr",0.1313097,0.186451122,0.412190886,0.755013245,1.03377581]
["GCAM","FullTech","Brazil","Secondary Energy|Liquids","EJ/yr",5.0771895,7.069061705,8.253590749,8.310239735,7.955717372]
["GCAM","FullTech","Brazil","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0.358414066,1.140993279,1.942066673]
["GCAM","FullTech","China","Capacity|Electricity|Biomass|w/o CCS","GW",1.627564529,9.482575469,4.836345764,0.349248478,0.020080781]
["GCAM","FullTech","China","Concentration|CO2","ppm",391.176,405.085,416.021,417.681,411.361]
["GCAM","FullTech","China","Price|Primary Energy|Coal","US$2010/GJ",2.09954199,2.08744564,2.05599836,2.01101738,1.96803577]
["GCAM","FullTech","China","Primary Energy|Non-Biomass Renewables","EJ/yr",2.76441249,4.430967523,8.930670023,12.67154593,13.9755548]
["GCAM","FullTech","China","Secondary Energy|Electricity|Coal","EJ/yr",11.8677,12.1824,6.637799,3.1966003,3.31217759]
["GCAM","FullTech","China","Secondary Energy|Hydrogen|Gas","EJ/yr",0,0.02654794,0.07778133,0.137052939,0.18423832]
["GCAM","FullTech","China","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,1.6712889,3.1447472,3.84080383]
["GCAM","FullTech","China","Water Withdrawal|Electricity|Oil","km3/yr",0.34761489,0.23512863,0.126387984,0.026171792,0.00316807]
["GCAM","FullTech","EU","Capacity|Electricity|Solar|PV","GW",12.776855024,25.121581984,38.641569492,39.052142174,43.017282276]
["GCAM","FullTech","EU","Forcing","W/m2",3.7453,4.59944,5.3885,5.76338,5.67852]
["GCAM","FullTech","EU","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0.100511709,0.2768436,0.28187978,0.30672586]
["GCAM","FullTech","EU","Resource|Cumulative Extraction|Coal","EJ",32.68475,133.31215,208.7455,262.25675,317.57465]
["GCAM","FullTech","EU","Secondary Energy|Liquids|Gas","EJ/yr",0.00339045,0.01108718,0.05827334,0.767649082,1.518683073]
["GCAM","FullTech","EU","Water Consumption|Electricity|Solar|PV","km3/yr",4.47725E-4,0.000841522,1.219967E-3,1.054407E-3,0.000889433]
["GCAM","FullTech","EU","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",14.8391979,10.272495393,6.09058035,1.967774663,0.287544505]
["GCAM","FullTech","India","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,164.1681144,1015.182228,1873.609189,2298.127482]
["GCAM","FullTech","India","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","India","Primary Energy","EJ/yr",30.10578216,39.9185909,54.05824709,62.6308076,67.34243351]
["GCAM","FullTech","India","Secondary Energy|Electricity|Fossil","EJ/yr",2.8700476,4.149484697,6.0440184,7.7850168,9.21455674]
["GCAM","FullTech","India","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,0.000538628,0.00284445,0.010197,0.0246259]
["GCAM","FullTech","India","Water Consumption|Electricity|Coal","km3/yr",1.042577,1.20526253,0.983056529,0.838730433,0.999446483]
["GCAM","FullTech","India","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0.00432959,0.027399575,0.117156517,0.297192217]
["GCAM","FullTech","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,75.87755487,179.0780985,240.4262659]
["GCAM","FullTech","Japan","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",108.4741973,116.9473219,89.47409338,26.16523112,4.037755324]
["GCAM","FullTech","Japan","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","Japan","Secondary Energy|Electricity","EJ/yr",3.998701115,4.2366174,4.875656742,5.552980965,5.904417132]
["GCAM","FullTech","Japan","Secondary Energy|Hydrogen|Coal","EJ/yr",0,0.000593609,0.002099403,0.004264644,0.00636291]
["GCAM","FullTech","Japan","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","Japan","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.011443879,0.032830092,0.099122204,0.155745129,0.206902864]
["GCAM","FullTech","Japan","Water Withdrawal|Electricity|Nuclear","km3/yr",1.45268,1.27951,1.2813082,1.3423162,1.2532691]
["GCAM","FullTech","LAM","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,-270.598232894,-595.21978906,-827.44182654]
["GCAM","FullTech","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",686.2840249,769.91554717,825.65312733,843.44171456,830.66931099]
["GCAM","FullTech","LAM","Primary Energy|Biomass|Gases","EJ/yr",0.003148125,0.011986568,0.008090198,0.002875228,0.000980562]
["GCAM","FullTech","LAM","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0.9092299,2.856936,4.787328]
["GCAM","FullTech","LAM","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.43412704,0.757421496,0.0176405947,0.004830546]
["GCAM","FullTech","LAM","Water Consumption|Electricity|Dry Cooling","km3/yr",0.002651059,0.009814302,0.030175171,0.066437671,0.113211108]
["GCAM","FullTech","LAM","Water Withdrawal|Electricity|Solar|PV","km3/yr",9.2e-07,2.97898E-4,0.000948378,1.684124E-3,0.001948267]
["GCAM","FullTech","MAF","Concentration|N2O","ppb",1962.084,2004.492,2046.33,2088.756,2130.858]
["GCAM","FullTech","MAF","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","FullTech","MAF","Primary Energy|Coal|Electricity","EJ/yr",1.0604777,1.01509187,0.535908891,0.07212363,0.004239384]
["GCAM","FullTech","MAF","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0.13180568,0.28484388,0.4122051]
["GCAM","FullTech","MAF","Secondary Energy|Electricity|Solar","EJ/yr",3.456E-4,0.238495015,0.970506797,2.280232364,4.763409857]
["GCAM","FullTech","MAF","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0.01090803,0.042699714,0.103321127]
["GCAM","FullTech","MAF","Water Withdrawal|Electricity|Gas","km3/yr",4.925566716,4.6814377,4.926524147,6.506142703,10.267329616]
["GCAM","FullTech","OECD90","Capacity Additions|Electricity|Nuclear","GW/yr",3.956690414,64.74258851,132.91324361,124.433627672,97.580330554]
["GCAM","FullTech","OECD90","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,72.349126533,158.102015541,212.371636264]
["GCAM","FullTech","OECD90","Primary Energy|Biomass|Liquids","EJ/yr",0.0194585,0.377117336,0.632192969,0.181685148,0.022587226]
["GCAM","FullTech","OECD90","Resource|Cumulative Extraction|Gas","EJ",190.87239,544.91929,944.32278,1259.489275,1631.088785]
["GCAM","FullTech","OECD90","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",5.590343495,7.496589979,12.873328434,18.31740413,23.69931535]
["GCAM","FullTech","OECD90","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",6.838480114,5.767531303,2.496486509,0.593755936,0.104197543]
["GCAM","FullTech","OECD90","Water Withdrawal|Electricity|Geothermal","km3/yr",0.156982339,0.572067701,1.421301508,1.618726441,1.649152545]
["GCAM","FullTech","REF","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.981144256,1.354435411,0.123746838,0.016523731,0.001551659]
["GCAM","FullTech","REF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",1057.3754169,642.1717788,521.88641831,362.79029988,229.15712222]
["GCAM","FullTech","REF","Primary Energy|Biomass","EJ/yr",1.6204746,3.925265,5.197135,8.266043,11.646157]
["GCAM","FullTech","REF","Primary Energy|Coal|w/ CCS","EJ/yr",0,0.018261726,0.088767191,0.275289488,0.491581953]
["GCAM","FullTech","REF","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",8.035644914,5.683097343,4.155079936,2.101430195,0.483407187]
["GCAM","FullTech","REF","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0.060849234,0.13846463,0.197245501]
["GCAM","FullTech","REF","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.053979153,0.041786106,0.023614558,5.823646E-3,1.10476E-3]
["GCAM","FullTech","REF","Water Withdrawal|Electricity|Solar","km3/yr",1.34E-5,0.007584321,0.068234944,0.231461933,0.47682723]
["GCAM","FullTech","Russia","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","FullTech","Russia","Price|Carbon","US$2010/tCO2",0,89.36608037,145.5680926,237.1149111,386.2351169]
["GCAM","FullTech","Russia","Primary Energy|Biomass|w/o CCS","EJ/yr",0.290638,0.8215059,0.7222207,0.55387142,0.61504511]
["GCAM","FullTech","Russia","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",3.29324,2.338235009,2.067601197,1.083674959,0.222451351]
["GCAM","FullTech","Russia","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","Russia","Water Consumption|Electricity|Geothermal","km3/yr",0.002195623,0.100254213,0.188686773,0.229288485,0.229288695]
["GCAM","FullTech","USA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,34.70032669,36.41549166,26.56940275]
["GCAM","FullTech","USA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",2.49e-05,9.16e-05,4.66e-05,-8.81e-07,-5.58e-08]
["GCAM","FullTech","USA","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",9426.52809,7952.511547,3008.938352,-596.5045056,-2170.046698]
["GCAM","FullTech","USA","Primary Energy|Biomass|Hydrogen","EJ/yr",0,5.54e-05,1.68e-05,2.71e-06,1.54E-7]
["GCAM","FullTech","USA","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",3.384560032,3.707582579,3.38220482,1.8523286,0.42654389]
["GCAM","FullTech","USA","Secondary Energy|Gases|Natural Gas","EJ/yr",22.9697,22.6584,24.2595,22.341,19.548]
["GCAM","FullTech","USA","Water Consumption|Electricity|Fossil","km3/yr",4.14836863,3.579383116,1.819615767,1.029402468,1.076904566]
["GCAM","FullTech","USA","Water Withdrawal|Electricity|Wet Tower","km3/yr",5.91934383,7.204681148,9.453516252,11.96159252,14.39579456]
["GCAM","FullTech","World","Capacity|Electricity|Coal|w/ CCS","GW",0,0,341.0841811,681.2231925,876.2280208]
["GCAM","FullTech","World","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",44334.07723,39789.50273,26149.38916,11635.8267,2761.586134]
["GCAM","FullTech","World","Final Energy|Other Sector","EJ/yr",0,0,0,0,0]
["GCAM","FullTech","World","Primary Energy|Coal|Hydrogen","EJ/yr",0,0.005770738,2.855523E-3,0.000483568,5.96e-05]
["GCAM","FullTech","World","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0.00566984,0.048263261,1.083673993,4.294569542,9.643087551]
["GCAM","FullTech","World","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0.111209835,0.445726812,1.063862249,1.963855]
["GCAM","FullTech","World","Water Consumption|Electricity|Oil","km3/yr",1.594917297,1.419156147,0.942801527,0.303992136,0.059637724]
["GCAM","Conv","ASIA","Capacity|Electricity|Coal|w/o CCS","GW",633.333444312,622.743069451,291.110861102,40.249305969,2.928194744]
["GCAM","Conv","ASIA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",666.00476233,1045.69574749,1142.20206592,886.34811711,438.93258981]
["GCAM","Conv","ASIA","Final Energy|Gases","EJ/yr",8.249331143,12.911617926,17.076098029,17.863744157,16.47326421]
["GCAM","Conv","ASIA","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,3.1666436,8.9331384,14.860214]
["GCAM","Conv","ASIA","Secondary Energy|Electricity|Nuclear","EJ/yr",1.0576465,4.03663615,13.04423329,22.9233552,31.42797801]
["GCAM","Conv","ASIA","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0.027801731,0.099799518,0.13671029,0.222136834]
["GCAM","Conv","ASIA","Water Consumption|Electricity|Wet Tower","km3/yr",8.149685956,10.608466966,13.63406844,18.297502291,24.461539567]
["GCAM","Conv","Brazil","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0.654385559,1.001129741,0.987210688]
["GCAM","Conv","Brazil","Capacity|Electricity|Hydro","GW",57.54693049,59.4467434,61.34655632,63.97331621,67.32741946]
["GCAM","Conv","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",22.27673547,38.6806948,37.20322513,26.81281169,17.53531008]
["GCAM","Conv","Brazil","Primary Energy|Coal|w/o CCS","EJ/yr",0.606886,0.26278863,0.22027911,0.24795715,0.31009489]
["GCAM","Conv","Brazil","Primary Energy|Oil|w/o CCS","EJ/yr",4.661719,6.791159,6.878516,5.801484,4.120558]
["GCAM","Conv","Brazil","Secondary Energy|Gases|Biomass","EJ/yr",0,0.000256753,0.000345257,0.000179296,8.44e-05]
["GCAM","Conv","Brazil","Water Consumption|Electricity|Once Through","km3/yr",0.0127618,0.013414478,0.014862787,0.017871645,0.024124224]
["GCAM","Conv","Brazil","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,4.93e-05,0.002948751,0.01359774,0.02413705]
["GCAM","Conv","China","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,43.73791064,83.39909151,101.0878837]
["GCAM","Conv","China","Final Energy|Industry","EJ/yr",45.9982558,43.49455614,43.92962284,41.23994985,38.97144754]
["GCAM","Conv","China","Primary Energy|Coal","EJ/yr",66.2219,51.3984,40.5343,32.1552,31.2072]
["GCAM","Conv","China","Primary Energy|Hydro","EJ/yr",2.60038,2.68502,2.76966,2.90904,3.10317]
["GCAM","Conv","China","Secondary Energy|Electricity|Hydro","EJ/yr",2.60038,2.68502,2.76966,2.90904,3.10317]
["GCAM","Conv","China","Water Consumption|Electricity|Hydro","km3/yr",12.2796,12.6793,13.079,13.7371,14.6538]
["GCAM","Conv","China","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0.1289947,0.2936542,0.4037401]
["GCAM","Conv","EU","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","Conv","EU","Emissions|CO2|Land Use","Mt CO2/yr",-209.70706709,90.9265818,183.91826916,132.47498836,-50.44780481]
["GCAM","Conv","EU","Final Energy|Transportation","EJ/yr",17.133098572,16.740457914,15.874236444,14.917737457,14.018499529]
["GCAM","Conv","EU","Primary Energy|Gas","EJ/yr",18.46987,15.99205,17.6151,18.10453,17.36606]
["GCAM","Conv","EU","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","Conv","EU","Secondary Energy|Liquids|Coal","EJ/yr",0.0207611,0.000415006,0.000224908,4.47312E-4,4.844e-05]
["GCAM","Conv","EU","Water Consumption|Electricity|Solar|CSP","km3/yr",1.397779E-3,0.004884705,0.024893703,0.104406208,0.192153637]
["GCAM","Conv","India","Capacity|Electricity|Coal|w/o CCS","GW",93.18001649,88.53770294,50.83743975,15.32479151,1.702616058]
["GCAM","Conv","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",853.5536752,855.344303,1049.71166,1057.915226,901.8702179]
["GCAM","Conv","India","Final Energy|Residential and Commercial","EJ/yr",8.24110835,9.86152453,11.84498748,14.23277861,16.76040129]
["GCAM","Conv","India","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","Conv","India","Secondary Energy|Electricity|Solar|PV","EJ/yr",8.28e-05,0.192890947,0.404495627,0.751157897,1.23425094]
["GCAM","Conv","India","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.002570467,0.010296308,0.021493504,0.02711257]
["GCAM","Conv","India","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","Conv","Japan","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,0.277076071,2.418016498,2.259057847,0.803281054]
["GCAM","Conv","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,76.24540293,151.5468863,188.6789132]
["GCAM","Conv","Japan","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["GCAM","Conv","Japan","GDP|PPP","billion US$2010/yr",4321.394025,4788.600371,5280.273529,5595.979315,5895.184529]
["GCAM","Conv","Japan","Resource|Cumulative Extraction|Oil","EJ",0.150154,1.53421315,3.52337665,5.30810165,6.54524665]
["GCAM","Conv","Japan","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,2.52E-6,6.35e-07,1.1e-07,9.82e-09]
["GCAM","Conv","Japan","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","Conv","Japan","Water Withdrawal|Electricity","km3/yr",3.77421721,3.304065364,2.603075999,2.052902758,1.858116181]
["GCAM","Conv","LAM","Capacity|Electricity|Nuclear","GW",3.497332854,4.236202365,7.341756159,17.401135916,40.454624698]
["GCAM","Conv","LAM","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",678.17781703,873.26878768,514.48839239,-106.581882497,-547.892654136]
["GCAM","Conv","LAM","Final Energy|Solids|Biomass|Traditional","EJ/yr",1.415830392,1.500563729,1.463862294,1.393115672,1.256984639]
["GCAM","Conv","LAM","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","Conv","LAM","Secondary Energy|Electricity|Gas","EJ/yr",1.1594933,1.77410437,2.782539083,4.354623199,5.758868721]
["GCAM","Conv","LAM","Secondary Energy|Liquids","EJ/yr",16.027380488,19.520733008,22.033284246,22.119041415,21.677035632]
["GCAM","Conv","LAM","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,1.947719744,6.068630712,10.403551848]
["GCAM","Conv","MAF","Capacity|Electricity|Biomass|w/o CCS","GW",0.119720316,1.490901627,1.092696648,0.258232289,0.029572718]
["GCAM","Conv","MAF","Concentration|CO2","ppm",2347.056,2429.448,2493.972,2502.9,2466.396]
["GCAM","Conv","MAF","Price|Primary Energy|Coal","US$2010/GJ",12.59721318,12.5132784,12.32748234,12.08064251,11.85409031]
["GCAM","Conv","MAF","Primary Energy|Non-Biomass Renewables","EJ/yr",0.453525799,1.021572826,2.056416196,3.10500156,4.551604321]
["GCAM","Conv","MAF","Secondary Energy|Electricity|Coal","EJ/yr",1.0604777,0.99579339,0.789456661,0.518078881,0.604295514]
["GCAM","Conv","MAF","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","Conv","MAF","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.011311729,0.09539555,0.075499479,0.018891336,0.002155294]
["GCAM","Conv","MAF","Water Withdrawal|Electricity|Oil","km3/yr",2.579317164,1.877934571,1.136525982,0.338785292,0.079435036]
["GCAM","Conv","OECD90","Capacity|Electricity|Solar|PV","GW",16.600457414,48.004735522,76.834273699,112.123668361,143.701272103]
["GCAM","Conv","OECD90","Forcing","W/m2",11.23818,13.85022,16.16682,17.26326,17.04798]
["GCAM","Conv","OECD90","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0.14974665,0.45953182,0.49978799,0.7164372]
["GCAM","Conv","OECD90","Resource|Cumulative Extraction|Coal","EJ",174.729401,545.43121,836.199401,1068.7620845,1322.304773]
["GCAM","Conv","OECD90","Secondary Energy|Liquids|Gas","EJ/yr",0.033444,0.08488862,0.342761587,2.191201411,3.946317719]
["GCAM","Conv","OECD90","Water Consumption|Electricity|Solar|PV","km3/yr",0.000581705,1.48186E-3,0.002473974,3.072787E-3,0.00347273]
["GCAM","Conv","OECD90","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",45.078007077,31.359989311,19.693791953,5.851832093,0.952615563]
["GCAM","Conv","REF","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,96.210097317,452.6689503,912.63211822,1297.92956802]
["GCAM","Conv","REF","Final Energy|Solar","EJ/yr",0,0,0,0,0]
["GCAM","Conv","REF","Primary Energy","EJ/yr",60.085705145,56.167791563,53.897439518,51.074665755,47.707668784]
["GCAM","Conv","REF","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","Conv","REF","Secondary Energy|Hydrogen|Nuclear","EJ/yr",0,0.002055928,0.006736014,0.016758076,0.03443045]
["GCAM","Conv","REF","Water Consumption|Electricity|Coal","km3/yr",1.273076545,0.887797487,0.290022003,0.165601329,0.212075163]
["GCAM","Conv","REF","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.00031435,0.01412473,0.038199135,0.058817121,0.074558707]
["GCAM","Conv","Russia","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,95.816116,210.8293293,312.9110365]
["GCAM","Conv","Russia","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",13.5368398,12.33125192,6.402485645,1.689451283,0.392323572]
["GCAM","Conv","Russia","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0.2463113,0.9971999,2.78064196,4.81750533]
["GCAM","Conv","Russia","Secondary Energy|Electricity","EJ/yr",5.705619999,5.200822358,6.594954836,8.01862949,9.271716818]
["GCAM","Conv","Russia","Secondary Energy|Hydrogen|Coal","EJ/yr",0,3.326931E-3,0.009731291,0.022031912,0.040266616]
["GCAM","Conv","Russia","Secondary Energy|Solids|Biomass","EJ/yr",0,0,0,0,0]
["GCAM","Conv","Russia","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.002195623,0.109736725,0.23653617,0.325586355,0.369201193]
["GCAM","Conv","USA","Capacity|Electricity|Oil|w/ CCS","GW",0,0,4.556895294,9.250221969,12.48608733]
["GCAM","Conv","USA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,-264.9322624,-516.8727519,-678.9228898]
["GCAM","Conv","USA","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0.051882,0.136844,0.222295]
["GCAM","Conv","USA","Primary Energy|Biomass|Gases","EJ/yr",0.299077,0.73232,0.300686,0.0592306,0.0125848]
["GCAM","Conv","USA","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,1.46931,3.6874,5.38131]
["GCAM","Conv","USA","Secondary Energy|Liquids|Biomass","EJ/yr",0,0.1646379,0.2380832,0.035861512,0.00434941]
["GCAM","Conv","USA","Water Consumption|Electricity|Dry Cooling","km3/yr",0.005035785,0.018358537,0.118705822,0.222374135,0.303489021]
["GCAM","Conv","USA","Water Withdrawal|Electricity|Solar|PV","km3/yr",6.11e-05,4.43156E-4,0.001112234,0.001578499,1.835155E-3]
["GCAM","Conv","World","Concentration|N2O","ppb",327.014,334.065,341.023,348.076,355.066]
["GCAM","Conv","World","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",0,0,0,0,0]
["GCAM","Conv","World","Price|Primary Energy|Oil","US$2010/GJ",11.09643486,11.49664599,12.05417629,12.54849045,12.68010891]
["GCAM","Conv","World","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,3.28443436,7.3865743,10.41239575]
["GCAM","Conv","World","Secondary Energy|Electricity|Solar","EJ/yr",0.120506105,1.537756642,3.747358882,6.52997954,10.36549923]
["GCAM","Conv","World","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0.196158504,0.58371567,1.054807279]
["GCAM","Conv","World","Water Withdrawal|Electricity|Fossil","km3/yr",395.8619339,270.9343279,127.325351,59.18773043,62.03671009]
["GCAM","NewRE","ASIA","Capacity Additions|Electricity|Nuclear","GW/yr",4.329571495,0,0,0,0]
["GCAM","NewRE","ASIA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,1.0219E-8,2.6616E-7,5.1725E-6]
["GCAM","NewRE","ASIA","Primary Energy|Biomass|Liquids","EJ/yr",0.0156704,9.43594468,22.48036051,34.650652,45.56416063]
["GCAM","NewRE","ASIA","Resource|Cumulative Extraction|Gas","EJ",72.8645475,186.2599795,330.816764,464.5607815,588.2688145]
["GCAM","NewRE","ASIA","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",3.861120979,9.669554235,26.963694862,52.211422302,85.775399726]
["GCAM","NewRE","ASIA","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",9.164297796,7.368230467,3.895971805,1.740283431,0.49672836]
["GCAM","NewRE","ASIA","Water Withdrawal|Electricity|Geothermal","km3/yr",0.084568521,0.556458886,0.860446013,0.881068702,0.881069202]
["GCAM","NewRE","Brazil","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",2.55479135,1.289090325,2.976028428,4.567656963,4.149285935]
["GCAM","NewRE","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",157.0652649,146.4314091,142.9960919,112.7149695,70.73742591]
["GCAM","NewRE","Brazil","Primary Energy|Biomass","EJ/yr",2.8166712,3.9783374,5.0832367,5.8740207,6.6351597]
["GCAM","NewRE","Brazil","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,1.29e-10,1.82e-10]
["GCAM","NewRE","Brazil","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",0.2299603,0.285542538,0.596033789,0.68034418,0.37550111]
["GCAM","NewRE","Brazil","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,1.68e-10]
["GCAM","NewRE","Brazil","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.04106301,0.033787947,0.028015925,0.01360873,0.004376994]
["GCAM","NewRE","Brazil","Water Withdrawal|Electricity|Solar","km3/yr",0,4.97e-05,0.006015433,0.074561915,0.377729043]
["GCAM","NewRE","China","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",0,0,0,0,0]
["GCAM","NewRE","China","Price|Carbon","US$2010/tCO2",0,163.9059492,266.9853668,434.8922953,708.3909708]
["GCAM","NewRE","China","Primary Energy|Coal","EJ/yr",66.2219,37.8363,16.79,4.9751,1.5957]
["GCAM","NewRE","China","Secondary Energy|Electricity|Oil","EJ/yr",0.0483861,0.2019438,0.2500857,0.087216371,0.019038191]
["GCAM","NewRE","China","Secondary Energy|Solids|Coal","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","China","Water Consumption|Electricity|Geothermal","km3/yr",0.000704341,0.136975351,0.137111459,0.136975313,0.136975612]
["GCAM","NewRE","EU","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,7.96e-09,1.38e-07,1.85e-06]
["GCAM","NewRE","EU","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",-1.03516E-4,6.28566E-4,3.86e-05,-1.47231E-4,-1.834e-05]
["GCAM","NewRE","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",4835.327286,2874.4391677,1675.916044,577.9673986,-376.87564183]
["GCAM","NewRE","EU","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.034552883,0.061556621,0.0640278,0.043644957]
["GCAM","NewRE","EU","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",2.56441,3.03751328,3.08063053,1.71321854,0.430080068]
["GCAM","NewRE","EU","Secondary Energy|Gases|Natural Gas","EJ/yr",18.46426,14.12677,12.46992,8.99021,5.15859]
["GCAM","NewRE","EU","Water Consumption|Electricity|Fossil","km3/yr",2.64141235,1.457179634,0.724161757,0.309434869,0.056842393]
["GCAM","NewRE","EU","Water Withdrawal|Electricity|Wet Tower","km3/yr",6.34630565,5.106327854,4.021437567,3.43566003,3.781936989]
["GCAM","NewRE","India","Emissions|CO2","Mt CO2/yr",2819.023243,1638.595446,1679.530225,1218.35425,387.6097089]
["GCAM","NewRE","India","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",2773.908308,1923.728825,1854.618045,1327.483606,508.4459197]
["GCAM","NewRE","India","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,6.86e-10,2.05e-08]
["GCAM","NewRE","India","Primary Energy|Coal|Hydrogen","EJ/yr",0,5.45887E-4,1.41471E-3,1.90898E-3,0.0012111]
["GCAM","NewRE","India","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,0.00304108,0.3650804,2.8626465,10.181639]
["GCAM","NewRE","India","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,5.88e-10]
["GCAM","NewRE","India","Water Consumption|Electricity|Oil","km3/yr",0.04880819,0.154539463,0.147410271,0.077515611,0.014066768]
["GCAM","NewRE","Japan","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["GCAM","NewRE","Japan","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",235.0401117,283.7106901,327.74782,261.2928029,59.18874151]
["GCAM","NewRE","Japan","Final Energy|Gases","EJ/yr",1.5515831,1.346700952,1.162144888,0.827943682,0.597958961]
["GCAM","NewRE","Japan","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,1.25e-10,2.59e-09,3.71e-08]
["GCAM","NewRE","Japan","Secondary Energy|Electricity|Nuclear","EJ/yr",1.03763,0.913939,0.758566,0.518813,0.279061]
["GCAM","NewRE","Japan","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","Japan","Water Consumption|Electricity|Wet Tower","km3/yr",0.11596125,0.13633879,0.198321737,0.542975372,1.247858912]
["GCAM","NewRE","LAM","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,2.876e-08]
["GCAM","NewRE","LAM","Capacity|Electricity|Hydro","GW",104.335089264,110.042907305,115.766695205,123.681189757,133.786941909]
["GCAM","NewRE","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",109.457545801,109.47003085,104.580176831,74.170602956,42.206339441]
["GCAM","NewRE","LAM","Primary Energy|Coal|w/o CCS","EJ/yr",1.44790175,0.45052874,0.20093965,0.10100545,0.04736288]
["GCAM","NewRE","LAM","Primary Energy|Oil|w/o CCS","EJ/yr",16.7045754,16.7572288,14.60787571,10.93040739,5.71852693]
["GCAM","NewRE","LAM","Secondary Energy|Gases|Biomass","EJ/yr",0.002344096,0.014176968,0.022953575,0.027127956,0.03745581]
["GCAM","NewRE","LAM","Water Consumption|Electricity|Once Through","km3/yr",0.073022539,0.061575694,0.051144255,0.032180883,0.01162284]
["GCAM","NewRE","LAM","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.000716137,0.049981708,0.383794509,1.379754929]
["GCAM","NewRE","MAF","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,1.257e-08]
["GCAM","NewRE","MAF","Final Energy|Industry","EJ/yr",16.296187847,18.485587624,23.51350505,28.459149292,35.177328123]
["GCAM","NewRE","MAF","Primary Energy|Coal","EJ/yr",4.6012303,2.27326686,0.96928978,0.26565563,0.12135407]
["GCAM","NewRE","MAF","Primary Energy|Hydro","EJ/yr",0.4437737,0.5963155,0.7489742,0.9660516,1.2475506]
["GCAM","NewRE","MAF","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","MAF","Water Consumption|Electricity|Hydro","km3/yr",2.095594,2.8159343,3.5368187,4.5619078,5.8912099]
["GCAM","NewRE","MAF","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,1.29e-09]
["GCAM","NewRE","OECD90","Capacity Additions|Electricity|Hydro","GW/yr",0,0,0,0,0]
["GCAM","NewRE","OECD90","Emissions|CO2|Land Use","Mt CO2/yr",363.35772935,-50.398212722,-276.739716001,-51.018647947,-5.15049201899998]
["GCAM","NewRE","OECD90","Final Energy|Transportation","EJ/yr",49.452200925,48.131544775,45.798596814,43.383720478,40.758886674]
["GCAM","NewRE","OECD90","Primary Energy|Gas","EJ/yr",48.086682,41.94934,39.635763,30.491614,17.88317]
["GCAM","NewRE","OECD90","Secondary Energy|Gases|Other","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","OECD90","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,1.942e-09,3.0101e-08]
["GCAM","NewRE","OECD90","Water Consumption|Electricity|Solar|CSP","km3/yr",3.181414E-3,0.026724106,0.816920695,3.165135113,7.486373387]
["GCAM","NewRE","REF","Capacity|Electricity|Coal|w/o CCS","GW",91.870956995,31.33965151,10.758760228,3.557245292,0.89684218]
["GCAM","NewRE","REF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",2144.0191071,1558.9560376,1435.6212707,1143.2964716,844.7906051800001]
["GCAM","NewRE","REF","Final Energy|Residential and Commercial","EJ/yr",13.942925754,13.063104673,13.756788241,13.756345797,13.508592758]
["GCAM","NewRE","REF","Primary Energy|Ocean","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","REF","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.00240838,0.083800125,0.210567006,0.377407334,0.508083999]
["GCAM","NewRE","REF","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0,0.012984386,0.028607327,0.031489075,0.022774509]
["GCAM","NewRE","REF","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["GCAM","NewRE","Russia","Capacity Additions|Electricity|Solar|CSP","GW/yr",0,1.421120358,11.96069513,39.27478857,30.06020065]
["GCAM","NewRE","Russia","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,1.04E-8,1.1e-07]
["GCAM","NewRE","Russia","Final Energy|Electricity","EJ/yr",3.06079242,4.242788453,5.37761337,7.269809734,9.097245894]
["GCAM","NewRE","Russia","Primary Energy|Gas|Hydrogen","EJ/yr",0,0.01418834,0.02779092,0.02792007,0.01816565]
["GCAM","NewRE","Russia","Resource|Cumulative Extraction|Oil","EJ",109.595,417.9577145,628.3746725,822.7350585,925.172553]
["GCAM","NewRE","Russia","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.00176409,3.55807E-3,3.63291E-3,0.00247743]
["GCAM","NewRE","Russia","Secondary Energy|Solids","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","Russia","Water Withdrawal|Electricity","km3/yr",40.03462682,16.82417736,13.06725886,8.406856258,5.106871485]
["GCAM","NewRE","USA","Capacity|Electricity|Nuclear","GW",106.407492,93.72357517,77.79010936,53.20374598,28.61741784]
["GCAM","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",4661.749091,2742.649929,1518.099689,730.7968931,183.602995]
["GCAM","NewRE","USA","Final Energy|Solids|Biomass|Traditional","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","USA","Primary Energy|Other","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","USA","Secondary Energy|Gases|Coal","EJ/yr",0.0605796,0.00152128,0.000461382,6.89e-05,5.82e-06]
["GCAM","NewRE","USA","Secondary Energy|Liquids","EJ/yr",35.1627751,34.36659763,32.04383786,28.59265879,24.63441565]
["GCAM","NewRE","USA","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,1.3e-10,1.28e-09,2.29E-8]
["GCAM","NewRE","World","Capacity|Electricity|Biomass|w/o CCS","GW",30.33483138,102.7670655,180.9603711,141.4865511,63.26598134]
["GCAM","NewRE","World","Concentration|CO2","ppm",391.176,403.282,412.336,417.412,415.669]
["GCAM","NewRE","World","Price|Primary Energy|Coal","US$2010/GJ",2.099540779,2.06495727,2.006930219,1.936319189,1.86038199]
["GCAM","NewRE","World","Primary Energy|Non-Biomass Renewables","EJ/yr",13.73596166,26.23024964,60.77624193,108.1128104,156.6068289]
["GCAM","NewRE","World","Secondary Energy|Electricity|Coal","EJ/yr",31.86571504,18.21612076,6.81720213,1.611100391,0.4632771]
["GCAM","NewRE","World","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["GCAM","NewRE","World","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",6.490091411,7.451135529,7.945236923,5.596761164,2.611397423]
["GCAM","NewRE","World","Water Withdrawal|Electricity|Oil","km3/yr",15.31810997,9.705329358,5.565104562,1.692368038,0.291422366]
["IMAGE","Base","AME","Capacity|Electricity|Oil|w/o CCS","GW",50.4349281025805,49.0364192634041,13.2131746902377,4.6080574370687,2.38181082242878]
["IMAGE","Base","AME","GDP|MER","billion US$2010/yr",2819.83213498125,4610.40063904531,7572.19237245125,11917.64405254,18470.0912058]
["IMAGE","Base","AME","Primary Energy|Biomass|w/o CCS","EJ/yr",11.6063304901123,17.5076326446533,24.3904384155273,29.2326620178223,28.4469360351562]
["IMAGE","Base","AME","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","AME","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",1.832852846,1.710982654,1.479889548,1.527691568,2.085932016]
["IMAGE","Base","AME","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","Base","AS","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.204294702312557,0.0297546294192829,0.0308915519569716,0.351253120668371,0.0653384530778033]
["IMAGE","Base","AS","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",3996.99898158586,5558.92298690636,7859.36504884333,9912.23389653947,12665.0808345817]
["IMAGE","Base","AS","Primary Energy|Biomass|Electricity","EJ/yr",0.492616136875,1.28510854801541,0.186675404430689,0.100103402418826,0.0617080095004962]
["IMAGE","Base","AS","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","AS","Secondary Energy|Electricity|Solar","EJ/yr",0.0040716,0.102247526092529,0.779786315140625,1.929658359,3.412703658]
["IMAGE","Base","AS","Water Consumption|Electricity|Once Through","km3/yr",0.44851108,0.431658579,0.467381592,0.411824698,0.217673511]
["IMAGE","Base","AS","Water Withdrawal|Electricity|Fossil","km3/yr",63.362120896,60.405036224,65.236469696,57.028718528,35.261423424]
["IMAGE","Base","ASIA","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0.149,0.434934498786926,2.32008071136475,3.19462837219238,3.47716207504272]
["IMAGE","Base","ASIA","Final Energy|Heat","EJ/yr",5.72324490356445,5.75482279968262,4.97547471618652,5.84302737426758,6.10754164123535]
["IMAGE","Base","ASIA","Price|Primary Energy|Coal","US$2010/GJ",11.1599343820333,12.9852584154153,15.0556022440457,15.5900168905234,15.8408382978106]
["IMAGE","Base","ASIA","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","ASIA","Secondary Energy|Solids|Coal","EJ/yr",29.1363791809082,33.5295915527344,34.3834561767578,29.7183446044922,28.4056950073242]
["IMAGE","Base","ASIA","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",2.657711769,10.278710498,1.76367473904201,0.066258627,0.0161841877187536]
["IMAGE","Base","ASIA","Water Withdrawal|Electricity|Oil","km3/yr",4.553784912,5.55747612,2.07220396114285,0.00246494697142524,0.000356359098151148]
["IMAGE","Base","Brazil","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["IMAGE","Base","Brazil","GDP|MER","billion US$2010/yr",1214.91827596,1785.96821562,2467.52186672,3148.95145094,3885.19976454]
["IMAGE","Base","Brazil","Primary Energy|Biomass|w/o CCS","EJ/yr",2.62205493164062,2.25814404296875,3.92982299804688,8.2860390625,10.51166015625]
["IMAGE","Base","Brazil","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","Brazil","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",0.068655664,0.06628488,0.109125,0.154484704,0.227910496]
["IMAGE","Base","Brazil","Water Consumption|Electricity|Solar|PV","km3/yr",0,0,0,0,0]
["IMAGE","Base","China","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",3.38194604492188,0.00409239912033081,0.000133640393614769,0.0243397808074951,0.00798575305938721]
["IMAGE","Base","China","Capacity|Electricity|Coal|w/o CCS","GW",709.210474609375,990.134224609375,1284.49904980469,1415.55660839844,1260.47281298828]
["IMAGE","Base","China","Final Energy|Residential and Commercial","EJ/yr",19.11665234375,26.900701171875,31.056373046875,32.9925341796875,33.0981494140625]
["IMAGE","Base","China","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","China","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","China","Secondary Energy|Hydrogen|Gas","EJ/yr",6.57194856530955e-15,0.010376717,0.0473668,0.10370601,0.238701792]
["IMAGE","Base","China","Water Withdrawal|Electricity|Fossil","km3/yr",98.766610432,147.840106496,138.2653952,80.245809152,24.091570176]
["IMAGE","Base","China","Water Withdrawal|Electricity|Solar","km3/yr",0,0.001815612,0.03626888,0.098439928,0.245959696]
["IMAGE","Base","CN","Capacity|Electricity|Wind","GW",45.20526171875,129.010551025391,167.993851074219,180.99533984375,221.617833984375]
["IMAGE","Base","CN","Final Energy|Hydrogen","EJ/yr",2.89854096990894E-9,0.0209694900512695,0.0807351226806641,0.197796005249023,0.47718359375]
["IMAGE","Base","CN","Primary Energy|Coal|w/o CCS","EJ/yr",72.1947265625,104.529296875,125.296796875,119.168,99.5512734375]
["IMAGE","Base","CN","Secondary Energy|Electricity|Hydro","EJ/yr",2.57639808,4.264294912,4.922881024,5.251227136,5.287899136]
["IMAGE","Base","CN","Water Consumption|Electricity|Hydro","km3/yr",12.023860224,19.901159424,22.97473024,24.507099136,24.678240256]
["IMAGE","Base","CN","Water Withdrawal|Electricity|Oil","km3/yr",0.5584736,1.62223296,1.876966016,2.3776630859375e-05,2.84850902557373e-08]
["IMAGE","Base","EIT","Capacity Additions|Electricity|Hydro","GW/yr",1.20797268676758,2.47514918518066,0.856374504089355,2.11232543182373,1.72205875015259]
["IMAGE","Base","EIT","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",394.314735412598,428.685173034668,479.470970153809,539.07299041748,636.160835266113]
["IMAGE","Base","EIT","Primary Energy|Biomass|w/o CCS","EJ/yr",1.89488795471191,3.86744750976562,3.85082049560547,5.16485125732422,7.66970761108398]
["IMAGE","Base","EIT","Primary Energy|Oil","EJ/yr",13.6453017578125,12.5700987548828,10.8085189208984,8.30150317382813,9.01130212402344]
["IMAGE","Base","EIT","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",0.015516,0.112373502,0.205294046,0.227358392,0.320206048]
["IMAGE","Base","EIT","Water Consumption|Electricity|Solar|PV","km3/yr",0,0,0,0,0]
["IMAGE","Base","EIT","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",11.429283584,8.67087632,6.357817696,4.412743776,3.278963272]
["IMAGE","Base","EU","Capacity|Electricity|Coal|w/o CCS","GW",120.862249023437,131.150828125,141.5017890625,172.778549804687,246.05266003418]
["IMAGE","Base","EU","Final Energy|Residential and Commercial","EJ/yr",22.5206374511719,23.1405904541016,24.0003751220703,24.475439453125,24.5294709472656]
["IMAGE","Base","EU","Primary Energy|Biomass","EJ/yr",3.53910214233398,3.11341537475586,3.33113415527344,4.11480798339844,4.9724748840332]
["IMAGE","Base","EU","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","EU","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","EU","Water Withdrawal|Electricity|Fossil","km3/yr",31.251992576,12.276998912,10.083526144,7.936143104,3.208177664]
["IMAGE","Base","EU","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["IMAGE","Base","IN","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,0,0]
["IMAGE","Base","IN","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["IMAGE","Base","IN","Primary Energy|Coal|w/o CCS","EJ/yr",11.53351953125,16.419849609375,26.844869140625,37.3262890625,51.12444921875]
["IMAGE","Base","IN","Secondary Energy|Electricity|Hydro","EJ/yr",0.443052,0.709818496,1.171596032,1.638525056,1.659261952]
["IMAGE","Base","IN","Water Consumption|Electricity|Hydro","km3/yr",2.067692032,3.312672,5.467753984,7.646879232,7.743655936]
["IMAGE","Base","IN","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","India","Capacity Additions|Electricity|Hydro","GW/yr",1.03387902832031,2.36769897460937,4.67831982421875,4.98951611328125,0.486906311035156]
["IMAGE","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",242.431304931641,341.673889160156,472.076904296875,602.15478515625,765.910095214844]
["IMAGE","Base","India","Final Energy|Transportation","EJ/yr",3.51987109375,5.1210390625,7.2492021484375,9.4817314453125,12.153490234375]
["IMAGE","Base","India","Primary Energy|Oil","EJ/yr",7.2201318359375,8.4341748046875,9.7810048828125,12.2769501953125,17.42966015625]
["IMAGE","Base","India","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["IMAGE","Base","India","Water Consumption|Electricity|Solar|PV","km3/yr",0,0,0,0,0]
["IMAGE","Base","India","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",3.998910976,2.929955072,1.800530944,0.444135616,0.008058858]
["IMAGE","Base","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0,0,0,0]
["IMAGE","Base","Japan","Final Energy|Residential and Commercial","EJ/yr",5.181615234375,5.05478295898437,5.04048901367188,4.91928894042969,4.73593603515625]
["IMAGE","Base","Japan","Primary Energy|Biomass","EJ/yr",0.376810604095459,0.558920352935791,0.319431798934937,0.226473464488983,0.367942120075226]
["IMAGE","Base","Japan","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.3300048,0.419322496,0.02696573,0,0]
["IMAGE","Base","Japan","Secondary Energy|Electricity|Other","EJ/yr",0.0094752,0.01476518,0.075464712,0.158115504,0.161125904]
["IMAGE","Base","Japan","Water Consumption|Electricity|Once Through","km3/yr",0.01991503,0.01453278,0.01212595,8.061459E-3,0.004623611]
["IMAGE","Base","Japan","Water Withdrawal|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["IMAGE","Base","LA","Capacity Additions|Electricity|Solar|PV","GW/yr",0.0473787498474121,0.616861785888672,2.44007507324219,3.07158666992188,4.26892083740234]
["IMAGE","Base","LA","Final Energy|Electricity","EJ/yr",2.78212872314453,4.50318295288086,6.54681433105469,8.85085388183594,11.2253950195313]
["IMAGE","Base","LA","Primary Energy|Coal|w/o CCS","EJ/yr",0.965243198394775,1.43702281188965,3.01193804931641,4.91538391113281,7.28403088378906]
["IMAGE","Base","LA","Primary Energy|Wind","EJ/yr",0.0123948,0.11827927134375,0.670925481,1.649993094,2.392404724]
["IMAGE","Base","LA","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,4.19176498413086e-07,3.58204215087891e-05,0.00040431306640625,0.00095115321875]
["IMAGE","Base","LA","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","LA","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","Base","LAM","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["IMAGE","Base","LAM","Final Energy|Transportation","EJ/yr",7.23551519775391,10.5297680664063,12.4762390136719,14.4497331542969,17.65949609375]
["IMAGE","Base","LAM","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","LAM","Secondary Energy|Electricity|Fossil","EJ/yr",2.020402864,2.54382450846798,3.3104232294487,4.03443892607234,5.42977822330413]
["IMAGE","Base","LAM","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","LAM","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",4.165699136,3.748910016,3.57080912,2.796359792,2.248162736]
["IMAGE","Base","MAF","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["IMAGE","Base","MAF","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",0,4.77503909738763e-05,0.000106276834960633,5.06777652909314e-05,4.69905110632903e-05]
["IMAGE","Base","MAF","Primary Energy|Biomass","EJ/yr",11.60633086586,17.5076320266724,24.3904393081665,29.2326580581665,28.4469314270019]
["IMAGE","Base","MAF","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","MAF","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",8.55307713543141e-18,0.000598012836669922,0.0067196344140625,0.05159151259375,0.1003393286875]
["IMAGE","Base","MAF","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","MAF","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["IMAGE","Base","OECD90","Capacity Additions|Electricity|Solar|PV","GW/yr",14.1717622447014,7.50722734069824,11.898523109436,18.5715386199951,28.2862513122559]
["IMAGE","Base","OECD90","Final Energy|Electricity","EJ/yr",26.1978946533203,30.9676624755859,34.1273771972656,36.0711175537109,39.7272766113281]
["IMAGE","Base","OECD90","Population","million",993.654233932495,1051.19104003906,1100.79671096802,1141.20718002319,1172.91051101685]
["IMAGE","Base","OECD90","Primary Energy|Wind","EJ/yr",0.9483948395,2.75575123667188,3.98253660059375,4.563493471,6.636395804]
["IMAGE","Base","OECD90","Secondary Energy|Solids|Biomass","EJ/yr",0.0428177289608866,0.673422738075256,1.890072265625,3.94225946044922,5.06186372375488]
["IMAGE","Base","OECD90","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","OECD90","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","Base","PAC","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["IMAGE","Base","PAC","Final Energy|Transportation","EJ/yr",7.65569189453125,8.13514111328125,7.93217309570313,8.06975695800781,8.05880383300781]
["IMAGE","Base","PAC","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","PAC","Secondary Energy|Electricity|Wind","EJ/yr",0.0414720015,0.100573849171875,0.288265332,0.430614931,0.509787406]
["IMAGE","Base","PAC","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","PAC","Water Consumption|Electricity|Solar|CSP","km3/yr",6e-06,4.61040709228516e-05,0.000749155415039063,0.00369196985351563,0.0090871273125]
["IMAGE","Base","REF","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["IMAGE","Base","REF","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",797.890171408653,840.591190382838,865.639384215077,840.901566048463,800.27784096698]
["IMAGE","Base","REF","Primary Energy|Biomass","EJ/yr",1.89488818454742,3.86744738769531,3.85082088470459,5.16485175323486,7.66970869445801]
["IMAGE","Base","REF","Primary Energy|Gas|Electricity","EJ/yr",4.795388311,4.38884280229688,4.492122644,5.236698519,6.696443479125]
["IMAGE","Base","REF","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","REF","Water Consumption|Electricity|Oil|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","REF","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["IMAGE","Base","RER","Capacity|Electricity|Storage","GW",4.1546708984375,8.2845869140625,9.0614326171875,9.8925634765625,14.247]
["IMAGE","Base","RER","Capacity|Electricity|Storage Reservoir","GWh",5.23780517578125,12.6126904296875,13.6367900390625,14.89476953125,23.763279296875]
["IMAGE","Base","RER","Population","million",409.896697998047,426.322906494141,439.567108154297,450.748992919922,459.191314697266]
["IMAGE","Base","RER","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","RER","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",2.625177882,1.454224576,1.38161184,1.848054412,2.258060086]
["IMAGE","Base","RER","Water Consumption|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","Base","RER","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","Base","Russia","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",5.501705078125,7.84777612304688,3.24762902832031,2.12380200195313,4.09045397949219]
["IMAGE","Base","Russia","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",112.85705947876,125.158351898193,151.693157196045,173.908092498779,185.217403411865]
["IMAGE","Base","Russia","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","Russia","Primary Energy|Nuclear","EJ/yr",0.622457984,0.474084,0.501348288,0.398688384,0.1208506]
["IMAGE","Base","Russia","Secondary Energy|Hydrogen|Other","EJ/yr",5.65030518373533e-16,4.95562591552734e-08,2.63440887451172e-07,1.02229498291016e-06,1.24721801757813E-6]
["IMAGE","Base","Russia","Water Consumption|Electricity|Solar|CSP","km3/yr",0,0,0,2.443101953125E-5,0.0004499216875]
["IMAGE","Base","Russia","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","Base","US","Capacity|Electricity|Solar|CSP","GW",0.471,2.0363459777832,3.53859765625,6.24060021972656,11.4765979766846]
["IMAGE","Base","US","Final Energy|Liquids","EJ/yr",35.0350347213186,35.6859752659127,31.4173186485767,26.8236028702259,30.9491724764604]
["IMAGE","Base","US","Price|Secondary Energy|Electricity","US$2010/GJ",76.6804538056564,77.5984602012253,74.5685032780075,71.9474687549591,68.7367282445526]
["IMAGE","Base","US","Secondary Energy|Electricity","EJ/yr",18.798973056,20.64300672,22.324233216,23.27200896,25.272066816]
["IMAGE","Base","US","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.083970802,0.087944109,0.042782519,0.009346631734375,0.00702085669335938]
["IMAGE","Base","US","Water Withdrawal|Electricity|Cooling Pond","km3/yr",15.463999488,11.9663104,9.202879488,6.175346176,5.1663232]
["IMAGE","Base","US","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["IMAGE","Base","USA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",0,0,0,0,0]
["IMAGE","Base","USA","Population","million",316.580810546875,342.454315185547,368.236999511719,390.884307861328,410.337097167969]
["IMAGE","Base","USA","Primary Energy|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","Base","USA","Secondary Energy|Heat","EJ/yr",0.508286992,0.446858456,0.284938824,0.20190249,0.171034489]
["IMAGE","Base","USA","Water Consumption|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","Base","USA","Water Withdrawal|Electricity|Biomass","km3/yr",2.674491904,0.516467104,9.200504E-3,0.1159824,0.03566504]
["IMAGE","Base","World","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",32.8345366210938,51.950765625,71.1470618896484,73.8198864746094,76.4533486328125]
["IMAGE","Base","World","Final Energy","EJ/yr",339.251,401.876,457.5815,541.064375,617.9113125]
["IMAGE","Base","World","GDP|PPP","billion US$2010/yr",75837.9660667187,115448.333939687,164606.511919688,214223.726970625,266061.649169687]
["IMAGE","Base","World","Primary Energy|Oil|w/o CCS","EJ/yr",173.45109375,178.061203125,165.47509375,159.429203125,179.6605]
["IMAGE","Base","World","Secondary Energy|Liquids|Oil","EJ/yr",126.47222265625,139.5712421875,141.67476171875,150.184578125,176.7823203125]
["IMAGE","Base","World","Water Consumption|Electricity|Gas","km3/yr",2.986224896,2.857379072,2.515820032,1.82640704,1.594205056]
["IMAGE","Base","World","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.0029934,0.0352959,0.136032704,0.305054912,0.636248192]
["IMAGE","FullTech","AME","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0.00318745835732835,0.0117974512977337,0.0106033783155819,0.000705958472759889]
["IMAGE","FullTech","AME","Final Energy|Solids","EJ/yr",10.5793554154858,12.439904094696,13.5848242111206,15.5460255889893,16.2958386688232]
["IMAGE","FullTech","AME","Primary Energy|Biomass|Electricity","EJ/yr",0.046571,0.671718548083027,1.5957182233942,2.41196219692157,1.07270809701438]
["IMAGE","FullTech","AME","Secondary Energy|Electricity|Other","EJ/yr",0.0107856,0.032437135796875,0.107688156375,0.280051933,0.586422528]
["IMAGE","FullTech","AME","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.638324,0.552492021,0.297889099796875,0.000661897503383636,4.8732889175415e-08]
["IMAGE","FullTech","AME","Water Consumption|Electricity|Once Through","km3/yr",0.063936545,0.0580416783125,0.05478805109375,0.0605124588125,0.076363665]
["IMAGE","FullTech","AME","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.00191652611645508,0.0094763652355957,0.04524447590625,0.176940478]
["IMAGE","FullTech","AS","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0.0406959834056882,0.89796768497763,2.53026353311725,3.80440890148748]
["IMAGE","FullTech","AS","Final Energy|Heat","EJ/yr",0.129128692626953,0.139181594848633,0.13145539855957,0.120684097290039,0.132724594116211]
["IMAGE","FullTech","AS","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0.504030078887939,4.90119440817833,11.3362383282185,16.4896260152541]
["IMAGE","FullTech","AS","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,7.36765400981903e-06,0.00700722978125,0.03262694,0.024661741]
["IMAGE","FullTech","AS","Water Consumption|Electricity","km3/yr",7.72740176,10.387473536,13.943149696,17.680470368,20.082375808]
["IMAGE","FullTech","AS","Water Withdrawal|Electricity|Coal","km3/yr",50.031750736,31.480320368,12.07230352,1.394985142,1.028375612]
["IMAGE","FullTech","AS","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,3.826366015625e-05,2.03169812754869E-4,0.00084040299631381]
["IMAGE","FullTech","ASIA","Capacity|Electricity|Solar|CSP","GW",0,0.551060380607843,5.30562412929535,62.2862271728516,162.74943359375]
["IMAGE","FullTech","ASIA","GDP|PPP","billion US$2010/yr",22275.3755112341,44774.9610060669,73452.3698183057,100532.904485571,126859.602610845]
["IMAGE","FullTech","ASIA","Primary Energy|Coal","EJ/yr",90.5119677581787,106.956051300049,83.1606264343262,30.7622022705078,32.172731262207]
["IMAGE","FullTech","ASIA","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0.00335966290637207,0.0138090840449219,0.1149600498125,0.334315643875]
["IMAGE","FullTech","ASIA","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",10.480340848,14.146516528,9.460345132,0.630672141,0.034843565]
["IMAGE","FullTech","ASIA","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","Brazil","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0,1.55356800556183E-3,2.52325493832473E-12,0,0]
["IMAGE","FullTech","Brazil","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",377.82658457756,427.226989626884,312.851171985269,235.246916733682,343.424454241991]
["IMAGE","FullTech","Brazil","Primary Energy|Biomass|Electricity","EJ/yr",0.1409236,0.0286597103203125,0.0427282844871216,0.145219958223785,0.142615973441238]
["IMAGE","FullTech","Brazil","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.0127606000900269,0.118947196960449,0.302417602539063,0.6306259765625]
["IMAGE","FullTech","Brazil","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,2.45125107467175E-11,1.19847202301025E-9,1.77083396911621e-08,2.18593406677246e-08]
["IMAGE","FullTech","Brazil","Water Consumption|Electricity|Once Through","km3/yr",0.005785216,0.004092341,0.002400457,0.004780555,0.01069589]
["IMAGE","FullTech","Brazil","Water Withdrawal|Electricity|Fossil","km3/yr",0.6690704,0.381960288,0.087829672,0.217299696,0.542516928]
["IMAGE","FullTech","China","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0.149,0,0,1.2994169921875,0.638518981933594]
["IMAGE","FullTech","China","Final Energy|Heat","EJ/yr",5.5941162109375,4.47519580078125,3.07477099609375,3.15214794921875,3.77181909179688]
["IMAGE","FullTech","China","Price|Primary Energy|Coal","US$2010/GJ",1.60544314840317,2.04243444855213,2.40476832205772,2.43541410229683,2.36236534406185]
["IMAGE","FullTech","China","Resource|Cumulative Extraction|Gas","EJ",22.58471936,112.529301504,230.937296896,331.345395712,378.344112128]
["IMAGE","FullTech","China","Water Consumption|Electricity","km3/yr",19.681189888,28.877979648,25.934790656,30.619490304,31.969820672]
["IMAGE","FullTech","China","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,6.144298046875e-05,6.92682734375e-05,0.284949088,0.721530496]
["IMAGE","FullTech","China","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0,0,1.37558097839355E-8,2.17841491699219e-08]
["IMAGE","FullTech","CN","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",3387.06709941228,5883.33165645599,4766.2521203359,280.110701918602,-740.096877018611]
["IMAGE","FullTech","CN","GDP|PPP","billion US$2010/yr",12769.8276729687,28174.5685483203,46203.4589414844,59954.0346085156,70070.8379628125]
["IMAGE","FullTech","CN","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,6.35552997,9.417372552]
["IMAGE","FullTech","CN","Secondary Energy|Electricity|Wind|Offshore","EJ/yr",0.001080163,0.008654503,0.009792466,0.300487616,0.371073696]
["IMAGE","FullTech","CN","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",7.325519872,11.516709888,8.143242752,0.570743488,0.01326914]
["IMAGE","FullTech","CN","Water Consumption|Electricity|Solar|PV","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","EIT","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.262267925262451,0.558558124542236,0,0,1.46211702376604E-5]
["IMAGE","FullTech","EIT","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",3330.0302041322,2910.32517477497,1992.10826128535,1263.68269639835,1055.44125421345]
["IMAGE","FullTech","EIT","Final Energy|Residential and Commercial","EJ/yr",12.7310391693115,12.1670986785889,11.2740419006348,10.7050317382812,11.5937359619141]
["IMAGE","FullTech","EIT","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.196017492294312,1.6126782989502,2.51331045532227,3.4420915222168]
["IMAGE","FullTech","EIT","Secondary Energy|Hydrogen|Electricity","EJ/yr",5.01812580587768e-22,7.39589455343932e-22,9.28297682295957E-22,4.13030483196372e-22,1.7561456971171e-24]
["IMAGE","FullTech","EIT","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,2.24478578125E-3,0.0086769773984375,0.020930877,0.07975111]
["IMAGE","FullTech","EIT","Water Withdrawal|Electricity|Fossil","km3/yr",24.5428864,12.37139712,5.073107648,2.782082368,2.436757232]
["IMAGE","FullTech","EU","Capacity|Electricity|Storage Reservoir|Daily","GWh",6.69706420898437,13.5623698730469,12.6818543701172,16.0553292236328,125.027650146484]
["IMAGE","FullTech","EU","Final Energy|Heat","EJ/yr",2.12878509521484,1.94724603271484,1.64937744140625,1.44073300170898,1.51745980834961]
["IMAGE","FullTech","EU","Price|Primary Energy|Coal","US$2010/GJ",4.22058018900871,4.59954903023243,4.96371421333313,4.85578843588829,4.6696391432786]
["IMAGE","FullTech","EU","Secondary Energy|Electricity|Hydro","EJ/yr",2.064535552,1.996197872,2.186335744,2.343218944,2.34357072]
["IMAGE","FullTech","EU","Water Consumption|Electricity","km3/yr",10.858511872,9.163320064,9.158755072,9.29900224,8.81546688]
["IMAGE","FullTech","EU","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.0011415,0.01153071,0.0112951722420044,0.010911721703125,0.048305317]
["IMAGE","FullTech","EU","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0.0004924743125,0.0039122406875,0.003947867375,0.003253611296875]
["IMAGE","FullTech","IN","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",934.566924969355,951.156755288442,394.42112048467,-257.819766799609,-91.3787620762984]
["IMAGE","FullTech","IN","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",103.209171295166,122.161773681641,129.332080841064,121.650058746338,139.720809936523]
["IMAGE","FullTech","IN","Primary Energy|Biomass|w/o CCS","EJ/yr",7.3773408203125,9.03222265625,8.15651904296875,6.564373046875,7.42788623046875]
["IMAGE","FullTech","IN","Primary Energy|Oil","EJ/yr",7.22013623046875,7.4150068359375,7.09698193359375,7.39139697265625,10.583400390625]
["IMAGE","FullTech","IN","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["IMAGE","FullTech","IN","Water Consumption|Electricity|Solar|PV","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","IN","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",3.998910976,3.99802112,2.415497984,0.01129695,0.002623479]
["IMAGE","FullTech","India","Capacity|Electricity|Coal|w/o CCS","GW",48.93421875,63.7324296905548,50.1438593780548,0.155451602175888,0.00221647491329372]
["IMAGE","FullTech","India","Final Energy|Residential and Commercial","EJ/yr",7.99343341064453,9.45206762695313,10.4031395263672,11.943037109375,15.2804643554687]
["IMAGE","FullTech","India","Primary Energy|Biomass","EJ/yr",7.37734106445312,9.09767211914063,9.89111987304688,10.0307026367188,8.97203173828125]
["IMAGE","FullTech","India","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0.488503104083495,1.024172032,0.337097088018542]
["IMAGE","FullTech","India","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,3.71587E-3,0.04704416,0.155423904,0.286380608]
["IMAGE","FullTech","India","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.070319048,0.089060632,0.01066863,0,0]
["IMAGE","FullTech","India","Water Withdrawal|Electricity|Solar","km3/yr",0,1.73274E-3,0.003426304,0.007754189,0.05820022]
["IMAGE","FullTech","Japan","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",276.740819215775,172.256588935852,115.868313858906,1.68540641122187,0.0259471515467643]
["IMAGE","FullTech","Japan","Price|Primary Energy|Coal","US$2010/GJ",2.04675455912352,2.28318616207123,2.52620997776031,2.49670962436199,2.40246426308632]
["IMAGE","FullTech","Japan","Primary Energy|Fossil","EJ/yr",16.6489641113281,13.3654897460938,9.23275390625,6.6037080078125,7.22657690429688]
["IMAGE","FullTech","Japan","Secondary Energy|Hydrogen|Biomass","EJ/yr",4.54755909740925e-11,1.2184431099236e-05,0.01230395,0.0319475,0.02471403]
["IMAGE","FullTech","Japan","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,0,0,0,0.000770086625]
["IMAGE","FullTech","Japan","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.05713302,0.036999152,0.003774879,1.57253002929688e-06,1.88937401771545e-09]
["IMAGE","FullTech","LA","Capacity|Electricity|Storage Reservoir","GWh",1.05022332763672,1.55232933044434,2.0310686340332,6.1102021484375,52.5860502929687]
["IMAGE","FullTech","LA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",366.531860351562,517.46614074707,468.874214172363,450.677688598633,643.260917663574]
["IMAGE","FullTech","LA","Final Energy|Transportation","EJ/yr",5.69823919677734,7.67519506835938,7.5024990234375,7.75492297363281,10.4065482177734]
["IMAGE","FullTech","LA","Primary Energy|Oil","EJ/yr",11.1064379882813,12.0875101318359,9.25086633300781,8.02870727539063,10.5085832519531]
["IMAGE","FullTech","LA","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["IMAGE","FullTech","LA","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,3.51077487792969e-05,0.006311204,0.02597139,0.057057227]
["IMAGE","FullTech","LA","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",2.622987072,1.62977392,0.92951236,0.189507192,0.094870465]
["IMAGE","FullTech","LAM","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,1.07235116194223E-4,1.07167014448351,20.1373600527101,34.6431268068651]
["IMAGE","FullTech","LAM","Final Energy|Residential and Commercial","EJ/yr",6.26884983825684,7.28765129089355,7.32432656860352,7.90978598022461,9.48371813964844]
["IMAGE","FullTech","LAM","Primary Energy|Biomass","EJ/yr",4.89055590820313,5.21042362213135,11.3772456817627,21.5266165161133,19.1849195098877]
["IMAGE","FullTech","LAM","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.660027616,0.376548144,0.113119618,0.00164641633691518,9.19897008873522e-09]
["IMAGE","FullTech","LAM","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,1.14746101379395E-7,0.00134800716455078,0.0204732108125,0.033163787]
["IMAGE","FullTech","LAM","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.42347896,0.229698328,0.0568019319375,0.000664170408015845,4.24578275007662e-10]
["IMAGE","FullTech","MAF","Capacity Additions|Electricity|Solar|PV","GW/yr",0.127251721143723,0.657760328292847,1.77575690984726,11.9258666381836,33.3036106567383]
["IMAGE","FullTech","MAF","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",290.948719804874,264.673798636674,157.149656686064,0.414909790208593,9.64426319360889e-05]
["IMAGE","FullTech","MAF","Final Energy|Gases","EJ/yr",3.32601871967316,3.55591084289551,4.6555652923584,7.22824076843262,11.0329456176758]
["IMAGE","FullTech","MAF","Primary Energy|Fossil","EJ/yr",40.1390706071854,40.1697585487366,36.9911528778076,37.9192147674561,54.6378286743164]
["IMAGE","FullTech","MAF","Secondary Energy|Hydrogen|Biomass","EJ/yr",5.79189474159136e-19,5.75797742619254e-05,0.002149062890625,0.00869945584375,0.00651744421875]
["IMAGE","FullTech","MAF","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.537432229,0.403260737625,0.149255607632629,0.0123102765039063,0.00755009476354981]
["IMAGE","FullTech","MAF","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0.0004504477109375,0.506164824,1.14610885,0.48283042]
["IMAGE","FullTech","OECD90","Capacity|Electricity|Nuclear","GW",288.180215820312,287.08118901062,284.185009689331,225.706264892578,139.217929016113]
["IMAGE","FullTech","OECD90","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",3290.59553909302,2989.67470550537,1950.47534179688,1450.08568954468,1970.41876220703]
["IMAGE","FullTech","OECD90","Final Energy|Transportation","EJ/yr",49.4447383422852,46.7909459228516,37.1409276123047,34.0000346679687,38.8228626708984]
["IMAGE","FullTech","OECD90","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",11.554942622,5.516375997,1.53277895379688,0.396598918099365,0.20219242898904]
["IMAGE","FullTech","OECD90","Secondary Energy|Hydrogen|Solar","EJ/yr",0,0,0,0,0]
["IMAGE","FullTech","OECD90","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0.016778793125,0.0359755685,0.101949365,0.230307047]
["IMAGE","FullTech","OECD90","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","PAC","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,1.79019327366352,0.336963922679424,0.176585796296597]
["IMAGE","FullTech","PAC","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",24.2653045958529,15.6130630590875,10.78750346034,8.10088469491651,-13.0718579748645]
["IMAGE","FullTech","PAC","Primary Energy|Biomass","EJ/yr",0.739788635969162,1.56907503795624,4.21601153659821,8.16225163221359,7.03529896211624]
["IMAGE","FullTech","PAC","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,4.6024040625E-4,0.0067735268125,0.234781914,0.59053621]
["IMAGE","FullTech","PAC","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",2.79020663348092e-09,4.00770717978477e-07,5.25318592190743E-7,4.03283615797758E-7,1.06223062425852e-08]
["IMAGE","FullTech","PAC","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.050150955,0.0257885833125,0.006102558,0.00197653740625,1.13676398437942E-4]
["IMAGE","FullTech","PAC","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","REF","Capacity Additions|Electricity|Wind","GW/yr",1.23204096603394,0.882017753601074,0.162156113566831,3.64625025177002,8.44601711273193]
["IMAGE","FullTech","REF","Final Energy|Gases","EJ/yr",6.37216278076172,7.79426123046875,8.76243566894531,10.0173918457031,11.1330979003906]
["IMAGE","FullTech","REF","Price|Carbon","US$2010/tCO2",0,310.865538294569,1096.11721936039,1018.29677556608,483.756568816498]
["IMAGE","FullTech","REF","Secondary Energy|Electricity|Biomass","EJ/yr",0.041850384,0.0694134393125,0.419947679015625,0.711467205798828,1.12759164083032]
["IMAGE","FullTech","REF","Secondary Energy|Solids|Biomass","EJ/yr",0.00595209872722626,0.259228730201721,0.573283561706543,1.3895099029541,1.58516079711914]
["IMAGE","FullTech","REF","Water Consumption|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","REF","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","RER","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,35.3775903480832,157.222559313469,501.708628045005,588.739958108324]
["IMAGE","FullTech","RER","Final Energy|Transportation","EJ/yr",14.88151953125,13.549330078125,10.6318603515625,10.2390400390625,11.58523046875]
["IMAGE","FullTech","RER","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0.0799391326904297,0.420114196777344,2.56645288085938,1.40306494140625]
["IMAGE","FullTech","RER","Secondary Energy|Electricity|Wind","EJ/yr",0.525427142,1.396206168,1.483999232,2.242720144,6.382909088]
["IMAGE","FullTech","RER","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0.00707891,0.01270088,0.05328774,0.1244604]
["IMAGE","FullTech","RER","Water Consumption|Electricity|Solar|CSP","km3/yr",0.0011415,0.01153071,0.01129425,0.01066493,0.04437064]
["IMAGE","FullTech","Russia","Capacity|Electricity|Biomass|w/o CCS","GW",1.75260706363659,3.61138305712874,3.96476098632813,2.73075610351563,2.68451000976563]
["IMAGE","FullTech","Russia","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",559.867734710375,490.864718953768,145.77321584026,-152.298665295045,-336.614822347959]
["IMAGE","FullTech","Russia","Final Energy|Other Sector","EJ/yr",0,6.67373687028885E-5,0.011497540473938,0.02410618019104,0.0185086002349854]
["IMAGE","FullTech","Russia","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0.036517494,0.290388496,0.255612658,0.5069408]
["IMAGE","FullTech","Russia","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",5.6061668374241e-16,1.82927303314209e-08,1.99208908081055e-08,1.2969409942627e-08,-1.15317296981812E-9]
["IMAGE","FullTech","Russia","Water Consumption|Electricity|Coal","km3/yr",0.081901744,0.079412088,0.053198488,0.01476156,0.006540357]
["IMAGE","FullTech","Russia","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","US","Capacity|Electricity|Storage Reservoir","GWh",11.5605493164063,11.6309448547363,14.7490365905762,69.1354235229492,626.565986816406]
["IMAGE","FullTech","US","Final Energy|Gases","EJ/yr",17.4559786987305,15.8178620605469,15.3669891967773,15.4925432739258,14.4308054199219]
["IMAGE","FullTech","US","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,1.9496720703125e-05,1.02536861199739,4.90765707862802,2.87640595308255]
["IMAGE","FullTech","US","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0.0218908423232422,0.07254965516956,0.083513854092597,0.125392873335405]
["IMAGE","FullTech","US","Secondary Energy|Solids|Biomass","EJ/yr",0.000627384301275015,0.157716636657715,0.74689860534668,2.43585610961914,3.39684469604492]
["IMAGE","FullTech","US","Water Consumption|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","FullTech","USA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0.391746398925781,0.00361236691474915,0.0211396999359131,1.03284158325195]
["IMAGE","FullTech","USA","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,19.0722653170739,220.643262344602,613.649100240978,585.060441504645]
["IMAGE","FullTech","USA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",640.997589111328,544.629913330078,440.751708984375,355.018798828125,370.237091064453]
["IMAGE","FullTech","USA","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0.0111125802993774,0.820185180664063,4.394833984375,2.7776220703125]
["IMAGE","FullTech","USA","Secondary Energy|Electricity|Wind","EJ/yr",0.3425328,1.132037448,1.60359968,2.78400992,9.482615584]
["IMAGE","FullTech","USA","Secondary Energy|Hydrogen|Other","EJ/yr",0,5.55223868215421e-10,7.89109986153596e-09,1.10508903503418E-7,4.05208587646484E-7]
["IMAGE","FullTech","USA","Water Consumption|Electricity|Solar|CSP","km3/yr",0.0018459,0.01940769,0.02898374,0.068662064,0.1660508]
["IMAGE","FullTech","World","Capacity|Electricity|Biomass|w/o CCS","GW",151.229689453125,261.373009765625,229.90961328125,91.649443359375,11.7451849365234]
["IMAGE","FullTech","World","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,38.9652901023965,1081.60105122867,4357.38426456222,5013.5034146806]
["IMAGE","FullTech","World","Final Energy|Solids|Coal","EJ/yr",37.37176953125,35.33580078125,34.2022109375,33.63433984375,34.5363203125]
["IMAGE","FullTech","World","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",1.21665984,3.484301312,5.06578624,1.8772624,0.176200996]
["IMAGE","FullTech","World","Secondary Energy|Electricity|Coal","EJ/yr",30.859437056,32.998176384,23.362376592,6.998106176,10.6120898289063]
["IMAGE","FullTech","World","Water Consumption|Electricity|Cooling Pond","km3/yr",1.397038976,1.208979968,0.697123008,0.2669972,0.036252728]
["IMAGE","FullTech","World","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["IMAGE","Conv","AME","Capacity|Electricity|Gas|w/ CCS","GW",0,5.06062538361319,88.7903107274501,188.500546530601,262.002839987632]
["IMAGE","Conv","AME","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0.630694455169648,7.57756160210477,16.1888468142024,26.3551328801744]
["IMAGE","Conv","AME","Price|Primary Energy|Gas","US$2010/GJ",32.1938556468535,30.3365703222585,36.2215620135069,40.7121880028057,46.3908413620186]
["IMAGE","Conv","AME","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0.528944936267566,6.4881151535511,12.8399542088203,18.1999327133964]
["IMAGE","Conv","AME","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,1.45395059509277E-4,0.002623776890625,0.011772560875,0.0157314618125]
["IMAGE","Conv","AME","Water Consumption|Electricity|Nuclear","km3/yr",0.02768251,0.070183153375,0.330342620796875,1.143161467,2.33942255609375]
["IMAGE","Conv","AME","Water Withdrawal|Electricity|Coal","km3/yr",4.346817492,3.760581254375,2.054701658,0.41813101,0.7157529876875]
["IMAGE","Conv","AS","Capacity|Electricity|Oil|w/o CCS","GW",35.4252833251953,33.9222310794459,12.9649425671047,2.49337750637552,0.175042957422074]
["IMAGE","Conv","AS","Emissions|CO2|Fossil Fuels and Industry|Energy Supply|Electricity","Mt CO2/yr",1706.55671691895,1654.42327880859,616.702356338501,-281.899168491364,-313.637519836426]
["IMAGE","Conv","AS","GDP|PPP","billion US$2010/yr",9505.54783826538,16600.3924577466,27248.9108768213,40578.8698770557,56788.7646480322]
["IMAGE","Conv","AS","Primary Energy|Oil|w/o CCS","EJ/yr",23.4807882080078,22.2520692138672,20.139623046875,23.3343920898437,31.4618171386719]
["IMAGE","Conv","AS","Secondary Energy|Liquids|Biomass","EJ/yr",0.0313793808400279,0.176167472499073,1.08372258210065,1.74813535165681,2.09826667520497]
["IMAGE","Conv","AS","Water Consumption|Electricity|Gas","km3/yr",0.445632546,0.483440344,0.499691444,0.5636728,0.51243296]
["IMAGE","Conv","AS","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["IMAGE","Conv","ASIA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0.893167113645177,50.9595123967301,231.29468515981,242.956903957141]
["IMAGE","Conv","ASIA","Final Energy|Solids|Biomass","EJ/yr",24.6263975375295,27.2948285522461,25.473268447876,24.0200683746338,20.6251730422974]
["IMAGE","Conv","ASIA","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0.00046145774609375,3.43590849390518,16.7620468811024,17.7363899402837]
["IMAGE","Conv","ASIA","Secondary Energy|Electricity|Solar","EJ/yr",0.0066708,0.235758434803589,0.697001629431885,2.66543494106494,3.5048874916875]
["IMAGE","Conv","ASIA","Water Consumption|Electricity|Cooling Pond","km3/yr",0.513199392,0.68122912,0.372123712,0.1409184,0]
["IMAGE","Conv","ASIA","Water Consumption|Electricity|Hydro","km3/yr",16.471523168,23.18130352,27.4785344,39.650253376,39.437882912]
["IMAGE","Conv","Brazil","Capacity Additions|Electricity|Wind","GW/yr",0.321758605957031,0,0.454437847137451,1.50104592895508,0.48208821105957]
["IMAGE","Conv","Brazil","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0.0114136957260295,0.229504320789905,0.474200079527994]
["IMAGE","Conv","Brazil","Final Energy|Heat","EJ/yr",0,0,0,0,0]
["IMAGE","Conv","Brazil","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0.031269558429718,0.212904740333557,0.613860107291723,1.06084341067611]
["IMAGE","Conv","Brazil","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,1.570441015625e-05,0.001288879,0.006764359,0.006572747]
["IMAGE","Conv","Brazil","Water Consumption|Electricity","km3/yr",10.428630016,13.675249664,17.366730752,20.02220032,20.62717952]
["IMAGE","Conv","Brazil","Water Withdrawal|Electricity|Coal","km3/yr",0.165492608,0.071281048,0.005499969,0.009936816,0.03134826]
["IMAGE","Conv","China","Capacity|Electricity|Oil|w/o CCS","GW",89.2515047302246,88.0520437927246,68.7081809387207,44.341266702652,0.157066009406]
["IMAGE","Conv","China","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",3387.06709941228,5748.94460042318,4419.93546485901,117.226522415876,-771.988456447919]
["IMAGE","Conv","China","GDP|PPP","billion US$2010/yr",12769.8276729687,28174.5685483203,46203.4589414844,59954.0346085156,70070.8379628125]
["IMAGE","Conv","China","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,5.54318233690581,7.58130784794839]
["IMAGE","Conv","China","Secondary Energy|Liquids|Biomass","EJ/yr",0.00893518260121346,0.435105966329575,3.23902127075195,6.84796415710449,7.43728612852097]
["IMAGE","Conv","China","Water Consumption|Electricity|Gas","km3/yr",0.149777904,0.600099008,0.505610688,0.126432,0.2526908]
["IMAGE","Conv","CN","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",17.296529296875,0,0,0.000308167994022369,0.00339243793487549]
["IMAGE","Conv","CN","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,35.8460365484158,66.3543492555618]
["IMAGE","Conv","CN","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",4716.50338745117,4420.0926361084,3361.81791687012,2370.34481811523,2470.25205993652]
["IMAGE","Conv","CN","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,9.754935952,11.197216504]
["IMAGE","Conv","CN","Secondary Energy|Electricity|Solar","EJ/yr",0.0025992,0.1637092545,0.199609556296875,1.559360064,1.859512864]
["IMAGE","Conv","CN","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",9.42336129128307e-17,0,0,0,0]
["IMAGE","Conv","CN","Water Consumption|Electricity|Once Through","km3/yr",0.598994304,0.800635072,0.456774592,0.189735296,0.0515109]
["IMAGE","Conv","EIT","Capacity Additions|Electricity|Wind","GW/yr",1.23204096603394,0.67446181678772,0.224120441753417,1.81888401794434,2.97022430038452]
["IMAGE","Conv","EIT","Capacity|Electricity|Storage Reservoir|Daily","GWh",5.00793794250488,4.91291607666016,4.52350765991211,4.69750939941406,5.47680255126953]
["IMAGE","Conv","EIT","Final Energy|Heat","EJ/yr",7.3353839263916,5.91171839904785,4.77006643676758,4.10421250915527,3.7709539642334]
["IMAGE","Conv","EIT","Price|Primary Energy|Coal","US$2010/GJ",7.75776021818161,8.70587824001551,9.60853097713947,9.50494208098412,9.19547822641373]
["IMAGE","Conv","EIT","Resource|Cumulative Extraction|Gas","EJ",154.423001984,443.591144448,754.611019776,1197.209419776,1845.791543296]
["IMAGE","Conv","EIT","Water Consumption|Electricity","km3/yr",3.92095424,3.20608544,3.25706864,3.721746464,4.189473088]
["IMAGE","Conv","EIT","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,0,6.77224487304688e-07,1.3999591796875E-4,0.0021513241875]
["IMAGE","Conv","EIT","Water Withdrawal|Electricity|Oil|w/ CCS","km3/yr",0,0.000857079921875,0.0047553038125,0.00864961128515625,0.00458213748828125]
["IMAGE","Conv","EU","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",1129.29860502481,649.759439130624,314.700360720356,-209.283555547396,-261.877390362012]
["IMAGE","Conv","EU","GDP|PPP","billion US$2010/yr",16109.5081322534,19107.6060365869,22524.8773815186,26400.9534857031,30615.2567419629]
["IMAGE","Conv","EU","Primary Energy|Coal","EJ/yr",11.6224970703125,7.69418896484375,4.74397888183594,5.5896259765625,8.33220690917969]
["IMAGE","Conv","EU","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",0.514370288,0.85490224,0.572785872,0.451300216,0.573802688]
["IMAGE","Conv","EU","Water Consumption|Electricity|Gas","km3/yr",0.369690254,0.207710002,0.16701787,0.174696496,0.357105576]
["IMAGE","Conv","EU","Water Consumption|Electricity|Wet Tower","km3/yr",3.424156096,2.42578944,1.970984336,1.88119592,2.146169952]
["IMAGE","Conv","IN","Capacity|Electricity|Coal|w/o CCS","GW",48.7822109375,60.4423007835749,38.2606992210749,2.32484694606683E-9,1.94760595932394]
["IMAGE","Conv","IN","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",755.053760528564,910.532897949219,953.06521987915,1063.4054107666,1278.48025131226]
["IMAGE","Conv","IN","Population","million",1214.48999023438,1376.61401367188,1515.9580078125,1632.27795410156,1719.46203613281]
["IMAGE","Conv","IN","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.102812599182129,0.689516784667969,2.41254907226562,2.122212890625]
["IMAGE","Conv","IN","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,3.20593896321952e-12,3.08158807456493e-12,1.24069102108479E-10,1.0952160358429E-9]
["IMAGE","Conv","IN","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0.003404744,0.08416316,0.320686912,0.625925184]
["IMAGE","Conv","IN","Water Withdrawal|Electricity|Fossil","km3/yr",51.433938944,33.058359296,12.2632704,5.322383872,1.337148032]
["IMAGE","Conv","India","Capacity|Electricity|Storage Reservoir|Daily","GWh",2.21644311523437,4.3039599609375,8.8071767578125,15.7324296875,24.719939453125]
["IMAGE","Conv","India","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",853.895887732506,699.928522109985,297.705618043741,0,10.4999986942858]
["IMAGE","Conv","India","Price|Primary Energy|Coal","US$2010/GJ",1.49297316661835,1.72581570384026,1.95167171836615,1.93792580395937,1.90002886701584]
["IMAGE","Conv","India","Secondary Energy|Electricity|Hydro","EJ/yr",0.443052,0.680807168,1.188883968,1.723053952,1.659235968]
["IMAGE","Conv","India","Water Consumption|Electricity","km3/yr",4.184957952,5.20647424,7.509693952,11.230359552,13.628309504]
["IMAGE","Conv","India","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,0.00156538,0.002902856,0.003841357,0.01379087]
["IMAGE","Conv","Japan","Capacity Additions|Electricity|Hydro","GW/yr",1.05178894042969,0,0.558789123535156,0.558789123535156,0.55094921875]
["IMAGE","Conv","Japan","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",460.910260677338,332.570028801759,193.735445539157,21.7378473219772,64.7120115657647]
["IMAGE","Conv","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",472.129285991192,344.896508425474,205.344290450215,45.7957432903349,92.5164045412093]
["IMAGE","Conv","Japan","Primary Energy|Coal","EJ/yr",4.15806201171875,2.99514697265625,2.60610302734375,2.31444506835938,2.50940502929688]
["IMAGE","Conv","Japan","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",0.0142651,0.0282243,0.04186686,0.171236896,0.170778592]
["IMAGE","Conv","Japan","Secondary Energy|Liquids","EJ/yr",5.797411703825,4.98901506400108,4.38953226514161,4.37930193523783,4.27640145335904]
["IMAGE","Conv","Japan","Water Consumption|Electricity|Wet Tower","km3/yr",0.078638256,0.053606552,0.02650765,0.01324253,0.01397768]
["IMAGE","Conv","LA","Capacity|Electricity|Coal|w/o CCS","GW",0.627657012939453,0.555263610839844,0.110939689140022,2.27991559159958e-05,0.194313390726698]
["IMAGE","Conv","LA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0.000538372565491348,0.0893080738630185,1.11128012698221,2.30469455952213]
["IMAGE","Conv","LA","Final Energy|Residential and Commercial","EJ/yr",5.07567280578613,5.89519496154785,6.20225079345703,7.25085531616211,8.58755828857422]
["IMAGE","Conv","LA","Secondary Energy|Electricity|Biomass","EJ/yr",0.0323424,0.13292149788623,0.324908092621217,0.488152711517678,0.407604479930557]
["IMAGE","Conv","LA","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,2.5262929906603e-11,1.58440444432199e-09,1.15533508360386E-8,1.49846791062737e-08]
["IMAGE","Conv","LA","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,1.74727099609375E-6,0.00262380025488281,0.030191362,0.081802206]
["IMAGE","Conv","LA","Water Withdrawal|Electricity|Sea Cooling","km3/yr",0,0,0,0,0]
["IMAGE","Conv","LAM","Capacity|Electricity|Storage Reservoir|Daily","GWh",1.35458721923828,1.87084878540039,2.34258930969238,3.54959362792969,4.7886171875]
["IMAGE","Conv","LAM","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",74.9044591017688,32.4676156548473,7.77773323716246,0.0059843097144352,1.57641954046994]
["IMAGE","Conv","LAM","Primary Energy|Coal|w/o CCS","EJ/yr",1.36718799209595,1.09411161804199,0.763619983673096,0.528814422607422,0.547044387817383]
["IMAGE","Conv","LAM","Secondary Energy|Electricity|Hydro","EJ/yr",2.625364416,3.417514488,4.344313384,5.057883744,5.250372688]
["IMAGE","Conv","LAM","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,2.43502988843843e-05,0.0036262488375664,0.017448027,0.018196611]
["IMAGE","Conv","LAM","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,6.8205869140625e-06,0.000992092716796875,0.010762495,0.033590645]
["IMAGE","Conv","LAM","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.34383528,1.265223534,0.863191846,0.03535737621875,0.000330234038514376]
["IMAGE","Conv","MAF","Capacity|Electricity|Oil|w/ CCS","GW",0,0.00122803577393101,0.00285693037666328,0.00398172713605999,0.00221459199277996]
["IMAGE","Conv","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",1348.06873678882,1211.18029785575,507.11140298238,161.192755251424,327.906771003269]
["IMAGE","Conv","MAF","GDP|MER","billion US$2010/yr",2819.83213498125,4610.40063904531,7572.19237245125,11917.64405254,18470.0912058]
["IMAGE","Conv","MAF","Primary Energy|Oil|w/ CCS","EJ/yr",0,0.161238198637962,0.565391126871109,0.607146755664784,0.204064946062397]
["IMAGE","Conv","MAF","Secondary Energy|Liquids","EJ/yr",13.7695181767396,16.1053001519957,18.6707682780768,22.4558741256221,26.7225056231836]
["IMAGE","Conv","MAF","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",1.832852846,1.373793858,0.506758215,0.039664019,0.070558799]
["IMAGE","Conv","MAF","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0,0.00124547868359375,0.00383902504902649,0.01211078421875,0.035429863]
["IMAGE","Conv","OECD90","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,17.7860419197486,83.0149430451759,629.862871050136,1629.57255744065]
["IMAGE","Conv","OECD90","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",194.412838337788,176.831683895822,125.211339423009,54.7596076942517,17.3648556217845]
["IMAGE","Conv","OECD90","Primary Energy|Biomass","EJ/yr",6.29469571685791,7.99879503440857,18.8535007791519,30.1380657405853,27.3385658073425]
["IMAGE","Conv","OECD90","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.828502070398438,0.579779746125,0.32760055363678,0.17506530540625,0.0389420708632813]
["IMAGE","Conv","OECD90","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0.0170275300854492,0.060419486296875,0.312953399,0.709590213]
["IMAGE","Conv","OECD90","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.207817641,0.0529099743125,0.01555961659375,0.00349382501757813,0.000615445923461914]
["IMAGE","Conv","PAC","Capacity Additions|Electricity|Solar|PV","GW/yr",1.43120644378662,0.127797996520996,0.316350940704346,4.00480764007568,0.65459659576416]
["IMAGE","Conv","PAC","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",691.379105051358,424.90836357077,247.148000324766,2.78734208510182,6.9149190094322]
["IMAGE","Conv","PAC","Final Energy|Gases","EJ/yr",2.90815228271484,3.08456451416016,3.3103193359375,4.27814697265625,4.74894702148437]
["IMAGE","Conv","PAC","Primary Energy|Fossil","EJ/yr",32.8494211425781,27.0897457275391,20.3227976074219,17.820686706543,19.1306329956055]
["IMAGE","Conv","PAC","Secondary Energy|Hydrogen|Biomass","EJ/yr",4.54767100052393e-11,3.41402441857781e-05,0.0176587443125,0.047761086296925,0.0359366046689003]
["IMAGE","Conv","PAC","Secondary Energy|Solids|Coal","EJ/yr",2.53463957214355,2.46873983764648,2.6290848236084,2.76371598815918,2.6018550567627]
["IMAGE","Conv","PAC","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.102617346,0.808299144,0.349846975,0.00475778019372559,0.00368955127141422]
["IMAGE","Conv","REF","Capacity|Electricity|Oil|w/ CCS","GW",0,0.0151004867553711,0.102804310798645,0.323465362429619,0.670116568446159]
["IMAGE","Conv","REF","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,1.80695156401508,203.151463914981,424.876358474884,490.017770952963]
["IMAGE","Conv","REF","GDP|MER","billion US$2010/yr",2551.44678480609,3754.79694060031,5328.9102446975,6962.20177163625,8328.2716552325]
["IMAGE","Conv","REF","Secondary Energy|Electricity|Fossil","EJ/yr",4.292111338,3.74092252533789,2.65095383217454,2.3355239402871,3.33695633643262]
["IMAGE","Conv","REF","Secondary Energy|Electricity|Wind|Offshore","EJ/yr",0,0.0004228388125,1.23566297839355E-3,0.010648586,0.046352964]
["IMAGE","Conv","REF","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,7.611975E-3,0.036932783,0.09641832,0.297653896]
["IMAGE","Conv","REF","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["IMAGE","Conv","RER","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,7.41253343100349,21.3919896632433,134.605346868436,354.442358016968]
["IMAGE","Conv","RER","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",134.617708623409,132.356654852629,100.705767671267,38.3935927723845,8.61615346123775]
["IMAGE","Conv","RER","Primary Energy|Gas|Electricity","EJ/yr",4.614598464,3.018850769,2.687228366,2.838155856,5.429322252]
["IMAGE","Conv","RER","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.269532096,0.186403476,0.188555295,0.132658496,0.02090601]
["IMAGE","Conv","RER","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",9.96128463745117e-08,5.3334677734375e-06,7.090044921875E-6,3.69052587890625E-6,-2.04228000640869e-08]
["IMAGE","Conv","RER","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.1033202,0.02232763,0.009116692,0.002902861,0.00040003390625]
["IMAGE","Conv","Russia","Capacity Additions|Electricity|Solar|PV","GW/yr",0.000200000002980232,2.81457710266113E-3,0.000505145013332367,0,0.284670013427734]
["IMAGE","Conv","Russia","Capacity|Electricity|Storage Reservoir","GWh",2.76803198242188,2.67946508789062,2.3170810546875,2.3760859375,2.27492602539062]
["IMAGE","Conv","Russia","Final Energy|Gases","EJ/yr",2.0062509765625,2.88490600585938,3.58123291015625,5.37652001953125,6.2813330078125]
["IMAGE","Conv","Russia","Primary Energy|Wind","EJ/yr",4.32E-5,0.005189197,0.01800427,0.01678762,0.165721552]
["IMAGE","Conv","Russia","Secondary Energy|Hydrogen|Biomass","EJ/yr",2.0068110018201e-16,2.23667593415082E-6,0.00488967741644961,0.01281945,0.01270401]
["IMAGE","Conv","Russia","Secondary Energy|Solids|Coal","EJ/yr",0.960409423828125,0.909445190429688,1.0950009765625,1.08330798339844,0.793474304199219]
["IMAGE","Conv","Russia","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","Conv","US","Capacity|Electricity|Oil|w/ CCS","GW",0,0.0127770795822144,0.0221895265580292,0.0228643156353701,0.936633528358148]
["IMAGE","Conv","US","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,3.74039681902432,105.973056765722,382.781126435859,396.688086022538]
["IMAGE","Conv","US","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0.0392406373023987,1.13969237518311,4.13279026031494,4.28927532196045]
["IMAGE","Conv","US","Primary Energy|Oil|w/o CCS","EJ/yr",43.0765710449219,36.5312280273438,21.7588486328125,16.1740410766602,20.7681990966797]
["IMAGE","Conv","US","Secondary Energy|Electricity|Wind","EJ/yr",0.3783996,1.170194318,1.277379207,1.140296398,1.137898284]
["IMAGE","Conv","US","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0.049429725703125,0.158216496203125,0.381523248,0.659989776]
["IMAGE","Conv","US","Water Consumption|Electricity|Solar|CSP","km3/yr",0.0018459,0.01460659,0.01950578009375,0.076455891,0.135259007]
["IMAGE","Conv","USA","Capacity|Electricity|Biomass|w/o CCS","GW",33.577580078125,44.9140498046875,38.4144990234375,15.9782055664063,9.15389987182617]
["IMAGE","Conv","USA","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",49.7798038025697,39.0702042107781,21.264016473045,13.9020714753618,5.93994491888831]
["IMAGE","Conv","USA","Final Energy|Other Sector","EJ/yr",0,1.33590197563171E-3,0.0746644515991211,0.150861801147461,0.147500503540039]
["IMAGE","Conv","USA","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0.269479808,1.045025024,1.799917056,2.293408208]
["IMAGE","Conv","USA","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0,1.63925603032112E-10,0,0,0]
["IMAGE","Conv","USA","Water Consumption|Electricity|Coal","km3/yr",3.518404096,1.498464,0.187732992,0.1929352,0.430750016]
["IMAGE","Conv","USA","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["IMAGE","Conv","World","Capacity|Electricity|Storage Reservoir","GWh",49.425078125,68.65890625,87.8253125,170.9255,227.65009375]
["IMAGE","Conv","World","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",12582.4086666107,13279.8964182536,8019.14699872335,306.92603935798,-829.999153812726]
["IMAGE","Conv","World","Price|Primary Energy|Oil","US$2010/GJ",12.0171507540321,12.4020691065407,13.5173075983238,14.5028426768684,14.4835566151619]
["IMAGE","Conv","World","Secondary Energy|Electricity|Nuclear","EJ/yr",9.9226368,9.48113408,12.656719872,29.19425024,45.226098688]
["IMAGE","Conv","World","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0.0006044258125,0.720177216,2.658366976,2.721560064]
["IMAGE","Conv","World","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","AME","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["IMAGE","NewRE","AME","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","AME","Price|Primary Energy|Gas","US$2010/GJ",32.1938556468535,30.25764045614,36.0003757856274,39.693235881896,41.8360030662346]
["IMAGE","NewRE","AME","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","AME","Secondary Energy|Gases","EJ/yr",3.32601873493195,3.04316794204712,4.3618450012207,6.66937118530273,9.37417004394531]
["IMAGE","NewRE","AME","Secondary Energy|Liquids|Biomass","EJ/yr",0.0119700884283441,0.141068005769659,0.739644049644767,0.964174971865788,1.67647663676459]
["IMAGE","NewRE","AME","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","AS","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["IMAGE","NewRE","AS","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","AS","Final Energy|Solids|Biomass","EJ/yr",13.7424785155058,16.1198041992187,19.8459133834839,21.9658139343262,23.3440615081787]
["IMAGE","NewRE","AS","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.077374790375,0.529566942,0.914740604286067,0.3490651621875,0.35980715834375]
["IMAGE","NewRE","AS","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","AS","Water Consumption|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","AS","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0.0127686682063599,0.914282853,2.571031356,4.084446816]
["IMAGE","NewRE","ASIA","Capacity|Electricity|Wind|Offshore","GW",0.1505,2.05512625980377,65.7945622558594,317.26207421875,1059.06051660156]
["IMAGE","NewRE","ASIA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",358.494244205455,1059.56813755135,1011.28740826001,803.593780146912,102.48984893163]
["IMAGE","NewRE","ASIA","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","ASIA","Secondary Energy|Electricity|Nuclear","EJ/yr",1.057647584,1.179514026,1.169840434,0.85264022,0.304299329]
["IMAGE","NewRE","ASIA","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",1.70874805860421e-16,1.10895145466805E-4,0.00707035206500244,0.0723492835859375,0.182557071]
["IMAGE","NewRE","ASIA","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","Brazil","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["IMAGE","NewRE","Brazil","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["IMAGE","NewRE","Brazil","Emissions|CO2|Fossil Fuels and Industry|Energy Supply|Electricity","Mt CO2/yr",43.1009483337402,22.1628093719482,6.40752601623535,13.8836898803711,9.79531097412109]
["IMAGE","NewRE","Brazil","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","Brazil","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","Brazil","Secondary Energy|Liquids|Biomass","EJ/yr",0.462435001553968,0.293944615960121,0.650205652236938,0.472839469909668,0.39491649055481]
["IMAGE","NewRE","Brazil","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","Brazil","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","China","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",4716.48611450195,3938.91343688965,3040.66724395752,1882.79674911499,1462.39730453491]
["IMAGE","NewRE","China","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","China","Secondary Energy|Electricity|Solar","EJ/yr",0.0025992,0.163382806296875,0.1996108535,15.626323968,26.101122304]
["IMAGE","NewRE","China","Water Consumption|Electricity|Cooling Pond","km3/yr",0.513199488,0.600785728,0.322702112,0.02506615,0]
["IMAGE","NewRE","China","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","CN","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0.149,0,0,3.6816298828125,9.8275693359375]
["IMAGE","NewRE","CN","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",66.7628472050031,539.535721143087,599.596093098323,695.231546958287,7.30568279201786]
["IMAGE","NewRE","CN","Final Energy|Hydrogen","EJ/yr",2.89854096990894E-9,0.0175836296081543,0.0563637008666992,0.145856506347656,0.311927612304688]
["IMAGE","NewRE","CN","Resource|Cumulative Extraction|Gas","EJ",22.584690688,118.589300736,269.819297792,406.17541632,438.73501184]
["IMAGE","NewRE","CN","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",9.42336129128307e-17,9.457021875e-05,4.56874E-3,0.056223512,0.128530096]
["IMAGE","NewRE","CN","Water Consumption|Electricity|Cooling Pond","km3/yr",0.513199488,0.600785728,0.322702112,0.02506615,0]
["IMAGE","NewRE","CN","Water Withdrawal|Electricity|Coal","km3/yr",95.76005632,95.485861888,44.223410176,0.1420756,0.003741958]
["IMAGE","NewRE","EIT","Capacity|Electricity|Oil|w/o CCS","GW",63.430680015564,26.5699170837402,10.2257729721069,7.35520147705078,4.4152527923584]
["IMAGE","NewRE","EIT","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",763.163379083077,475.708981975913,317.036775522865,198.549746380498,140.957572109376]
["IMAGE","NewRE","EIT","GDP|PPP","billion US$2010/yr",5299.40483417603,7531.41506809937,10238.0756653625,12865.3655151929,14983.9415234058]
["IMAGE","NewRE","EIT","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","EIT","Secondary Energy|Liquids|Biomass","EJ/yr",0.039616566078605,0.204833162807627,1.10566570824385,0.961826763570309,1.24098851966858]
["IMAGE","NewRE","EIT","Water Consumption|Electricity|Gas","km3/yr",0.36076049,0.20742832,0.121954632,0.089529043,0.095615885]
["IMAGE","NewRE","EU","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",1.10560709762573,0,2.53906365846097,2.03419598388672,4.82768637084961]
["IMAGE","NewRE","EU","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","EU","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",2687.75124740601,2088.1822013855,1450.79590988159,1280.19358444214,1115.50146961212]
["IMAGE","NewRE","EU","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","EU","Secondary Energy|Electricity|Solar","EJ/yr",0.0840672,0.62112464,0.689473358,1.339113244,6.249838792]
["IMAGE","NewRE","EU","Secondary Energy|Hydrogen|Gas","EJ/yr",1.27270279449527e-07,0.0050090344375,0.084010176,0.306348138,0.333439658]
["IMAGE","NewRE","EU","Water Consumption|Electricity|Other","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","IN","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0,0.634342407226563,0.720568725585938,1.71925305175781,0]
["IMAGE","NewRE","IN","Capacity|Electricity|Wind","GW",13.065,25.4578482055664,71.172419921875,266.434375,243.9630546875]
["IMAGE","NewRE","IN","Final Energy|Hydrogen","EJ/yr",1.00160102434188E-11,0.00235203194618225,0.010658519744873,0.0310334491729736,0.089942756652832]
["IMAGE","NewRE","IN","Resource|Cumulative Extraction|Gas","EJ",6.657757184,27.448969216,60.458041344,78.767742976,91.677892608]
["IMAGE","NewRE","IN","Secondary Energy|Electricity|Wind","EJ/yr",0.0707652,0.208906734,0.634955712,2.155540224,1.920685664]
["IMAGE","NewRE","IN","Water Consumption|Electricity","km3/yr",4.184957952,4.968327168,6.861824,9.055609856,10.366449664]
["IMAGE","NewRE","IN","Water Withdrawal|Electricity|Oil","km3/yr",1.491596032,1.415856,0.117137504,0,0]
["IMAGE","NewRE","India","Capacity|Electricity|Oil|w/o CCS","GW",5.53361181640625,5.54150586096592,1.28891102061317,9.90793887467589e-09,9.90793887467589e-09]
["IMAGE","NewRE","India","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",934.566924969355,825.087616840998,334.102476636569,21.9318807745973,45.3415615484118]
["IMAGE","NewRE","India","Primary Energy|Biomass|w/o CCS","EJ/yr",7.377337890625,9.440728515625,9.958025390625,9.8127412109375,10.082080078125]
["IMAGE","NewRE","India","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","India","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",0.0707652,0.197346704,0.468356416,1.596685056,1.445870976]
["IMAGE","NewRE","India","Water Consumption|Electricity|Gas","km3/yr",0.111881296,0.147448608,0.103727504,0.02012551,0.04676946]
["IMAGE","NewRE","Japan","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0,0,0.00031235259771347,0.0594158782958984,0.0628976707458496]
["IMAGE","NewRE","Japan","Capacity|Electricity|Coal|w/o CCS","GW",21.735869140625,20.822419921875,10.28991015625,0,0]
["IMAGE","NewRE","Japan","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",683.18790435791,530.396766662598,369.433605194092,279.314925670624,225.31939458847]
["IMAGE","NewRE","Japan","Primary Energy|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","Japan","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","Japan","Secondary Energy|Hydrogen|Gas","EJ/yr",4.51343270787038e-09,0.00100367666992188,0.013011784,0.043541533,0.049258536]
["IMAGE","NewRE","Japan","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.047449648,0.02291008,0.009458717,0,0]
["IMAGE","NewRE","Japan","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","LA","Capacity|Electricity|Wind","GW",1.5099700012207,9.55124406242371,43.3133099899292,142.600895080566,284.915423828125]
["IMAGE","NewRE","LA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["IMAGE","NewRE","LA","Price|Primary Energy|Coal","US$2010/GJ",5.48709042598009,6.30751712458849,6.89201045583487,6.79569688206434,6.54920918679714]
["IMAGE","NewRE","LA","Secondary Energy|Electricity|Hydro","EJ/yr",2.491728816,3.05767548,4.205713888,4.696783404,3.89996928]
["IMAGE","NewRE","LA","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,7.48106304931641e-06,9.7992119140625e-05,0.0007627683515625,0.006686978]
["IMAGE","NewRE","LA","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0,1.91012231933594E-4,0.019662947,0.242060472,0.847709808]
["IMAGE","NewRE","LAM","Capacity Additions|Electricity|Hydro","GW/yr",3.80256243896484,5.84707159423828,4.2405052986145,3.66671884918213,2.67662525177002]
["IMAGE","NewRE","LAM","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",347.671903359393,260.302661142002,126.816764667941,34.426326979883,16.9359901919961]
["IMAGE","NewRE","LAM","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",647.835572600365,473.627324953675,287.915500681847,173.349065493792,138.359455468133]
["IMAGE","NewRE","LAM","Primary Energy|Oil","EJ/yr",14.4599331054687,13.4358192138672,10.0395621337891,8.94996606445313,7.46409692382812]
["IMAGE","NewRE","LAM","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",0.0168552,0.10068422,0.564661038,1.9863648,3.590874112]
["IMAGE","NewRE","LAM","Secondary Energy|Liquids","EJ/yr",10.6537272545202,11.2222223071158,10.794987364769,10.4900656394958,10.3601843862534]
["IMAGE","NewRE","LAM","Water Consumption|Electricity|Wet Tower","km3/yr",0.935985536,0.665644972,0.31360654,0.500853464,1.209471968]
["IMAGE","NewRE","MAF","Capacity|Electricity|Coal|w/o CCS","GW",36.0185545876026,29.2808353332012,15.5033626547396,0.000157049301671744,3.37185773044979e-07]
["IMAGE","NewRE","MAF","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","MAF","Final Energy|Solids","EJ/yr",10.5793563279137,12.3256949520111,14.844987487793,16.3355073471069,17.8205228881836]
["IMAGE","NewRE","MAF","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","MAF","Secondary Energy|Electricity|Other","EJ/yr",0.0107856,0.0262827608125,0.1011067055,0.227520837,0.334240651]
["IMAGE","NewRE","MAF","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.638324,0.469785454929688,0.168073260824219,1.86285607147217E-6,9.48147425428033e-10]
["IMAGE","NewRE","MAF","Water Withdrawal|Electricity|Solar","km3/yr",0,0.001399873296875,0.24129583,1.108526969,2.281658768]
["IMAGE","NewRE","OECD90","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",0.137431564331055,0,0.000273979306221008,0,0.00171330499649048]
["IMAGE","NewRE","OECD90","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",2990.64489081502,1126.62960138793,211.289646381071,16.0149535837035,3.17436852342704]
["IMAGE","NewRE","OECD90","Primary Energy|Coal|w/o CCS","EJ/yr",36.4121270141602,15.8207042694092,4.77060014343262,1.23555018568039,0.404698470871896]
["IMAGE","NewRE","OECD90","Secondary Energy|Electricity|Hydro","EJ/yr",4.584535568,4.67293744,4.994929888,5.468996912,3.818663256]
["IMAGE","NewRE","OECD90","Secondary Energy|Hydrogen|Biomass","EJ/yr",2.35415327602709e-10,2.01608160888672E-4,0.0124894004746094,0.051756446625,0.105953197]
["IMAGE","NewRE","OECD90","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",0.0029934,0.0297786955,0.10219341609375,1.316058023,5.05983379859375]
["IMAGE","NewRE","PAC","Capacity Additions|Electricity|Hydro","GW/yr",1.20462484741211,0,3.00070462799072,0.851723670959473,1.05955172729492]
["IMAGE","NewRE","PAC","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["IMAGE","NewRE","PAC","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",1068.63863589441,672.76942310553,402.523596117664,116.167555871285,52.3037507530789]
["IMAGE","NewRE","PAC","Primary Energy|Oil","EJ/yr",16.3624943847656,11.4651907958984,7.35493646240234,5.23381854248047,4.13243048095703]
["IMAGE","NewRE","PAC","Secondary Energy|Electricity|Fossil","EJ/yr",4.574774604,3.231595738,2.17703062054199,0.51109482,0.1407863095]
["IMAGE","NewRE","PAC","Secondary Energy|Liquids","EJ/yr",10.9464635213355,8.84420156512782,7.85876605467558,7.60681423601889,6.65061512446776]
["IMAGE","NewRE","PAC","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",2.001614392,1.811885184,0.966576336,0.07613744,0.01150129559375]
["IMAGE","NewRE","REF","Capacity|Electricity|Coal|w/o CCS","GW",128.611812042236,103.588931650162,73.5088046875,44.460648223877,11.2921506195068]
["IMAGE","NewRE","REF","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","REF","Primary Energy|Biomass","EJ/yr",1.8948905620575,5.01687087249756,9.0571450958252,10.1508356170654,13.3592787132263]
["IMAGE","NewRE","REF","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","REF","Secondary Energy|Electricity|Other","EJ/yr",1.818E-3,1.279365E-3,0.058018158,0.12411316,0.125783892]
["IMAGE","NewRE","REF","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.069174569,0.024186826,0.0057754901875,0.00998907871875,0.0048110428125]
["IMAGE","NewRE","REF","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","RER","Capacity Additions|Electricity|Solar|PV","GW/yr",11.4453798828125,0,0.697514282226563,7.2776181640625,12.9578798828125]
["IMAGE","NewRE","RER","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",538.638845086098,150.637846440077,41.2469931567709,11.2349673484762,1.00453388101111]
["IMAGE","NewRE","RER","Final Energy|Gases","EJ/yr",10.98258984375,9.9873037109375,9.935494140625,9.3592666015625,7.9320859375]
["IMAGE","NewRE","RER","Primary Energy|Wind","EJ/yr",0.525427238,1.3829658,1.344880368,4.180075328,6.650312192]
["IMAGE","NewRE","RER","Secondary Energy|Hydrogen|Biomass","EJ/yr",1.89938694238663e-10,1.4437109375E-4,0.0105066,0.02454736,0.02129952]
["IMAGE","NewRE","RER","Secondary Energy|Solids|Coal","EJ/yr",1.37907202148438,1.0285,1.44656396484375,1.40863403320313,1.44236804199219]
["IMAGE","NewRE","RER","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",1.706925952,0.69571872,1.426141952,0.265811904,0.162763104]
["IMAGE","NewRE","Russia","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["IMAGE","NewRE","Russia","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","Russia","GDP|MER","billion US$2010/yr",1057.60555691125,1620.77981134,2312.39838808,2989.80909158,3480.05715242]
["IMAGE","NewRE","Russia","Secondary Energy|Electricity|Fossil","EJ/yr",2.447244184,1.92882702640625,1.52535217920313,0.979221062,0.915854917]
["IMAGE","NewRE","Russia","Secondary Energy|Electricity|Wind|Offshore","EJ/yr",0,0,1.252551E-3,0.007576219,0.1872636]
["IMAGE","NewRE","Russia","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",0.322959616,0.2308936,0.1451588,0.06953832,0.0731244]
["IMAGE","NewRE","US","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["IMAGE","NewRE","US","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["IMAGE","NewRE","US","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",6538.65752339363,4846.5387852788,3122.34675002098,2052.63270629942,1411.65710789338]
["IMAGE","NewRE","US","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["IMAGE","NewRE","US","Secondary Energy|Electricity|Other","EJ/yr",0.0872028,0.0978935590703125,0.219583086830078,0.2160251471875,0.160324488]
["IMAGE","NewRE","US","Water Consumption|Electricity|Cooling Pond","km3/yr",0.883839872,0.520425312,0.316653504,0.087379936,0.001624079]
["IMAGE","NewRE","US","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.191638404,0.066351644,0.0231985819140625,3.86159584960938E-3,0.00036530849609375]
["IMAGE","NewRE","USA","Capacity Additions|Electricity|Solar|PV","GW/yr",1.29406896972656,6.873205078125,21.82825,16.343580078125,4.06121899414063]
["IMAGE","NewRE","USA","Capacity|Electricity|Storage Reservoir","GWh",10.026650390625,10.3309599609375,22.657279296875,1071.298,3178.597]
["IMAGE","NewRE","USA","Final Energy|Gases","EJ/yr",14.493009765625,11.558669921875,10.8031396484375,10.9785595703125,9.1061259765625]
["IMAGE","NewRE","USA","Primary Energy|Wind","EJ/yr",0.3425328,0.942822922,1.786100704,6.221599264,8.254888256]
["IMAGE","NewRE","USA","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",3.641870654,6.3642258,6.625951976,1.925841496,0.133239676]
["IMAGE","NewRE","USA","Secondary Energy|Solids|Coal","EJ/yr",0.833919372558594,0.708565612792969,0.624476501464844,1.12809997558594,1.17007202148437]
["IMAGE","NewRE","USA","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["IMAGE","NewRE","World","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["IMAGE","NewRE","World","Consumption","billion US$2010/yr",44800.3296989441,68886.0092922974,99824.224372406,131822.276999512,165875.089628601]
["IMAGE","NewRE","World","Primary Energy|Coal|Electricity","EJ/yr",86.592979968,70.337354496,37.102899968,1.461751584,0.314302676]
["IMAGE","NewRE","World","Secondary Energy|Electricity|Gas","EJ/yr",16.927059384,23.266928384,22.97309824,11.20514176,3.205412992]
["IMAGE","NewRE","World","Secondary Energy|Gases|Natural Gas","EJ/yr",47.76898828125,48.14369140625,59.122921875,71.45115625,74.111046875]
["IMAGE","NewRE","World","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["POLES","Base","ASIA","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",144.308915039062,107.128525390625,140.451454101562,101.931548828125,113.832712890625]
["POLES","Base","ASIA","Capacity|Electricity|Gas|w/o CCS","GW",439.34015545,813.636249111111,1472.13068661111,2409.35140536111,3326.04349911111]
["POLES","Base","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",1606.790046875,1935.666890625,2315.238625,2632.19340625,2744.98153125]
["POLES","Base","ASIA","Primary Energy|Fossil|w/ CCS","EJ/yr",4.95478391498342e-06,1.23984918753684E-4,1.03796480177717E-4,5.90474005682627e-08,1.25042152867536E-7]
["POLES","Base","ASIA","Primary Energy|Secondary Energy Trade","EJ/yr",-0.00376885787750244,-0.0447175446023254,-0.732864142923706,-2.1291358265321,-3.54068478149304]
["POLES","Base","ASIA","Secondary Energy|Gases","EJ/yr",18.7335597151406,27.6929918174531,42.972497465625,49.9271664953672,45.0958944157031]
["POLES","Base","ASIA","Water Consumption|Electricity|Sea Cooling","km3/yr",17.9995682239532,40.0249648094177,70.254777431488,97.6111214160919,120.451618015766]
["POLES","Base","ASIA","Water Withdrawal|Electricity|Wet Tower","km3/yr",15.9746944904327,30.4355759620667,45.2111592292786,55.235613822937,62.5336661338806]
["POLES","Base","Brazil","Capacity|Electricity|Biomass|w/ CCS","GW",9.99999974737875e-08,1.17647054139525e-07,1.17647054139525e-07,1.17647054139525e-07,1.17647054139525e-07]
["POLES","Base","Brazil","Final Energy|Industry","EJ/yr",4.189849822125,5.2666457180625,6.1125664156875,6.638412141,6.9657891541875]
["POLES","Base","Brazil","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",8.28726552909107e-08,1.11067139766046e-05,6.33833790213934e-06,3.922881859996e-09,1.03508666986142E-8]
["POLES","Base","Brazil","Primary Energy|Oil","EJ/yr",4.378157694,5.9737085769375,6.3365386275,6.0175718488125,5.4912557626875]
["POLES","Base","Brazil","Secondary Energy|Hydrogen|Electricity","EJ/yr",3.07735530689824e-08,4.92751092410088e-05,3.92504154956818E-4,0.000209279747989655,0.000755499518508911]
["POLES","Base","Brazil","Secondary Energy|Hydrogen|Gas","EJ/yr",2.07961723409593e-07,0.000186648470020294,0.0016891595599823,0.01551699912854,0.0220343689291992]
["POLES","Base","Brazil","Water Withdrawal|Electricity|Cooling Pond","km3/yr",3.39444667929456e-08,5.40351123845539e-08,7.19674488891542e-08,7.68973720255417e-08,6.51439435728207e-08]
["POLES","Base","China","Capacity Additions|Electricity|Solar|PV","GW/yr",0.5796201171875,3.21001611328125,5.50047216796875,17.06453515625,22.34651953125]
["POLES","Base","China","Capacity|Electricity|Storage Reservoir","GWh",1.99999994947575e-07,141.380421875,454.41734375,588.416,692.3298125]
["POLES","Base","China","Land Cover|Cropland|Energy Crops","million ha",23118.30078125,23102.6123046875,22841.2719726562,22292.6171875,21493.53515625]
["POLES","Base","China","Primary Energy|Hydro","EJ/yr",2.60028720801562,3.99746668921875,5.7668152381875,5.9961419746875,6.0547728751875]
["POLES","Base","China","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",3.60064790903998e-10,0,0,0,0]
["POLES","Base","China","Secondary Energy|Solids","EJ/yr",78.3302519508311,98.3542878404297,112.238383339266,105.63687080775,83.467992465]
["POLES","Base","China","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.0583911053836346,0.511440694332123,1.06450390815735,1.48613023757935,1.37128150463104]
["POLES","Base","China","Water Withdrawal|Electricity|Once Through","km3/yr",66.3542327880859,98.1619186401367,97.2548294067383,60.8966903686523,13.3174047470093]
["POLES","Base","CN","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["POLES","Base","CN","Final Energy|Solids|Biomass|Traditional","EJ/yr",7.8550824830625,6.0492122814375,3.9982219486875,2.4665910721875,1.5114760138125]
["POLES","Base","CN","Primary Energy|Biomass|Hydrogen","EJ/yr",5.21538505669151e-05,0.0484398738045829,0.215873861933245,0.301174709828404,0.586879856605748]
["POLES","Base","CN","Resource|Cumulative Extraction|Gas","EJ",14.0741475163594,59.886596397375,160.27473641175,341.516473966125,561.885506073]
["POLES","Base","CN","Secondary Energy|Liquids|Biomass","EJ/yr",0.0443227619311523,0.221782707580078,0.771389606390625,1.62186917315625,2.02876774692187]
["POLES","Base","CN","Water Consumption|Electricity|Wet Tower","km3/yr",5.80508661270142,12.3136215209961,17.8078536987305,20.2249183654785,20.8240070343018]
["POLES","Base","CN","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["POLES","Base","EIT","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["POLES","Base","EIT","Final Energy|Residential and Commercial","EJ/yr",6.20917306410937,6.48151207676367,6.83692591028906,7.18388913367969,7.00620379488281]
["POLES","Base","EIT","Primary Energy","EJ/yr",28.0119940529369,31.8901033158432,34.8200570144765,36.4588656735478,35.3802561767791]
["POLES","Base","EIT","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",2.50581696479981,3.55124429643375,4.36869518533186,4.68610872745584,4.42116476682869]
["POLES","Base","EIT","Secondary Energy|Hydrogen|Nuclear","EJ/yr",1.90543879514735e-09,4.96647203162313e-06,1.51536900472641E-4,1.84117797743225E-3,0.00873467125213623]
["POLES","Base","EIT","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",3.18161996748501e-10,0,0,0,0]
["POLES","Base","EIT","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",22.0330982208252,19.8172225952148,18.36962890625,15.6740970611572,11.0358600616455]
["POLES","Base","EU","Capacity|Electricity|Wind|Onshore","GW",80.425296875,147.373328125,215.762953125,315.67846875,480.1380625]
["POLES","Base","EU","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",73.3939453125,31.74621484375,26.79823046875,37.84574609375,31.53948046875]
["POLES","Base","EU","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["POLES","Base","EU","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",1.94434980276637E-8,0,0,0,0]
["POLES","Base","EU","Secondary Energy|Heat","EJ/yr",2.32177522078125,2.32976808365625,2.68442945845312,3.10764150590625,3.47608971871875]
["POLES","Base","EU","Water Consumption|Electricity","km3/yr",10.4428977966309,9.6983060836792,9.76789855957031,9.7872428894043,10.0229511260986]
["POLES","Base","EU","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",3.17276406288147,1.05859553813934,0.587207853794098,0.491272985935211,0.173779115080833]
["POLES","Base","IN","Capacity|Electricity|Solar|PV","GW",0.0210007663157885,5.51487768363953,20.7892514648438,86.27845703125,262.94906640625]
["POLES","Base","IN","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",1.76746587385423e-07,0,0,0,0]
["POLES","Base","IN","Primary Energy|Biomass|Traditional","EJ/yr",5.298845481,4.8807359325,4.1210822863125,3.268918677375,2.49828138660938]
["POLES","Base","IN","Secondary Energy|Electricity","EJ/yr",3.4894309595355,6.023827393794,9.767559744342,14.449992730596,20.334432739176]
["POLES","Base","IN","Secondary Energy|Electricity|Ocean","EJ/yr",3.60064790903998e-10,3.15416756307939e-09,3.15416756307939e-09,3.15416756307939e-09,3.15416756307939e-09]
["POLES","Base","IN","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["POLES","Base","IN","Water Withdrawal|Electricity|Nuclear","km3/yr",1.27291917800903,2.04798865318298,2.41467690467834,2.07274651527405,1.62679600715637]
["POLES","Base","India","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","Base","India","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",925.6251875,1239.589875,1650.609875,2034.836875,2409.14625]
["POLES","Base","India","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",1.28594568179999E-9,0,0,0,0]
["POLES","Base","India","Primary Energy|Gas","EJ/yr",2.3886328561875,4.0823151350625,8.549104114125,11.942251689375,13.34767278825]
["POLES","Base","India","Secondary Energy|Electricity|Geothermal","EJ/yr",3.60064790903998e-10,0,0,0,0]
["POLES","Base","India","Water Consumption|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","Base","India","Water Consumption|Electricity|Fossil","km3/yr",1.30073118209839,2.05275797843933,3.15890336036682,4.38363885879517,5.71627807617188]
["POLES","Base","Japan","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","Base","Japan","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",3.41519917128608E-7,2.6591229470796E-8,8.45123795443214e-08,1.887378457468e-07,3.37930920068175e-07]
["POLES","Base","Japan","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",49.51693359375,47.71202734375,41.6689140625,35.6428359375,30.39381640625]
["POLES","Base","Japan","Primary Energy|Coal|w/ CCS","EJ/yr",2.42806319183728e-09,2.70883571256491E-10,8.4519939810707e-10,1.94059794738132e-09,3.54868577342131e-09]
["POLES","Base","Japan","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",1.08019437271199E-9,0,0,0,0]
["POLES","Base","Japan","Secondary Energy|Electricity|Wind","EJ/yr",0.0183764591204766,0.0810675067125937,0.242218235185875,0.53549815982175,0.894836810388375]
["POLES","Base","Japan","Water Consumption|Electricity|Oil","km3/yr",0.0230040866881609,0.0130953844636679,0.00740615464746952,0.00636671110987663,0.00781253911554813]
["POLES","Base","Japan","Water Withdrawal|Electricity|Solar","km3/yr",0.000379908888135105,0.00392018398270011,0.00882135331630707,0.01459223870188,0.0201727747917175]
["POLES","Base","LA","Capacity Additions|Electricity|Wind","GW/yr",0.327,1.09809790039063,1.98655212402344,3.67860668945313,4.7160361328125]
["POLES","Base","LA","Final Energy|Gases","EJ/yr",0.445710577746094,0.769738682460937,1.15594898540625,1.5176607024375,1.69280256023438]
["POLES","Base","LA","Primary Energy|Coal|Electricity","EJ/yr",0.145800525085714,0.389957110451116,0.830052289889397,1.29038644650937,1.79458385981786]
["POLES","Base","LA","Primary Energy|Non-Biomass Renewables","EJ/yr",1.48301390715653,1.92178713427184,2.4306771219862,3.04534728122057,3.72299210506823]
["POLES","Base","LA","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["POLES","Base","LA","Water Consumption|Electricity|Hydro","km3/yr",6.86706590652466,8.59011650085449,9.98617744445801,10.7183866500854,11.0215063095093]
["POLES","Base","LA","Water Withdrawal|Electricity|Coal","km3/yr",0.196989789605141,0.440278440713882,0.860603451728821,1.27357280254364,1.61965239048004]
["POLES","Base","LAM","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","Base","LAM","Emissions|CO2|Land Use","Mt CO2/yr",1185.5543125,-397.956703125,-1961.838625,-2962.995375,-3380.502625]
["POLES","Base","LAM","Primary Energy|Biomass|Traditional","EJ/yr",1.38114927070312,1.38244842574805,1.31653913733984,1.22979479479102,1.11276900215332]
["POLES","Base","LAM","Primary Energy|Gas|w/ CCS","EJ/yr",3.74406846873171e-09,0,0,0,0]
["POLES","Base","LAM","Secondary Energy|Hydrogen","EJ/yr",0.000124283756350301,0.00745914849108124,0.0776596694848022,0.404143355781738,0.958293285240234]
["POLES","Base","LAM","Secondary Energy|Hydrogen|Nuclear","EJ/yr",1.25264703111914E-5,0.000952846453674316,0.00375868970191956,0.0257124764984436,0.126313376904053]
["POLES","Base","LAM","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["POLES","Base","MAF","Capacity|Electricity|Gas|w/ CCS","GW",6.99999975040555e-07,7.77777750045061e-07,7.77777750045061e-07,7.77777750045061e-07,7.77777750045061e-07]
["POLES","Base","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Industry","Mt CO2/yr",492.90832421875,666.8512265625,803.17490234375,936.5586015625,1033.904984375]
["POLES","Base","MAF","Final Energy|Solar","EJ/yr",0.0759902513422852,0.16338985977832,0.233250185144531,0.3505241295,0.509262726375]
["POLES","Base","MAF","Primary Energy|Fossil|w/o CCS","EJ/yr",40.9496945387686,54.637832972725,69.2920822086497,79.9759016421139,83.8854674354108]
["POLES","Base","MAF","Secondary Energy|Gases","EJ/yr",22.689158895,37.16152130025,56.445359499,63.783406854,59.6489052195]
["POLES","Base","MAF","Secondary Energy|Hydrogen|Other","EJ/yr",3.88379810140905e-05,0.0676965382769205,0.0880629836289367,0.208194945390927,0.399037368999847]
["POLES","Base","MAF","Water Consumption|Electricity|Solar","km3/yr",3.11484513804317E-3,0.0112141286954284,0.0428064800798893,0.119605354964733,0.235039785504341]
["POLES","Base","OECD90","Capacity|Electricity|Biomass|w/ CCS","GW",3.39999994321261e-06,3.99999978253618e-06,3.99999978253618e-06,3.99999978253618e-06,3.99999978253618e-06]
["POLES","Base","OECD90","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",2.71236900880467e-06,0,0,0,0]
["POLES","Base","OECD90","Final Energy|Liquids","EJ/yr",115.123186026938,107.590342917573,97.7747277914385,84.9722975309795,73.6033375681875]
["POLES","Base","OECD90","Primary Energy|Oil","EJ/yr",124.407848330648,112.997875319367,96.2332520165859,80.3939384172656,66.6970722804375]
["POLES","Base","OECD90","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.185264491080716,1.2166765124354,2.43642180803902,4.63591765113332,8.30484624543426]
["POLES","Base","OECD90","Secondary Energy|Hydrogen|Gas","EJ/yr",1.04138602563798E-4,0.153427735330067,0.591031684223877,0.615815477840286,0.582678377132904]
["POLES","Base","OECD90","Water Withdrawal|Electricity|Cooling Pond","km3/yr",37.1307545972437,29.3943178536916,31.9675239244547,34.1542038587826,34.620428571765]
["POLES","Base","PAC","Capacity Additions|Electricity|Solar|PV","GW/yr",0.991000122070313,3.05161010742188,3.50418212890625,5.15065966796875,6.00670556640625]
["POLES","Base","PAC","Capacity|Electricity|Storage Reservoir","GWh",25.374,30.70630859375,34.46965234375,37.84364453125,42.9080625]
["POLES","Base","PAC","Final Energy|Gases","EJ/yr",1.44187226282813,1.38604161192188,1.612368081,1.74215920809375,1.81589840535937]
["POLES","Base","PAC","Primary Energy|Biomass|Modern","EJ/yr",0.297669468867548,0.558481463332031,1.1358037927272,1.5490256881459,1.63603980635592]
["POLES","Base","PAC","Secondary Energy|Electricity|Biomass","EJ/yr",0.084449598192,0.104946779208094,0.120674901948187,0.109761598063266,0.149987861706375]
["POLES","Base","PAC","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",8.38489685107743e-09,1.09358317131042E-4,0.0002577239015522,0.000520520671005249,0.00138140778337097]
["POLES","Base","PAC","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",2.62435101427982e-10,0,0,0,0]
["POLES","Base","PAC","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["POLES","Base","REF","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["POLES","Base","REF","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",1785.1233125,2050.5486875,2344.687125,2627.99325,2660.60925]
["POLES","Base","REF","Final Energy|Solids|Coal","EJ/yr",4.33541095664062,4.63377859755469,4.59815105566406,4.72280893699219,5.37822017648437]
["POLES","Base","REF","Resource|Cumulative Extraction|Gas","EJ",304.524855626625,849.575419455375,1513.85590737788,2312.121027816,3171.85335716287]
["POLES","Base","REF","Secondary Energy|Electricity|Hydro","EJ/yr",1.80120615876,1.77227185777312,1.88592743709562,2.02769558201925,2.17076868054225]
["POLES","Base","REF","Secondary Energy|Liquids|Coal","EJ/yr",0.0418349379770508,0.0659398231208496,0.125848819450195,0.330706674237305,0.611917358677734]
["POLES","Base","REF","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["POLES","Base","RER","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",7.80766822572332e-09,0.0511377143859863,0.047673454284668,0.080176155090332,0.0895899810791016]
["POLES","Base","RER","Emissions|CO2","Mt CO2/yr",63.316482421875,77.156298828125,83.86681640625,96.205384765625,101.27446484375]
["POLES","Base","RER","Primary Energy","EJ/yr",2.32505064860704,2.68140068839613,2.99947566174807,3.37923449996277,3.58484776095084]
["POLES","Base","RER","Primary Energy|Secondary Energy Trade","EJ/yr",-0.0335964078912964,0.00563482390731812,0.00251514905932617,2.18305051940918E-4,-0.00168386776446533]
["POLES","Base","RER","Secondary Energy|Electricity|Gas","EJ/yr",0.02135184264,0.0409262802484219,0.0619803802418906,0.0983917924915781,0.112713060480891]
["POLES","Base","RER","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",9.46553946334916e-10,0,0,0,0]
["POLES","Base","RER","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",0.0723879635334015,0.308932065963745,0.371854364871979,0.346988797187805,0.148863554000854]
["POLES","Base","Russia","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0,0.0245080757141113,0.102534027099609,0.220469985961914,0.325031311035156]
["POLES","Base","Russia","Capacity|Electricity|Wind|Onshore","GW",0.009,0.674127380371094,6.28332373046875,24.69568359375,57.60665234375]
["POLES","Base","Russia","Population","million",142.958,141.969,139.632,137.792,136.715]
["POLES","Base","Russia","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",2.57189136359999e-09,0,0,0,0]
["POLES","Base","Russia","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",7.20129581807996e-10,0,0,0,0]
["POLES","Base","Russia","Water Consumption|Electricity","km3/yr",3.89648365974426,4.47228240966797,5.36879253387451,6.10131454467773,6.74677038192749]
["POLES","Base","Russia","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",2.86274909973145,3.02937936782837,3.28474569320679,3.48607182502747,3.69513511657715]
["POLES","Base","Russia","Water Withdrawal|Electricity|Once Through","km3/yr",29.9806747436523,26.7451190948486,26.5015888214111,22.5716190338135,15.6861009597778]
["POLES","Base","US","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",1.76746587385423e-07,0,0,0,0]
["POLES","Base","US","GDP|PPP","billion US$2010/yr",14497.1263088,18867.64358344,23224.79265176,26940.64444832,30221.2186738]
["POLES","Base","US","Primary Energy|Biomass|w/ CCS","EJ/yr",1.79560178147221E-9,5.52220355624607e-20,3.57573401792377e-20,2.34568455853276e-20,1.53904015662789E-20]
["POLES","Base","US","Secondary Energy|Electricity|Ocean","EJ/yr",3.60064790903998e-10,3.15416756307939e-09,3.15416756307939e-09,3.15416756307939e-09,3.15416756307939e-09]
["POLES","Base","US","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["POLES","Base","US","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",1.09975334394719e-10,0,0,0,0]
["POLES","Base","US","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["POLES","Base","USA","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",2336.7225,2473.9415,2859.76425,3173.952,3283.12875]
["POLES","Base","USA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",1575.908375,1472.10225,1192.46975,995.3569375,812.32075]
["POLES","Base","USA","Primary Energy|Biomass|Hydrogen","EJ/yr",3.65357133443467e-08,0.00310839653639112,0.0530653937726702,0.127737583978271,0.296090975688825]
["POLES","Base","USA","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",11.0185193754718,13.1686483973116,15.0839992468558,16.2131300678888,15.7071344363165]
["POLES","Base","USA","Secondary Energy|Gases|Biomass","EJ/yr",0,0,0,0,0]
["POLES","Base","USA","Water Consumption|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","Base","USA","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["POLES","Base","World","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",2.07155523821712e-06,0,0,0,0]
["POLES","Base","World","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",869.4794375,1103.60875,1247.400375,1283.295125,1311.40275]
["POLES","Base","World","Primary Energy|Coal|w/ CCS","EJ/yr",1.59094105696678e-05,0.00102206303681946,1.19551927127838E-4,1.19483449859619E-5,2.01617191586494e-05]
["POLES","Base","World","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",6.15710768081546e-08,0,0,0,0]
["POLES","Base","World","Secondary Energy|Electricity|Wind","EJ/yr",1.33701928265925,4.706198613297,11.983902614262,23.54298097392,38.823436160856]
["POLES","Base","World","Water Consumption|Electricity|Oil","km3/yr",1.61601173877716,1.86377584934235,1.73160982131958,1.66030502319336,1.49014449119568]
["POLES","Base","World","Water Withdrawal|Electricity|Solar","km3/yr",0.0111685711890459,0.0702737420797348,0.225508287549019,0.590457916259766,1.10141444206238]
["POLES","FullTech","ASIA","Capacity Additions|Electricity|Wind","GW/yr",31.7241108398437,125.19999609375,169.4340859375,256.570021484375,335.02498828125]
["POLES","FullTech","ASIA","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["POLES","FullTech","ASIA","Final Energy|Heat","EJ/yr",6.59522003227954,9.9250736789729,11.9035747751133,13.1810120024711,13.0157555812501]
["POLES","FullTech","ASIA","Primary Energy|Non-Biomass Renewables","EJ/yr",8.36771790492437,21.6835250253323,51.0233681933242,71.33642510244,94.3145765054217]
["POLES","FullTech","ASIA","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["POLES","FullTech","ASIA","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",2.88717245054888e-06,0.0461644043561554,0.112031647322388,0.076612846185791,0.0840761088230896]
["POLES","FullTech","ASIA","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",31.5581964254379,53.7016446590424,75.2624731063843,71.723774433136,68.242733001709]
["POLES","FullTech","Brazil","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","FullTech","Brazil","Capacity|Electricity|Solar|CSP","GW",1.06149644125253E-6,0.0018853976726532,1.22036279296875,4.78833026123047,8.17412536621094]
["POLES","FullTech","Brazil","Emissions|CO2|Land Use","Mt CO2/yr",287.9961875,-276.05746875,-1722.13225,-2237.031,-2910.08125]
["POLES","FullTech","Brazil","Primary Energy|Gas|Hydrogen","EJ/yr",8.43297518149484e-08,0.000304729191132954,0.029171758896528,0.439243938689314,0.920061346979632]
["POLES","FullTech","Brazil","Resource|Cumulative Extraction|Oil","EJ",23.3174767138594,91.5024814541719,167.531796171984,218.960160986672,248.806706407805]
["POLES","FullTech","Brazil","Secondary Energy|Hydrogen","EJ/yr",6.70263218745589e-07,0.000979371952033996,0.0104460436400757,0.135899705091797,0.292074684257813]
["POLES","FullTech","Brazil","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["POLES","FullTech","China","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",57.990296875,17.651177734375,0.160648529052734,1.230423828125,1.44373986816406]
["POLES","FullTech","China","Capacity|Electricity|Gas|w/o CCS","GW",62.3599999,149.441531138889,353.871515625,553.140765625,729.6500625]
["POLES","FullTech","China","Final Energy|Solar","EJ/yr",0.493315107046875,1.45035053282812,1.89253320004688,2.16007838803125,1.889922828375]
["POLES","FullTech","China","Primary Energy|Fossil|w/o CCS","EJ/yr",88.0648673128539,125.809995484294,70.9428750865312,39.2563886428125,30.69226111275]
["POLES","FullTech","China","Primary Energy|Solar","EJ/yr",0.49669611159375,1.66078220821875,3.50478303665625,5.88666435075,7.69727741175]
["POLES","FullTech","China","Secondary Energy|Hydrogen|Other","EJ/yr",2.70026010610804E-5,0.0179581234679677,0.186938698895694,0.58522163746341,0.996642739767906]
["POLES","FullTech","China","Water Consumption|Electricity|Solar","km3/yr",9.39089004532434e-05,0.00584939867258072,0.0510087981820107,0.167612567543983,0.293240666389465]
["POLES","FullTech","China","Water Withdrawal|Electricity|Gas","km3/yr",1.10961771011353,3.17113780975342,5.05810546875,8.53335571289062,3.9739875793457]
["POLES","FullTech","CN","Capacity|Electricity|Biomass|w/o CCS","GW",0.960001303808596,15.2117860151654,51.4108826948529,105.450470703125,138.5753515625]
["POLES","FullTech","CN","Final Energy|Liquids","EJ/yr",15.5463933010562,23.4532419629766,21.9741696550547,16.3452317103281,14.52321632475]
["POLES","FullTech","CN","Price|Primary Energy|Coal","US$2010/GJ",3.55990976251799,4.20257910668958,4.37327035395705,4.95005218144689,5.68802569422053]
["POLES","FullTech","CN","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["POLES","FullTech","CN","Secondary Energy|Hydrogen|Gas","EJ/yr",1.69159914751053e-05,0.0166068946691895,0.185501223509766,0.582268375019531,0.991357454742188]
["POLES","FullTech","CN","Water Consumption|Electricity|Fossil","km3/yr",6.5684552192688,10.2461309432983,4.23425960540771,3.47564125061035,4.43514919281006]
["POLES","FullTech","CN","Water Withdrawal|Electricity|Cooling Pond","km3/yr",10.2731599807739,11.6144275665283,4.49900531768799,2.48600220680237,0]
["POLES","FullTech","EIT","Capacity|Electricity|Storage","GW",1.99999994947575e-07,9.157345703125,19.524673828125,97.3364921875,180.6788125]
["POLES","FullTech","EIT","Final Energy|Electricity","EJ/yr",2.5231063303125,3.116035058625,3.185589582,3.78903470146875,4.445537698125]
["POLES","FullTech","EIT","Land Cover|Cropland|Energy Crops","million ha",20768.271484375,20289.5788574219,19740.6079101562,19287.8869628906,18952.7661132812]
["POLES","FullTech","EIT","Secondary Energy|Electricity|Biomass","EJ/yr",2.01636280810386e-08,0.0084059246105332,0.0788204421575156,0.95496329995875,2.0117380726845]
["POLES","FullTech","EIT","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",7.95941324080923e-09,1.55792758879461E-3,0.0125656934070329,0.00845510518346738,0.00588704922196886]
["POLES","FullTech","EIT","Secondary Energy|Solids","EJ/yr",6.67565691795358,7.23837933395508,4.98519299446875,5.02197542261719,6.4922038515]
["POLES","FullTech","EIT","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",1.75791754486454e-07,0.0542460568249226,0.396215081214905,0.436193078756332,0.222953766584396]
["POLES","FullTech","EU","Capacity|Electricity|Oil|w/ CCS","GW",0,0,0,0,0]
["POLES","FullTech","EU","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",1230.333625,967.041125,452.96340625,113.7276484375,21.2408125]
["POLES","FullTech","EU","Final Energy|Solids|Coal","EJ/yr",2.37678126834375,1.86543380995312,0.819886570101563,0.456086645683594,0.475222243359375]
["POLES","FullTech","EU","Resource|Cumulative Extraction|Gas","EJ",46.3241208164062,104.21001460125,147.06366582375,179.515844554922,208.713777380156]
["POLES","FullTech","EU","Secondary Energy|Heat","EJ/yr",2.32177522078125,2.32430480029688,2.9233133836875,3.584956658625,3.6106171633125]
["POLES","FullTech","EU","Secondary Energy|Liquids|Coal","EJ/yr",0.006764331331604,0,0,0,0]
["POLES","FullTech","EU","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["POLES","FullTech","IN","Capacity|Electricity|Gas|w/ CCS","GW",9.99999974737875e-08,1.11111112346407e-07,11.0645888671875,98.0790859375,224.23465625]
["POLES","FullTech","IN","Emissions|CO2","Mt CO2/yr",1692.4725078125,1910.3259375,1212.4255546875,536.3225703125,154.184921875]
["POLES","FullTech","IN","Final Energy|Residential and Commercial","EJ/yr",8.296217469,8.74024167403125,8.6398916011875,9.120776328,10.8208377527344]
["POLES","FullTech","IN","Primary Energy","EJ/yr",29.1702121075952,35.4739405185665,35.3151854453015,37.5838342981344,46.5229083912591]
["POLES","FullTech","IN","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",2.87056260719981,3.48968221725375,1.93605193131834,0.352492208272547,0.238040347754601]
["POLES","FullTech","IN","Secondary Energy|Hydrogen|Nuclear","EJ/yr",4.49697943319916E-9,0.000368456176139832,0.00148225056289673,0.00683754986206055,0.0301587490458984]
["POLES","FullTech","IN","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",2.86599383114705e-10,0,0.063877560198307,0.133276969194412,0.238026589155197]
["POLES","FullTech","IN","Water Withdrawal|Electricity|Solar|CSP","km3/yr",9.07820067368448e-05,0.00572222378104925,0.0242966841906309,0.0489462800323963,0.069444015622139]
["POLES","FullTech","India","Capacity|Electricity|Wind|Onshore","GW",13.395,96.2361796875,275.43734375,447.1026875,632.5405]
["POLES","FullTech","India","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",35.10605859375,37.72475390625,60.8997265625,16.365125,4.2897998046875]
["POLES","FullTech","India","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",2.57189136359999e-09,0,0.489491167330246,0.964881111071149,1.62200627800614]
["POLES","FullTech","India","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",7.20129581807996e-10,0,0.137057526852469,0.270166711099922,0.454161757841719]
["POLES","FullTech","India","Secondary Energy|Electricity|Solar","EJ/yr",2.70684053716553E-4,0.0674573315407031,0.606365607416625,1.67454436374,3.252923970939]
["POLES","FullTech","India","Water Consumption|Electricity|Biomass","km3/yr",0.00322774681262672,0.125053599476814,0.441102027893066,0.795442521572113,1.27405631542206]
["POLES","FullTech","India","Water Withdrawal|Electricity|Once Through","km3/yr",37.5179977416992,34.838565826416,20.436637878418,15.5734062194824,11.1234245300293]
["POLES","FullTech","Japan","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",4.02391137695312,1.75574499511719,2.67164068645798e-15,9.09494701772928e-16,0.0209117469787598]
["POLES","FullTech","Japan","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",242.710109198154,186.438375,35.541169921875,-28.3185078125,-45.7427192382813]
["POLES","FullTech","Japan","Primary Energy|Biomass|w/ CCS","EJ/yr",1.38843664592423e-09,9.10186148088542e-10,1.55621180926391e-09,0.21150765028125,0.69676758309375]
["POLES","FullTech","Japan","Secondary Energy|Electricity|Biomass","EJ/yr",0.084449598192,0.126021048456375,0.195354873173812,0.293247884494687,0.407589359131125]
["POLES","FullTech","Japan","Secondary Energy|Electricity|Oil","EJ/yr",0.350890348896,0.235642129824937,0.0830632572892969,0.0266356177671094,6.0463172519577E-5]
["POLES","FullTech","Japan","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",1.16072082501084e-11,0,0.00611649127677083,0.0294570308178663,0.0353331007063389]
["POLES","FullTech","Japan","Water Withdrawal|Electricity|Sea Cooling","km3/yr",89.2851333618164,82.7570114135742,79.5782241821289,74.1384811401367,70.8847579956055]
["POLES","FullTech","LA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0.893815124511719,2.00523120117187,1.1247939453125]
["POLES","FullTech","LA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",41.9815859375,41.72889453125,27.623126953125,15.8270810546875,11.0564462890625]
["POLES","FullTech","LA","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",1.28594568179999E-9,0,0,0.489833098286384,1.92675898634464]
["POLES","FullTech","LA","Primary Energy|Gas","EJ/yr",0.8939936660625,1.62626335059375,1.4598174436875,1.39818398610937,1.05598153047656]
["POLES","FullTech","LA","Secondary Energy|Electricity|Geothermal","EJ/yr",3.60064790903998e-10,0,0,0,0]
["POLES","FullTech","LA","Water Consumption|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","FullTech","LA","Water Consumption|Electricity|Solar|CSP","km3/yr",8.64033378178419e-09,5.41805775355897E-6,0.00350466300733387,0.0137479389086366,0.0234599858522415]
["POLES","FullTech","LAM","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,9.82287658691406,13.1272384033203]
["POLES","FullTech","LAM","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",18.195296875,25.3257275390625,13.1815244140625,4.63300988769531,2.35148922729492]
["POLES","FullTech","LAM","Price|Primary Energy|Oil","US$2010/GJ",25.1335382466103,37.0873665657018,23.0450531330949,10.0109495050167,8.54411602156932]
["POLES","FullTech","LAM","Primary Energy|Coal|w/o CCS","EJ/yr",2.01016548938135,2.9059724676645,1.32236473069116,0.372776215095703,0.170683559762695]
["POLES","FullTech","LAM","Secondary Energy|Electricity|Wind","EJ/yr",0.0227572021021465,0.241462197561094,1.3796560183905,3.11949397036125,4.74101226612675]
["POLES","FullTech","LAM","Water Consumption|Electricity|Coal","km3/yr",0.18075031042099,0.304735850542784,0.183203851804137,0.132623082026839,0.172700643539429]
["POLES","FullTech","LAM","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.455715239048004,0.452234214171767,0.207020630594343,0.0582916845993395,0.00434022904209996]
["POLES","FullTech","MAF","Capacity Additions|Electricity|Wind","GW/yr",0.168,3.57138525390625,13.2953037109375,27.205509765625,38.917015625]
["POLES","FullTech","MAF","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["POLES","FullTech","MAF","Final Energy|Heat","EJ/yr",0.0555781498637695,0.168906101660156,0.264856845339844,0.357983379808594,0.383242867558594]
["POLES","FullTech","MAF","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",1.80032393580702e-08,0,0.576388321069922,1.3335725724077,2.42026707636763]
["POLES","FullTech","MAF","Resource|Cumulative Extraction|Gas","EJ",117.72403157025,411.081469574625,775.508548829625,1127.00516075775,1538.2810273815]
["POLES","FullTech","MAF","Secondary Energy|Hydrogen|Coal","EJ/yr",1.34507372488976E-5,0.00119185312211609,5.21429378329468E-3,0.0036929114362793,0.00283950659344482]
["POLES","FullTech","MAF","Water Consumption|Electricity|Hydro","km3/yr",2.16414308547974,2.7165744304657,3.5603711605072,3.81331396102905,4.10081481933594]
["POLES","FullTech","OECD90","Capacity Additions|Electricity|Nuclear","GW/yr",1.53840209960938,19.4100553436279,18.0687324981689,18.948273563385,38.732926838398]
["POLES","FullTech","OECD90","Capacity|Electricity|Oil|w/o CCS","GW",310.125736999512,255.273532958984,245.11867199707,218.336259277344,182.749596435547]
["POLES","FullTech","OECD90","Emissions|CO2|Land Use","Mt CO2/yr",-2041.27348632813,-1754.90339453125,-1444.18375488281,-828.99503125,-1180.17934375]
["POLES","FullTech","OECD90","Primary Energy|Gas|Hydrogen","EJ/yr",1.33649248341917e-05,0.0887634790013552,4.26929441272496,18.8412254162096,61.1058379825195]
["POLES","FullTech","OECD90","Primary Energy|Gas|w/ CCS","EJ/yr",2.54596640642267E-8,0,7.99594752877625,39.8654630661621,57.5634961402559]
["POLES","FullTech","OECD90","Secondary Energy|Hydrogen","EJ/yr",3.69963800109965E-4,0.433176874377731,1.78491836990479,6.20144848199487,20.8980645121208]
["POLES","FullTech","OECD90","Secondary Energy|Liquids|Gas","EJ/yr",0.545232653648438,0.0464208434604492,0.0420300238447266,0.0517992408808594,0]
["POLES","FullTech","OECD90","Water Withdrawal|Electricity","km3/yr",359.957687497139,224.749526262283,136.828146636486,96.1852939724922,124.283955395222]
["POLES","FullTech","PAC","Capacity|Electricity|Gas|w/o CCS","GW",119.9819999,163.381562388889,154.978186035156,124.10816796875,127.71490625]
["POLES","FullTech","PAC","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",167.8141875,138.24853125,83.5317421875,48.3916171875,29.937490234375]
["POLES","FullTech","PAC","Final Energy|Solids","EJ/yr",2.3327522471412,2.40616645217029,1.90758724013672,1.39334143469238,0.823222282385743]
["POLES","FullTech","PAC","Primary Energy|Solar","EJ/yr",0.0366901672675781,0.187908572179688,0.419039803125,0.703994474179688,0.910884705539063]
["POLES","FullTech","PAC","Secondary Energy|Gases|Biomass","EJ/yr",3.7365245285511e-05,0.00081497404234314,3.47074482540894E-3,0.00341683057589722,0.00337422342068481]
["POLES","FullTech","PAC","Secondary Energy|Hydrogen|Solar","EJ/yr",-1.15825305696684E-8,-0.00372840718164378,-0.0342150366107848,-0.0856462403145325,-0.137773207404336]
["POLES","FullTech","PAC","Water Withdrawal|Electricity|Gas","km3/yr",0.480593502521515,0.403121292591095,0.281699866056442,0.300984144210815,0.245157778263092]
["POLES","FullTech","REF","Capacity Additions|Electricity|Hydro","GW/yr",0.072,0.0480409240722656,0.0276237888336182,0.049511402130127,1.42974230957031]
["POLES","FullTech","REF","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",1.43731963180471E-6,0,0,430.378265625,975.64415625]
["POLES","FullTech","REF","Final Energy|Liquids","EJ/yr",13.5914144571463,15.6440033351104,13.929649763625,11.0764291769648,10.2532907225742]
["POLES","FullTech","REF","Primary Energy|Oil","EJ/yr",17.2417310780625,20.513612570625,16.3956638424375,12.089208369375,10.40684876775]
["POLES","FullTech","REF","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",2.78926356412567,2.50166221190887,0.531253813359691,0.0534290416685859,0.00464985010364065]
["POLES","FullTech","REF","Secondary Energy|Hydrogen|Gas","EJ/yr",7.53631635699305e-07,0.0971670417890625,0.164673580086914,0.460589673788086,0.832885643707031]
["POLES","FullTech","REF","Water Withdrawal|Electricity|Cooling Pond","km3/yr",3.06019032336735E-7,6.8315894452553e-07,1.10095362515494e-06,1.60936275506174e-06,1.8990244257111E-6]
["POLES","FullTech","REF","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["POLES","FullTech","RER","Capacity|Electricity|Storage Reservoir","GWh",3.15300048828125,7.91701904296875,9.547412109375,16.2651962890625,25.663341796875]
["POLES","FullTech","RER","Land Cover|Cropland|Energy Crops","million ha",504.805297851562,524.322853088379,541.494598388672,556.120223999023,569.010009765625]
["POLES","FullTech","RER","Primary Energy|Hydro","EJ/yr",0.598108298730469,0.6222337115625,0.625500355957031,0.625175838070313,0.618933376511719]
["POLES","FullTech","RER","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",1.08019434651383e-09,0,0,0.00744441533954297,0.0307398712435312]
["POLES","FullTech","RER","Secondary Energy|Solids","EJ/yr",0.204046912718262,0.267366262592285,0.298432967668945,0.338935573584229,0.370504551557373]
["POLES","FullTech","RER","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.063135102391243,0.118918187916279,0.0731220170855522,0.0800201892852783,0.0388531945645809]
["POLES","FullTech","RER","Water Withdrawal|Electricity|Oil","km3/yr",0.00362203596159816,0.0476266629993916,0.0174703728407621,0.0102113541215658,1.67076021898538E-3]
["POLES","FullTech","Russia","Capacity|Electricity|Oil|w/o CCS","GW",16,14.6554208984375,7.19302734375,6.287572265625,5.14161767578125]
["POLES","FullTech","Russia","Final Energy|Solids|Coal","EJ/yr",1.04076701001562,0.993759631242187,0.417579942832031,0.202754560201172,0.121557625435547]
["POLES","FullTech","Russia","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",1.05161653522893E-8,1.15714741094104E-7,3.15383294726988e-07,2.09677139383608e-07,1.39400212345312e-07]
["POLES","FullTech","Russia","Resource|Cumulative Extraction|Oil","EJ",122.88473358525,344.112841446187,562.906743787125,755.710476733687,908.106104318062]
["POLES","FullTech","Russia","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",2.93899544011219e-09,0.00159579298086548,0.0515445575097656,0.153917838079102,0.285589825787109]
["POLES","FullTech","Russia","Water Consumption|Electricity|Fossil","km3/yr",0.695477068424225,0.858265697956085,0.455000907182693,0.453290045261383,0.263304471969604]
["POLES","FullTech","Russia","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["POLES","FullTech","US","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Oil","Mt CO2/yr",0,0,0,0,0]
["POLES","FullTech","US","Final Energy|Residential and Commercial","EJ/yr",20.3140108466367,21.1621191472617,18.8503005375703,18.2833196658047,19.8852315408984]
["POLES","FullTech","US","Primary Energy","EJ/yr",87.0909058644076,88.7569400232745,70.2986662823121,63.0530996006465,68.1528798196609]
["POLES","FullTech","US","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",11.0185193754718,11.7997934086941,5.3921090963707,0.518483051559703,0.198875424446984]
["POLES","FullTech","US","Secondary Energy|Hydrogen|Nuclear","EJ/yr",4.33428579944302e-09,0.000853465454200745,0.0118152766043701,0.0536486238325195,0.136610510475586]
["POLES","FullTech","US","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",2.90325458118801e-10,0,0.0955881029367447,0.196301892399788,0.274872660636902]
["POLES","FullTech","US","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",84.1324462890625,40.88232421875,7.92909479141235,0.375147223472595,0.050894983112812]
["POLES","FullTech","USA","Capacity|Electricity|Wind|Onshore","GW",40.298,122.014421875,478.68021875,731.1561875,942.6605625]
["POLES","FullTech","USA","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",34.3002421875,53.6153125,49.99474609375,15.026126953125,0.352737762451172]
["POLES","FullTech","USA","Price|Carbon","US$2010/tCO2",0.98181813955307,26.1272735595703,346.5,1088.09997558594,1490.39990234375]
["POLES","FullTech","USA","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",7.20129581807996e-10,0,0.216430246527047,0.445711346416406,0.639127537877812]
["POLES","FullTech","USA","Secondary Energy|Electricity|Solar","EJ/yr",0.0205457563596445,0.236864971771875,0.64641522129975,1.31612607255825,2.537945097903]
["POLES","FullTech","USA","Water Consumption|Electricity|Biomass","km3/yr",0.0927817970514297,0.0961872711777687,0.259388983249664,0.763302326202393,1.8312577009201]
["POLES","FullTech","USA","Water Consumption|Electricity|Nuclear","km3/yr",1.53219425678253,1.82307088375092,2.80196070671082,2.38698983192444,2.46863889694214]
["POLES","FullTech","USA","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["POLES","FullTech","World","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",8639.35098991976,9330.135,1822.3438125,-875.07375,-2066.8805859375]
["POLES","FullTech","World","Primary Energy|Biomass|Hydrogen","EJ/yr",0.000544521910735539,0.233953184085519,0.755103661146763,0.810696310463169,0.897690105803571]
["POLES","FullTech","World","Primary Energy|Biomass|w/ CCS","EJ/yr",1.33575542607307E-5,0.00823525275970459,0.00935987390167236,15.246086970375,57.2574155265]
["POLES","FullTech","World","Secondary Energy|Electricity|Ocean","EJ/yr",2.05236922693849e-08,0.0832489578968906,0.335887292581875,0.57111757016175,0.676674223189875]
["POLES","FullTech","World","Secondary Energy|Hydrogen|Biomass","EJ/yr",1.52466135005951E-4,0.0655068915439453,0.211429025121094,0.226994966929688,0.251353229625]
["POLES","FullTech","World","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",6.14725159664431e-09,0,1.82505702972412,8.64299201965332,12.8825855255127]
["POLES","Conv","ASIA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,67.8956943359375,94.070783203125,85.998361328125]
["POLES","Conv","ASIA","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",9341.8666875,10535.7701875,2318.056265625,393.987192382813,-1568.96875]
["POLES","Conv","ASIA","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",1649.58140625,2488.7233125,1935.25796875,1656.9205859375,892.086171875]
["POLES","Conv","ASIA","Primary Energy|Gas","EJ/yr",20.5671653406562,41.535097065,55.9708413249375,106.754844535875,91.0529975638125]
["POLES","Conv","ASIA","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0706159089360648,0.183143064506344,0.303508156011187,0.232407496133156,0.25664980115025]
["POLES","Conv","ASIA","Secondary Energy|Gases|Coal","EJ/yr",0,0.683254311724731,0.618102925089478,0.428801775226227,0.341258911865936]
["POLES","Conv","ASIA","Water Consumption|Electricity|Fossil","km3/yr",16.8631038665771,19.8048120737076,7.59433054924011,12.5587937831879,10.890148639679]
["POLES","Conv","Brazil","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,1.37743676757812,2.69145068359375]
["POLES","Conv","Brazil","Capacity|Electricity|Coal|w/ CCS","GW",1.99999994947575e-07,2.35294108279049e-07,0.300830825805664,0.915422241210938,1.68053967285156]
["POLES","Conv","Brazil","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",433.9589375,561.663375,308.053125,75.5491328125,-173.72990625]
["POLES","Conv","Brazil","Primary Energy|Coal|w/o CCS","EJ/yr",0.605486908380385,0.565535881421253,0.175806461188477,0.0582422109082031,0.0241241351220703]
["POLES","Conv","Brazil","Primary Energy|Oil|w/o CCS","EJ/yr",4.378157694,5.534974459125,3.32923574615625,1.63899367579688,1.05967237457812]
["POLES","Conv","Brazil","Secondary Energy|Electricity|Wind|Offshore","EJ/yr",2.59246651546732E-8,6.31255524490723E-3,0.0259572331798594,0.0646560344292187,0.093170761468875]
["POLES","Conv","Brazil","Secondary Energy|Solids|Biomass","EJ/yr",2.14029494029687,4.157538193125,12.0421085048437,19.3771102899375,27.9604863059063]
["POLES","Conv","Brazil","Water Withdrawal|Electricity|Solar","km3/yr",1.51154338823289e-07,0.000421526579884812,0.00794194079935551,0.0275796074420214,0.0449871830642223]
["POLES","Conv","China","Capacity Additions|Electricity|Wind","GW/yr",13.641806640625,69.8636328125,59.90223828125,130.0144296875,123.269703125]
["POLES","Conv","China","Final Energy|Gases","EJ/yr",2.17329510164062,4.75832338621875,5.9551518943125,4.1215022746875,3.256834525875]
["POLES","Conv","China","Primary Energy|Coal|Electricity","EJ/yr",42.0864056182286,51.1247875913357,9.85233256498928,4.56014956312768,5.37538851187232]
["POLES","Conv","China","Primary Energy|Non-Biomass Renewables","EJ/yr",3.3509787052931,10.2291032468868,20.1928350061999,27.6437113866061,33.630538385705]
["POLES","Conv","China","Secondary Energy|Hydrogen|Coal","EJ/yr",9.04906698578596e-06,0.0243208845681152,0.019181399744751,0.0128324615042725,0.00853441257568359]
["POLES","Conv","China","Water Consumption|Electricity|Hydro","km3/yr",12.526330947876,22.5258560180664,30.5158805847168,27.2897510528564,27.0830783843994]
["POLES","Conv","China","Water Withdrawal|Electricity|Coal","km3/yr",78.8667602539062,65.573860168457,9.14658164978027,2.84335684776306,1.46830797195435]
["POLES","Conv","CN","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","Conv","CN","Emissions|CO2|Land Use","Mt CO2/yr",-292.35975,-386.98725,-180.997125,-69.695359375,-256.49440625]
["POLES","Conv","CN","Final Energy|Transportation","EJ/yr",7.60192206046875,13.1037555852773,12.4330568425313,10.6461683000859,11.8064859905039]
["POLES","Conv","CN","Primary Energy|Gas|w/ CCS","EJ/yr",7.48813693746342e-10,0,5.1920604928125,16.077648252375,19.717898146875]
["POLES","Conv","CN","Secondary Energy|Hydrogen","EJ/yr",5.96739913287163e-05,0.0913050413701172,0.328049415720703,1.00749863179688,2.16688864345313]
["POLES","Conv","CN","Water Consumption|Electricity|Gas","km3/yr",0.0441036522388458,0.247456386685371,1.04956161975861,2.56957507133484,3.09758329391479]
["POLES","Conv","CN","Water Withdrawal|Electricity","km3/yr",82.7631225585938,105.155937194824,57.7845993041992,40.4787864685059,19.1228485107422]
["POLES","Conv","EIT","Capacity|Electricity|Gas|w/o CCS","GW",206.6839999,308.847999888889,306.00841796875,290.77698828125,336.78638671875]
["POLES","Conv","EIT","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Residential and Commercial","Mt CO2/yr",151.125046875,116.4260546875,37.1512109375,13.6547294921875,7.80339892578125]
["POLES","Conv","EIT","Final Energy|Solids","EJ/yr",1.39838388867006,1.51732340489575,1.66804276951758,1.77135426740039,2.00378205708398]
["POLES","Conv","EIT","Primary Energy|Coal|w/o CCS","EJ/yr",4.77089849732606,3.12021514266202,1.60238973861914,1.28267580625488,1.17339848635254]
["POLES","Conv","EIT","Secondary Energy|Gases","EJ/yr",22.428614331,22.18941983025,12.630116761875,15.857610978375,14.360735775375]
["POLES","Conv","EIT","Secondary Energy|Hydrogen|Other","EJ/yr",2.01098025837673e-08,0.0327549770270361,0.0700424856260735,0.200060707408727,0.315093099161797]
["POLES","Conv","EIT","Water Consumption|Electricity|Solar","km3/yr",8.90583873314199e-09,9.65616563917138e-05,0.00619878200814128,0.0143310474231839,0.0204755440354347]
["POLES","Conv","EIT","Water Withdrawal|Electricity|Gas","km3/yr",14.9748754501343,9.95694065093994,3.20322942733765,2.3122410774231,0.304369032382965]
["POLES","Conv","EU","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",2.15892493724823e-06,0,0,20.20226171875,61.20344140625]
["POLES","Conv","EU","Final Energy|Liquids","EJ/yr",21.6715704022969,18.7030798111406,12.8232196645781,7.44868599820312,6.27150568457813]
["POLES","Conv","EU","Price|Primary Energy|Coal","US$2010/GJ",3.32870188421787,3.89898281629509,4.90607463244074,5.84106254249632,6.46306679972471]
["POLES","Conv","EU","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["POLES","Conv","EU","Secondary Energy|Hydrogen|Gas","EJ/yr",7.63358532800674e-05,0.0477822740888672,0.261107267466797,0.580943727105469,0.93993692709375]
["POLES","Conv","EU","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",4.59663329621662e-09,0,0,0.0374580658972263,0.116242818534374]
["POLES","Conv","EU","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","Conv","IN","Capacity|Electricity|Storage Reservoir","GWh",1.99999994947575e-07,12.3214169921875,123.5839765625,384.81046875,653.1693125]
["POLES","Conv","IN","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",3.63932049367577e-08,0,58.17016796875,211.25871875,289.6370625]
["POLES","Conv","IN","Policy Cost|Area under MAC Curve","billion US$2010/yr",0,8.17343997955322,514.080017089844,2041.67126464844,2825.43701171875]
["POLES","Conv","IN","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",3.60064790903998e-10,0,0,0.436471703892562,1.35147340893375]
["POLES","Conv","IN","Secondary Energy|Hydrogen|Coal","EJ/yr",7.24583409517072e-09,1.12245127102661E-3,0.00716575010888672,4.90761464419556E-3,0.00326556249362183]
["POLES","Conv","IN","Secondary Energy|Solids|Biomass","EJ/yr",7.11634382199536,7.58067441844922,8.78897782504687,8.74431987890625,6.320789717625]
["POLES","Conv","IN","Water Withdrawal|Electricity|Oil","km3/yr",1.75123965740204,2.65143465995789,2.26069736480713,0.142223253846169,0.0482948534190655]
["POLES","Conv","India","Capacity|Electricity|Storage","GW",1.99999994947575e-07,12.3214169921875,123.5839765625,384.81046875,653.1693125]
["POLES","Conv","India","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",925.6251875,722.1749375,218.520828125,-62.82323828125,-268.02625]
["POLES","Conv","India","Primary Energy|Biomass|Hydrogen","EJ/yr",2.84871983695276e-08,0.00504836667153495,1.40305687314442E-3,0.00344241615886688,0.00642330237481253]
["POLES","Conv","India","Resource|Cumulative Extraction|Gas","EJ",8.16946504284375,25.9500249331172,42.8140832639766,56.8558278921797,66.811054864377]
["POLES","Conv","India","Secondary Energy|Electricity|Hydro","EJ/yr",0.412000546752,0.719906809905,0.900095219231625,0.853011008098875,0.85945611175875]
["POLES","Conv","India","Secondary Energy|Liquids|Coal","EJ/yr",0.0370524414836426,0,0,0,0]
["POLES","Conv","India","Water Withdrawal|Electricity|Geothermal","km3/yr",0,0,0,0,0]
["POLES","Conv","Japan","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0.367846160888672,0.19374690246582,0.500934478759766,0.408953399658203,0.412428192138672]
["POLES","Conv","Japan","Emissions|CO2","Mt CO2/yr",1109.451875,991.01621484375,437.3669140625,161.757568359375,81.1386015625]
["POLES","Conv","Japan","Primary Energy","EJ/yr",18.6174949571534,17.5403236881735,12.7864805379667,11.3443668485463,11.5001446036124]
["POLES","Conv","Japan","Primary Energy|Secondary Energy Trade","EJ/yr",-3.60064800042892e-10,-0.00627772926900035,-0.0404490472292054,-0.0683483501994203,-0.0342511164181703]
["POLES","Conv","Japan","Secondary Energy|Electricity|Gas","EJ/yr",1.09645132572,1.3223841113025,1.04159196531225,1.17324178301475,1.11546713544975]
["POLES","Conv","Japan","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",3.19805570914156e-11,0,2.38950620405376E-3,0.00334961921907961,0.00434215692803264]
["POLES","Conv","Japan","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",1.89955639839172,1.10825788974762,0.201261922717094,0.0146376881748438,0.00408178847283125]
["POLES","Conv","Japan","Water Withdrawal|Electricity|Solar|PV","km3/yr",0.00037990027340129,0.00415297551080585,0.00693406071513891,0.0110347652807832,0.0144403334707022]
["POLES","Conv","LA","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",12.3597333984375,7.323052734375,0.217774551391602,1.69118135027651E-20,0]
["POLES","Conv","LA","Price|Carbon","US$2010/tCO2",2.40000009536743,63.3600006103516,840,2637.81811523438,3613.0908203125]
["POLES","Conv","LA","Primary Energy|Coal|Hydrogen","EJ/yr",4.27388846049351e-07,0.000916974506950378,1.93081454470498E-3,1.25387239927564E-3,0.000833656052868707]
["POLES","Conv","LA","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",0.0408241463038704,0.0463215172319297,0.00748498504311914,0.00056738072343164,0.000197989928648439]
["POLES","Conv","LA","Secondary Energy|Gases|Coal","EJ/yr",0,0.0146699323659668,0.0177241779228516,0.013867336298584,0.0127239302647705]
["POLES","Conv","LA","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",6.86706590652466,8.8276891708374,10.7617664337158,11.4046640396118,12.0725164413452]
["POLES","Conv","LA","Water Withdrawal|Electricity|Once Through","km3/yr",1.38696229457855,2.23214650154114,2.4002788066864,2.99232816696167,3.20968341827393]
["POLES","Conv","LAM","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",8.84951878106222e-07,0,18.7784520263672,31.3656616210938,35.0060551757812]
["POLES","Conv","LAM","GDP|PPP","billion US$2010/yr",8714.36792426,12627.69099192,17240.59617918,22152.88028658,27572.9003462]
["POLES","Conv","LAM","Primary Energy|Biomass|w/ CCS","EJ/yr",1.77835332209989E-6,0.000713400632326126,4.54960357200704E-7,4.29791861239453,13.7170692458437]
["POLES","Conv","LAM","Secondary Energy|Electricity|Ocean","EJ/yr",1.80032395451999E-9,1.5770837815397e-08,2.42899698329112e-08,1.95435963850887E-8,2.11865732603101e-08]
["POLES","Conv","LAM","Secondary Energy|Liquids|Other","EJ/yr",0,0,0,0,0]
["POLES","Conv","LAM","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",6.07657674178697e-10,0,0.315030515193939,0.639714524149895,0.424315359443426]
["POLES","Conv","MAF","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,11.3170068359375,16.428380859375,16.918994140625]
["POLES","Conv","MAF","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",24.611642578125,10.4955458984375,15.67921875,8.2273525390625,16.48373828125]
["POLES","Conv","MAF","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",561.935125,639.991,379.8779375,195.8758125,165.821828125]
["POLES","Conv","MAF","Primary Energy|Biomass|Hydrogen","EJ/yr",7.35382153425898e-05,0.0672357448294503,0.106968545460728,0.938194387709263,1.10671695734514]
["POLES","Conv","MAF","Primary Energy|Gas|Electricity","EJ/yr",8.970883218375,14.36027688465,15.13432018737,18.96494007486,22.51281007653]
["POLES","Conv","MAF","Secondary Energy|Gases|Coal","EJ/yr",0,0.0352763019777832,0.0412395736882324,0.0318450374318848,0.0367803454812012]
["POLES","Conv","MAF","Water Consumption|Electricity|Fossil","km3/yr",1.38489878177643,1.50944221019745,0.937250077724457,1.11144387722015,1.29321360588074]
["POLES","Conv","MAF","Water Consumption|Electricity|Solar|PV","km3/yr",1.85690041689668e-05,1.4586882898584E-3,0.0143327740952373,0.0359204523265362,0.0625278875231743]
["POLES","Conv","OECD90","Capacity|Electricity|Coal|w/ CCS","GW",6.79999988642521e-06,7.99999956507236e-06,63.2390697250366,700.082506965637,1008.79065740967]
["POLES","Conv","OECD90","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",7489.81708349609,5859.22926513672,1504.86156091309,474.337565979004,-1451.65066333008]
["POLES","Conv","OECD90","Final Energy|Other","EJ/yr",0,0,0,0,0]
["POLES","Conv","OECD90","Primary Energy|Coal|w/o CCS","EJ/yr",70.3513246786325,42.358575599026,6.85326999151868,4.01342067920874,1.11301059219159]
["POLES","Conv","OECD90","Secondary Energy|Electricity|Wind","EJ/yr",1.26621574480825,5.29979766963237,15.9491974990451,26.0270281969515,30.7446845503956]
["POLES","Conv","OECD90","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",3.66865539757325e-06,0.148755699378273,1.90459816864838,12.4092883515883,4.30840250883105]
["POLES","Conv","OECD90","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.603929184420849,0.722052037483081,0.327941261319211,0.322195445012772,0.000566038404940628]
["POLES","Conv","PAC","Capacity Additions|Electricity|Wind","GW/yr",0.219,2.98092431640625,7.83929736328125,10.6526416015625,12.00983203125]
["POLES","Conv","PAC","Emissions|CO2|Energy|Supply|Electricity|Oil|w/ CCS","MtCO2/yr",0,0,0,0,0]
["POLES","Conv","PAC","Final Energy|Heat","EJ/yr",0.0463820164101562,0.0765930084609375,0.173297008160156,0.312026932810547,0.373742634023437]
["POLES","Conv","PAC","Primary Energy|Non-Biomass Renewables","EJ/yr",0.359234501414619,0.685573581137292,1.48395967227903,2.44203846075476,3.34086767025216]
["POLES","Conv","PAC","Secondary Energy|Electricity|Other","EJ/yr",0,0,0,0,0]
["POLES","Conv","PAC","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",1.77505952829961E-10,0.0047703157649231,0.0120275578927002,0.00849156712756348,0.00568807278936768]
["POLES","Conv","PAC","Water Withdrawal|Electricity|Coal","km3/yr",0.996770977973938,0.486041784286499,0.0865061432123184,0.0440307073295116,0.0396355353295803]
["POLES","Conv","REF","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","Conv","REF","Capacity|Electricity|Solar|CSP","GW",0.00102284084178973,0.044779509305954,3.24556074523926,7.98744650268555,12.3103197631836]
["POLES","Conv","REF","Emissions|CO2|Secondary Energy|Electricity","MtCO2/yr",1785.1233125,1343.38990625,254.231203125,-410.398234375,-953.31234375]
["POLES","Conv","REF","Primary Energy|Gas|w/ CCS","EJ/yr",1.34786457258597E-8,0,2.77834199920312,5.27211619748438,3.14370800760938]
["POLES","Conv","REF","Secondary Energy","EJ/yr",144.71337824958,145.529303770401,113.964944484331,112.0412572361,108.829600364176]
["POLES","Conv","REF","Secondary Energy|Hydrogen|Biomass","EJ/yr",4.00348461468704e-07,0.0230809277422485,0.0379367189934082,0.0272035579537354,0.0193294160551758]
["POLES","Conv","REF","Water Consumption|Electricity|Ocean","km3/yr",0,0,0,0,0]
["POLES","Conv","REF","Water Withdrawal|Electricity|Hydro","km3/yr",34.0782604217529,39.0068836212158,46.8256988525391,45.6201992034912,47.4198627471924]
["POLES","Conv","RER","Capacity|Electricity|Gas|w/o CCS","GW",2.92433319609376,10.7398482994792,11.873853515625,15.0787287597656,16.561779296875]
["POLES","Conv","RER","Final Energy|Solar","EJ/yr",1.85998027807617E-3,0.0107602651010742,0.0408063252392578,0.0540552984697266,0.0591087486928711]
["POLES","Conv","RER","Primary Energy|Fossil|w/o CCS","EJ/yr",1.44251182279269,1.44886133747238,0.831784849300415,0.577370064339844,0.51398515580658]
["POLES","Conv","RER","Primary Energy|Solar","EJ/yr",0.00231703885217285,0.0177022728632813,0.0566674129379883,0.0832087657617187,0.103790342689453]
["POLES","Conv","RER","Secondary Energy|Hydrogen|Other","EJ/yr",3.98681867127822E-6,0.000954707593927643,0.00638792347507033,0.0176880166768261,0.0354621365108412]
["POLES","Conv","RER","Water Consumption|Electricity|Solar","km3/yr",1.2718003745249E-5,1.9961636280641E-4,0.000527808908373117,0.00105848687235266,1.58829696010798E-3]
["POLES","Conv","RER","Water Withdrawal|Electricity|Gas","km3/yr",0.0659391731023788,0.0620035044848919,0.026481730863452,0.0249439179897308,0.00509996898472309]
["POLES","Conv","Russia","Capacity|Electricity|Biomass|w/o CCS","GW",1.49999996210681e-06,1.0259730268842,7.0862210737592,42.8554375,98.9448828125]
["POLES","Conv","Russia","Final Energy|Liquids","EJ/yr",4.329606547994,5.2878224727334,4.12553562683203,3.01001845454297,2.79783355665234]
["POLES","Conv","Russia","Price|Primary Energy|Coal","US$2010/GJ",3.32870188421787,3.89898281629509,4.90607463244074,5.84106254249632,6.46306679972471]
["POLES","Conv","Russia","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["POLES","Conv","Russia","Secondary Energy|Hydrogen|Gas","EJ/yr",1.42907185378717E-8,0.0323884679216309,0.0698834928032227,0.198818416230469,0.312333256107422]
["POLES","Conv","Russia","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",1.71819905525616e-10,0,0,0.474386215209961,1.04974687099457]
["POLES","Conv","Russia","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","Conv","US","Capacity|Electricity|Storage Reservoir","GWh",22.311,56.4823359375,93.20496875,364.22846875,510.35971875]
["POLES","Conv","US","Capacity|Electricity|Wind","GW",40.298,178.176609375,555.821375,839.4291875,990.740625]
["POLES","Conv","US","Policy Cost|Area under MAC Curve","billion US$2010/yr",0,8.5536003112793,742.559997558594,2872.583984375,3898.52514648438]
["POLES","Conv","US","Primary Energy|Wind","EJ/yr",0.324637357710937,1.4775891013125,4.753211238,7.283306253375,8.714516731875]
["POLES","Conv","US","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",3.60064790903998e-10,0,0,0.639469740088125,2.6212575664485]
["POLES","Conv","US","Secondary Energy|Solids","EJ/yr",24.3617001235313,17.3470408734375,8.34038788190625,7.45928089185938,8.30347715123438]
["POLES","Conv","US","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",2.45693182945251,1.63640856742859,2.34364032745361,1.6324679851532,0.943609237670898]
["POLES","Conv","US","Water Withdrawal|Electricity|Oil","km3/yr",1.61760950088501,1.60750925540924,0.489651530981064,1.10421958379447E-3,1.22397438641267e-20]
["POLES","Conv","USA","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",2336.7225,1734.28075,400.866875,-99.1566640625,-563.43775]
["POLES","Conv","USA","Final Energy|Solids|Coal","EJ/yr",1.27954021401562,1.09715143064062,0.355579404292969,0.179022211839844,0.135491328544922]
["POLES","Conv","USA","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",1.50106997070907e-09,5.38580356934108e-07,3.56792231802163e-07,2.37207125664489E-7,1.57703031814058e-07]
["POLES","Conv","USA","Secondary Energy|Electricity|Hydro","EJ/yr",1.030984343784,1.22159015915625,1.2965926696785,1.249720559217,1.233542847753]
["POLES","Conv","USA","Secondary Energy|Liquids|Coal","EJ/yr",0.083736,0,0,0,0]
["POLES","Conv","USA","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",4.00300792513519e-10,0,0.526008188724518,0.952957034111023,0.633666813373566]
["POLES","Conv","USA","Water Withdrawal|Electricity|Hydro","km3/yr",19.5102195739746,26.0904884338379,24.8948554992676,24.2443695068359,23.7708568572998]
["POLES","Conv","World","Emissions|CO2","Mt CO2/yr",34649.08075,32705.8,13557.976375,5528.357875,-2043.648296875]
["POLES","Conv","World","Emissions|CO2|Fossil Fuels and Industry|Energy Demand","Mt CO2/yr",15850.659375,16201.38265625,8821.85034375,4845.52965625,2804.1249765625]
["POLES","Conv","World","Primary Energy|Biomass","EJ/yr",51.9160530915,69.058523646,111.297672999,141.903662481,172.765088631]
["POLES","Conv","World","Secondary Energy|Electricity|Gas","EJ/yr",17.163149410908,25.670807313732,25.643996888724,44.740870707384,37.260265240728]
["POLES","Conv","World","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",1.292210906103,8.639666660124,26.13133379358,44.786368495512,60.119144698536]
["POLES","Conv","World","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",15.7213726043701,13.7841453552246,1.81755042076111,0.591114699840546,0.0663040354847908]
["POLES","NewRE","ASIA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","NewRE","ASIA","Capacity|Electricity|Wind|Onshore","GW",90.19138671875,1734.821828125,3839.429125,6290.5259375,8815.8420625]
["POLES","NewRE","ASIA","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",207.58076953125,398.20696875,439.96912890625,292.299905273438,201.963608703613]
["POLES","NewRE","ASIA","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",2.05751305345404E-8,0,0,0,0]
["POLES","NewRE","ASIA","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",5.76103654967132e-09,0,0,0,0]
["POLES","NewRE","ASIA","Secondary Energy|Electricity|Solar","EJ/yr",0.011167021774927,0.90991019185875,7.34436296616937,16.527385694034,26.9646693419835]
["POLES","NewRE","ASIA","Water Consumption|Electricity|Biomass","km3/yr",0.02912711747922,0.78161646425724,2.6106792986393,4.82101809978485,6.29421043395996]
["POLES","NewRE","ASIA","Water Withdrawal|Electricity|Once Through","km3/yr",219.401481628418,191.005300521851,68.0955419540405,34.980188369751,17.3183914422989]
["POLES","NewRE","Brazil","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",1.30050354003906,0.379884704589844,8.03801469828613e-16,0,0.0365743980407715]
["POLES","NewRE","Brazil","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",12.3057244323154,11.8010361328125,1.65609655761719,0.113207992553711,3.5176682472229E-3]
["POLES","NewRE","Brazil","Primary Energy|Biomass|w/ CCS","EJ/yr",3.95259057814255E-8,0.000315298810066223,0,0,0]
["POLES","NewRE","Brazil","Primary Energy|Gas|w/o CCS","EJ/yr",0.893993665313686,1.45839867454687,0.657232333945312,0.278488559144531,0.157116293648437]
["POLES","NewRE","Brazil","Secondary Energy|Electricity|Oil","EJ/yr",0.05784441012,0.0362752029708047,0.000947339631070312,4.24775815318844e-12,8.598948763749e-08]
["POLES","NewRE","Brazil","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",1.21531534835739E-10,0,0,0,0]
["POLES","NewRE","Brazil","Water Withdrawal|Electricity|Ocean","km3/yr",0,0,0,0,0]
["POLES","NewRE","China","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",1.18,8.7646552734375,0.171415161132812,0.148082885742188,1.54328967285156]
["POLES","NewRE","China","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",462.5799375,757.4183125,551.4536875,323.01059375,266.6964375]
["POLES","NewRE","China","Primary Energy|Biomass|Hydrogen","EJ/yr",5.21807398732219e-05,0.26197789027274,0.958745585804966,2.97903348858817,10.0554144297991]
["POLES","NewRE","China","Primary Energy|Gas|Electricity","EJ/yr",0.82847309832,5.6793992328825,6.91409031228,2.92962242463375,1.49234276085375]
["POLES","NewRE","China","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",3.60064790903998e-10,0,0,0,0]
["POLES","NewRE","China","Water Consumption|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","NewRE","China","Water Consumption|Electricity|Solar|CSP","km3/yr",8.64033378178419e-09,5.56276609131601e-06,0.00656889006495476,0.112409591674805,0.271642237901688]
["POLES","NewRE","CN","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","NewRE","CN","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",498.026,446.4309375,116.4718046875,48.74483203125,27.233056640625]
["POLES","NewRE","CN","Final Energy|Other","EJ/yr",0,0,0,0,0]
["POLES","NewRE","CN","Primary Energy|Coal|w/o CCS","EJ/yr",66.4439966409149,72.8112623895,18.7572879135,5.7550516385625,3.179005839]
["POLES","NewRE","CN","Primary Energy|Oil|w/o CCS","EJ/yr",18.211602643875,26.61397250175,19.7447865615,11.263082077125,8.40562902]
["POLES","NewRE","CN","Secondary Energy|Electricity|Wind|Offshore","EJ/yr",0.00115189089679687,0.339971524486312,0.746505528062625,1.16970954732675,1.150697788326]
["POLES","NewRE","CN","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.0311878379434347,0.250696778297424,0.442025363445282,0.226941749453545,0.0876177251338959]
["POLES","NewRE","CN","Water Withdrawal|Electricity|Fossil","km3/yr",80.3556671142578,76.2792739868164,16.9272613525391,2.55330944061279,0.395914733409882]
["POLES","NewRE","EIT","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0,0.193975204467773,0.449182006835938,0.832433471679688,0.974255798339844]
["POLES","NewRE","EIT","Final Energy|Heat","EJ/yr",4.7995937859375,4.41996845259375,3.331175085,3.16792226728125,3.0429014754375]
["POLES","NewRE","EIT","Policy Cost|Other","billion US$2010/yr",0,0,0,0,0]
["POLES","NewRE","EIT","Primary Energy|Nuclear","EJ/yr",0.613604430834629,0.638358887989292,0.46821423191318,0.132692221429217,0.0790335218276022]
["POLES","NewRE","EIT","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",3.00991813009023e-09,0,0,0,0]
["POLES","NewRE","EIT","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",2.86274909973145,3.4623920917511,4.69306945800781,5.25083255767822,4.72505378723145]
["POLES","NewRE","EIT","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",9.0500522631487e-09,0,0,0,0]
["POLES","NewRE","EU","Capacity|Electricity|Solar|CSP","GW",0.639033325195313,3.64350738525391,13.833376953125,28.7610986328125,39.5088374023438]
["POLES","NewRE","EU","Emissions|CO2|Secondary Energy|Electricity","MtCO2/yr",1230.333625,788.5315625,328.53365625,129.249734375,103.508484375]
["POLES","NewRE","EU","Final Energy|Transportation","EJ/yr",15.0329765607187,14.3563391447344,9.95579597221875,6.60095671746094,6.30784539133594]
["POLES","NewRE","EU","Primary Energy|Gas|w/ CCS","EJ/yr",2.0217968664947e-08,0,0,0,0]
["POLES","NewRE","EU","Secondary Energy|Hydrogen","EJ/yr",0.000272859254465103,0.133500779085937,0.3246045665625,0.606357521332031,1.23030320069531]
["POLES","NewRE","EU","Secondary Energy|Liquids|Gas","EJ/yr",0,0,0,0,0]
["POLES","NewRE","EU","Water Withdrawal|Electricity","km3/yr",75.6072616577148,44.162109375,21.7474308013916,6.25971984863281,2.20780277252197]
["POLES","NewRE","IN","Capacity|Electricity|Gas|w/o CCS","GW",41.9119999,112.663710826389,134.237156138889,110.582624888889,44.1388241076389]
["POLES","NewRE","IN","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",7.04423116985709e-07,0.282432312011719,0,0,0]
["POLES","NewRE","IN","Final Energy|Solids","EJ/yr",10.6337275850945,10.6794197786739,8.24425723985834,6.36227703128897,7.47062005827585]
["POLES","NewRE","IN","Primary Energy|Solar","EJ/yr",0.0124996845003662,0.132894837914063,0.921419332171875,2.01584165610937,3.4268800995]
["POLES","NewRE","IN","Secondary Energy|Gases|Biomass","EJ/yr",0.00294166046310425,0.0869642211005859,0.192690498814453,0.240772421443359,0.287658775529297]
["POLES","NewRE","IN","Secondary Energy|Hydrogen|Solar","EJ/yr",-1.27393998446438E-8,-2.23948162713499E-3,-0.00223289893611145,0.00430233053466797,0.0245145266235352]
["POLES","NewRE","IN","Water Withdrawal|Electricity|Gas","km3/yr",2.44323706626892,3.24045181274414,1.56389617919922,0.359710842370987,0.129961460828781]
["POLES","NewRE","India","Capacity|Electricity|Biomass|w/o CCS","GW",5.26400136484375,40.6357147261029,139.798296757353,292.216781132353,436.292406132353]
["POLES","NewRE","India","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",1.77059642737731e-07,0,0,0,0]
["POLES","NewRE","India","Price|Primary Energy|Coal","US$2010/GJ",3.55990976251799,4.13341376026824,4.49584836341185,5.70870714359825,6.01172540594881]
["POLES","NewRE","India","Primary Energy|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["POLES","NewRE","India","Secondary Energy|Electricity|Fossil","EJ/yr",2.87056260828,2.62950378175012,0.916979149979719,0.204485849266219,0.0992285987780786]
["POLES","NewRE","India","Water Consumption|Electricity","km3/yr",3.21097350120544,4.68695402145386,5.36431217193604,5.48397397994995,5.50946092605591]
["POLES","NewRE","India","Water Withdrawal|Electricity|Cooling Pond","km3/yr",2.34817250088781E-8,2.7106871414162e-08,2.39549606817491e-08,1.92955660338612e-08,1.24113990196406e-08]
["POLES","NewRE","India","Water Withdrawal|Electricity|Other","km3/yr",0,0,0,0,0]
["POLES","NewRE","Japan","Capacity|Electricity|Storage Reservoir","GWh",25.374,30.68578125,48.157875,173.516390625,208.049203125]
["POLES","NewRE","Japan","Land Cover|Cropland|Energy Crops","million ha",458.019714355469,445.353507995605,427.679176330566,408.171348571777,388.444900512695]
["POLES","NewRE","Japan","Primary Energy|Hydro","EJ/yr",0.294690964060547,0.307555275041016,0.324969439640625,0.320132131945312,0.311217048685547]
["POLES","NewRE","Japan","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",3.60064790903998e-10,0,0,0,0]
["POLES","NewRE","Japan","Secondary Energy|Solids","EJ/yr",0.292966632474237,0.810978191754484,0.853816000149106,0.71372451628124,0.839259989816591]
["POLES","NewRE","Japan","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.061551533639431,0.109321892261505,0.158268705010414,0.169084548950195,0.168651014566422]
["POLES","NewRE","Japan","Water Withdrawal|Electricity|Oil","km3/yr",0.422191888093948,0.212235450744629,0.0362003073096275,0.00229851575568318,1.14020542241633E-3]
["POLES","NewRE","LA","Emissions|CO2|Energy|Supply|Electricity and Heat","Mt CO2/yr",40.1364375,47.78619921875,13.81167578125,7.178697265625,5.48072021484375]
["POLES","NewRE","LA","Final Energy|Solids|Coal","EJ/yr",0.461731057207031,0.361936307777344,0.127665518581055,0.0542905810927734,0.0283018097175293]
["POLES","NewRE","LA","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",8.19306355252463e-08,0.000695477139452525,0,0,0]
["POLES","NewRE","LA","Resource|Cumulative Extraction|Oil","EJ",23.3174767138594,91.0850967454219,159.7015242405,195.338409564094,211.688628350168]
["POLES","NewRE","LA","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",1.45953488678307,1.98969330045681,2.91794228352422,4.29642090408375,5.66168462607712]
["POLES","NewRE","LA","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",4.58960786042795e-10,0,0,0,0]
["POLES","NewRE","LA","Water Withdrawal|Electricity|Hydro","km3/yr",27.5248165130615,35.6545143127441,43.5040664672852,45.940299987793,46.2771644592285]
["POLES","NewRE","LAM","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","NewRE","LAM","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0.000350863682106137,0.168977233886719,0,0,0]
["POLES","NewRE","LAM","Final Energy|Solids","EJ/yr",7.05813567830849,8.70676185525732,11.9581766651272,14.6674068853447,17.1071260458091]
["POLES","NewRE","LAM","Primary Energy|Fossil","EJ/yr",30.0342097769414,36.8450175375,18.5092068070898,8.00813114105273,5.81327807741895]
["POLES","NewRE","LAM","Secondary Energy|Electricity|Gas","EJ/yr",1.27901149313625,2.23577238847894,1.16337224509889,0.376258742510062,0.241159387987055]
["POLES","NewRE","LAM","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",1.68714625603528e-09,0,0,0,0]
["POLES","NewRE","LAM","Water Consumption|Electricity|Once Through","km3/yr",0.0628256192430854,0.0913056675344706,0.0842032227665186,0.0717355962842703,0.0540286609902978]
["POLES","NewRE","LAM","Water Withdrawal|Electricity|Solar|PV","km3/yr",4.88583083324556e-06,1.44015037221834E-3,0.0191666139289737,0.0532502671703696,0.0914201941341162]
["POLES","NewRE","MAF","Emissions|CO2|Energy|Supply|Electricity|Oil|w/o CCS","MtCO2/yr",336.34790625,323.9195,80.9977734375,19.415998046875,13.26365625]
["POLES","NewRE","MAF","Price|Carbon","US$2010/tCO2",3.08181834220886,81.1909103393555,1076.263671875,3379.71801757812,4629.27294921875]
["POLES","NewRE","MAF","Primary Energy|Coal|Hydrogen","EJ/yr",4.77236345912729e-05,0.00499863580414908,0,0,0]
["POLES","NewRE","MAF","Secondary Energy|Electricity|Solar","EJ/yr",0.00709706444872851,0.127161131759437,1.2073771637775,2.7074854346715,4.063608517896]
["POLES","NewRE","MAF","Water Consumption|Electricity|Biomass","km3/yr",0.0019933998119086,0.0174371264874935,0.150396600365639,0.335519999265671,0.546524107456207]
["POLES","NewRE","MAF","Water Consumption|Electricity|Nuclear","km3/yr",0.0281499866396189,0.0357726514339447,0.0343531295657158,0.00320666236802936,0.0019252352649346]
["POLES","NewRE","OECD90","Capacity Additions|Electricity|Oil|w/o CCS","GW/yr",22.4394225196838,10.8729232559204,2.03550549316407,1.0441337890625,27.854483109355]
["POLES","NewRE","OECD90","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",5543.86368897204,2880.69070861816,507.902323532104,245.696312198639,209.623879959106]
["POLES","NewRE","OECD90","Final Energy","EJ/yr",237.271471010169,233.007746251983,173.442440915486,159.057996973688,176.094816126834]
["POLES","NewRE","OECD90","Primary Energy|Biomass|w/o CCS","EJ/yr",17.5866531147533,27.5151731165212,54.5085535804392,69.5759208774647,85.7573671148319]
["POLES","NewRE","OECD90","Secondary Energy|Electricity|Oil","EJ/yr",1.6073591975865,1.65837920092107,0.928835118411183,0.789406337282904,0.865289854111656]
["POLES","NewRE","OECD90","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",3.79413508545319e-06,3.12367671544647E-3,0.00134421284783936,0.000799441082061768,0.000576526052581787]
["POLES","NewRE","OECD90","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",1.96024995949119,2.88791301194578,1.54100935428869,0.8721284167259,0.836172488459852]
["POLES","NewRE","OECD90","Water Withdrawal|Electricity|Once Through","km3/yr",303.569759845734,154.411038100719,54.5757998526096,16.1353727541864,4.24055697256699]
["POLES","NewRE","PAC","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",431.21328125,354.05271875,126.79859375,27.992015625,14.16605078125]
["POLES","NewRE","PAC","Emissions|CO2|Fossil Fuels and Industry|Energy Demand|Transportation","Mt CO2/yr",223.7573125,208.388296875,98.7400078125,43.09143359375,31.027853515625]
["POLES","NewRE","PAC","Primary Energy|Gas","EJ/yr",3.60228183328125,3.91989411675,2.370999232125,0.720978980695313,0.301718450619141]
["POLES","NewRE","PAC","Secondary Energy|Electricity|Geothermal","EJ/yr",0.009476905536,0.0309676966197187,0.0433671503853516,0.0428754650229141,0.0621808631973281]
["POLES","NewRE","PAC","Secondary Energy|Gases|Coal","EJ/yr",0,1.5140019548893e-05,3.66248448050022e-05,3.49024268939495e-05,3.32009264924526e-05]
["POLES","NewRE","PAC","Water Consumption|Electricity|Solar|CSP","km3/yr",8.64033378178419e-09,9.69998563959962e-06,0.0055811027996242,0.0121353399008512,0.0118103874847293]
["POLES","NewRE","REF","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","NewRE","REF","Capacity|Electricity|Coal|w/ CCS","GW",3.59999980719294e-06,4.23529383260757e-06,4.23529383260757e-06,4.23529383260757e-06,4.23529383260757e-06]
["POLES","NewRE","REF","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",5007.715875,4470.573625,1756.890875,783.8371875,470.021953125]
["POLES","NewRE","REF","Primary Energy|Coal|w/o CCS","EJ/yr",17.3970834518537,12.1292555183256,4.35548485148676,2.95879550333835,2.59351066177679]
["POLES","NewRE","REF","Primary Energy|Oil|w/o CCS","EJ/yr",17.2417310780625,20.0009918998125,13.3333843519687,8.82943785,7.42134799321875]
["POLES","NewRE","REF","Secondary Energy|Electricity|Wind|Offshore","EJ/yr",2.36562570793904E-7,0.0382725574006025,0.298499352245016,0.493045479089437,0.603738161123906]
["POLES","NewRE","REF","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.0831366423517466,0.358271025121212,0.159374583512545,0.0696442648768425,0.0291236881166697]
["POLES","NewRE","REF","Water Withdrawal|Electricity|Fossil","km3/yr",65.3392200469971,43.8979892730713,10.2037627696991,2.82129573822021,0.604155704379082]
["POLES","NewRE","RER","Capacity Additions|Electricity|Wind|Offshore","GW/yr",0,0.0270317440032959,0.014207818031311,0.068081428527832,0.0648965072631836]
["POLES","NewRE","RER","Final Energy|Heat","EJ/yr",0.0711260146318359,0.0707730089238281,0.107537109600586,0.118847582165039,0.113263386556641]
["POLES","NewRE","RER","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",7.71567390367023e-09,0,0,0,0]
["POLES","NewRE","RER","Primary Energy|Ocean","EJ/yr",1.08019440012868e-09,9.46250324975699e-09,9.46250324975699e-09,9.46250324975699e-09,9.46250324975699e-09]
["POLES","NewRE","RER","Secondary Energy|Hydrogen|Coal","EJ/yr",1.25047385432571E-6,0.00049289905721283,6.5033330786705e-05,0.000267347533121109,0]
["POLES","NewRE","RER","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",8.5355330662569e-09,3.39929744052887E-4,6.5033330786705e-05,0.000267347533121109,0]
["POLES","NewRE","RER","Water Withdrawal|Electricity|Coal","km3/yr",0.00282677263021469,0.0428793057799339,0.0037595562171191,0.00046195340109989,1.43441691761836E-4]
["POLES","NewRE","Russia","Capacity Additions|Electricity|Oil|w/ CCS","GW/yr",0,0,0,0,0]
["POLES","NewRE","Russia","Capacity|Electricity|Solar|CSP","GW",1.20495178271085e-06,0.00340042757987976,1.99567495727539,5.02901403808594,8.35313525390625]
["POLES","NewRE","Russia","Final Energy|Transportation","EJ/yr",2.81713278297656,3.38101055722266,2.53935281111133,1.97024544154688,1.94669716519336]
["POLES","NewRE","Russia","Primary Energy|Gas|w/ CCS","EJ/yr",7.48813693746342e-10,0,0,0,0]
["POLES","NewRE","Russia","Secondary Energy","EJ/yr",59.3334516383853,59.9219161196988,43.1825859369989,32.4736303525337,28.5366006075398]
["POLES","NewRE","Russia","Secondary Energy|Liquids|Gas","EJ/yr",0.272652675117187,0.0131399309069824,0,0,0]
["POLES","NewRE","Russia","Water Withdrawal|Electricity","km3/yr",31.4282875061035,24.1323051452637,10.2474365234375,4.38234806060791,3.48702025413513]
["POLES","NewRE","Russia","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",11.4745712280273,13.8777303695679,18.7762031555176,20.967399597168,18.8173046112061]
["POLES","NewRE","US","Capacity|Electricity|Hydro","GW",101.0236015625,124.5572265625,152.811890625,188.0916875,196.63159375]
["POLES","NewRE","US","Final Energy|Solids","EJ/yr",4.07130462791016,4.32281457632813,7.70187896662501,9.19980679819922,10.5105234214687]
["POLES","NewRE","US","Primary Energy|Biomass|Electricity","EJ/yr",0.969975992828571,1.58912278749844,5.24733484135982,11.2785886198768,16.2927521676]
["POLES","NewRE","US","Primary Energy|Wind","EJ/yr",0.324637357710937,2.38174409826562,7.4869646349375,10.676909143125,12.165771857625]
["POLES","NewRE","US","Secondary Energy|Hydrogen|Solar","EJ/yr",-1.18597423236345e-08,-0.126321913223161,-0.0131595863185959,7.15182690344238E-3,0.0228003458291016]
["POLES","NewRE","US","Water Consumption|Electricity|Solar|CSP","km3/yr",0.00308349658735096,0.0376441031694412,0.127948746085167,0.211331278085709,0.24571019411087]
["POLES","NewRE","US","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",6.69746147430317E-10,0,0,0,0]
["POLES","NewRE","USA","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",4.45838406449184e-07,0,0,0,0]
["POLES","NewRE","USA","Final Energy|Liquids","EJ/yr",32.3668292594766,29.3766596305313,15.401979851625,8.18281578311719,6.62648237775]
["POLES","NewRE","USA","Price|Primary Energy|Coal","US$2010/GJ",2.26763857781084,3.14699805066455,4.61189943112969,5.23589856966047,5.41854741728908]
["POLES","NewRE","USA","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",7.18039063699187,3.4856511792975,0.60203340901125,0.142473970386844,0.0670438125894375]
["POLES","NewRE","USA","Secondary Energy|Hydrogen|Gas","EJ/yr",1.18597423236351E-8,0.126335258964844,0.0143705930317383,0,0]
["POLES","NewRE","USA","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",1.23005466923232E-10,0,0,0,0]
["POLES","NewRE","USA","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0,0,0,0]
["POLES","NewRE","World","Capacity|Electricity|Storage Reservoir","GWh",102.3060078125,480.419125,1380.66425,3867.717,6562.305]
["POLES","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",2.07522441633046e-06,0,0,0,0]
["POLES","NewRE","World","Policy Cost|Area under MAC Curve","billion US$2010/yr",0,113.180130004883,8377.63671875,31803.1484375,42552.2734375]
["POLES","NewRE","World","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",2.05236922693849e-08,0,0,0,0]
["POLES","NewRE","World","Secondary Energy|Electricity|Oil|w/ CCS","EJ/yr",0,0,0,0,0]
["POLES","NewRE","World","Secondary Energy|Solids|Biomass","EJ/yr",46.7579959565625,60.8066751358125,91.603457748,113.6819142945,136.75147275375]
["POLES","NewRE","World","Water Withdrawal|Electricity|Oil","km3/yr",17.1679668426514,19.8035182952881,8.94865798950195,2.22636985778809,0.93540620803833]
["REMIND","Base","AME","Capacity|Electricity|Wind|Onshore","GW",1.02,4.693,24.127,90.73,254.32]
["REMIND","Base","AME","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",1885.3,4118,4174.1,4136,4250]
["REMIND","Base","AME","Primary Energy|Fossil|w/o CCS","EJ/yr",49.755,81.727,88.26,106.16,133.35]
["REMIND","Base","AME","Secondary Energy|Electricity|Oil","EJ/yr",0.9582,0.4563,0.101,0,0]
["REMIND","Base","AME","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0151,7.6E-3,0.0208,0.1769,0.714]
["REMIND","Base","AME","Water Consumption|Electricity|Geothermal","km3/yr",0.0198,0.0187,0.0231,0.1125,0.3235]
["REMIND","Base","AS","Capacity|Electricity|Gas|w/o CCS","GW",165.6,191.3,200.9,196.2,166.4]
["REMIND","Base","AS","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",0,0,0,0,0]
["REMIND","Base","AS","Primary Energy","EJ/yr",44.57,53.03,63.17,74.23,83.94]
["REMIND","Base","AS","Secondary Energy|Electricity|Gas","EJ/yr",2.188,2.795,2.822,2.067,1.004]
["REMIND","Base","AS","Secondary Energy|Gases|Natural Gas","EJ/yr",4.104,4.813,4.22,3.831,4.45]
["REMIND","Base","AS","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.5829,0.7173,0.673,0.4106,0.1121]
["REMIND","Base","ASIA","Capacity Additions|Electricity|Wind|Onshore","GW/yr",16.4389,26.678,38.45,53.59,70.39]
["REMIND","Base","ASIA","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["REMIND","Base","ASIA","Population","million",3681,4015,4274,4435,4500]
["REMIND","Base","ASIA","Primary Energy|Biomass|Traditional","EJ/yr",24.189,22.627,18.519,13.275,7.9]
["REMIND","Base","ASIA","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","ASIA","Water Consumption|Electricity|Dry Cooling","km3/yr",0.0173,0.0196,0.0394,0.0548,0.061]
["REMIND","Base","ASIA","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","Base","China","Capacity Additions|Electricity|Hydro","GW/yr",2.032,0.0984,0.8043,1.313,4.63]
["REMIND","Base","China","Final Energy|Transportation","EJ/yr",7.127,13.68,21.45,25.08,28.01]
["REMIND","Base","China","Primary Energy|Fossil|w/o CCS","EJ/yr",83.77,119.6,137.3,133.7,119.5]
["REMIND","Base","China","Secondary Energy","EJ/yr",71.24,100.6,117,119.4,114.5]
["REMIND","Base","China","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","Base","China","Water Withdrawal|Electricity|Cooling Pond","km3/yr",10.45,12.29,10.4,7.708,3.47]
["REMIND","Base","China","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","Base","CN","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",0,0,0,0,0]
["REMIND","Base","CN","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","CN","Primary Energy|Oil","EJ/yr",16.92,26.37,36.65,37.83,36.31]
["REMIND","Base","CN","Secondary Energy|Gases|Natural Gas","EJ/yr",3.477,5.042,4.857,5.666,6.572]
["REMIND","Base","CN","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.0428,0.2434,0.3231,0.4828,0.4878]
["REMIND","Base","CN","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",1.68,1.694,1.034,0.3288,0]
["REMIND","Base","EIT","Consumption","billion US$2010/yr",720.031,961.5183,1237.3456,1515.3883,1822.232]
["REMIND","Base","EIT","Primary Energy|Biomass|Other Carrier","EJ/yr",0.4259,0.4683,0.5452,0.7071,0.9594]
["REMIND","Base","EIT","Secondary Energy|Electricity|Coal","EJ/yr",0.3856,0.2723,0.1728,0.0845,0.0122]
["REMIND","Base","EIT","Secondary Energy|Electricity|Solar|PV","EJ/yr",0,0.0103,0.01,0.0078,0.0011]
["REMIND","Base","EIT","Water Consumption|Electricity|Solar|PV","km3/yr",0,0.0003,0.0003,0.0002,0]
["REMIND","Base","EU","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",1.379,6.129,6.411,3.886,6.697]
["REMIND","Base","EU","Capacity|Electricity|Solar|PV","GW",28.6,138,190.6,271.8,419.6]
["REMIND","Base","EU","Final Energy|Transportation","EJ/yr",17.18,16.62,18.8,19.9,19.82]
["REMIND","Base","EU","Resource|Cumulative Extraction|Oil","EJ",5.145,3.997,4.166,4.489,4.871]
["REMIND","Base","EU","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",2.206,3.582,4.394,5.221,6.846]
["REMIND","Base","EU","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","Base","EU","Water Withdrawal|Electricity|Wet Tower","km3/yr",6.188,5.228,4.759,4.579,4.461]
["REMIND","Base","IN","Capacity|Electricity|Coal|w/o CCS","GW",99.96,209.2,368.4,528.6,595.4]
["REMIND","Base","IN","Final Energy|Hydrogen","EJ/yr",0.0347,0.0352,0.0739,0.1593,0.2615]
["REMIND","Base","IN","Primary Energy|Nuclear","EJ/yr",0.0782,0.4315,1.176,2.185,4.129]
["REMIND","Base","IN","Secondary Energy|Gases|Coal","EJ/yr",0,0,0.0029,0.0676,0.4921]
["REMIND","Base","IN","Secondary Energy|Liquids|Coal","EJ/yr",0,0,0.0005,0.0164,0.1447]
["REMIND","Base","IN","Water Withdrawal|Electricity|Oil","km3/yr",1.556,1.299,0.834,0.3504,0.0516]
["REMIND","Base","India","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["REMIND","Base","India","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",994.6,1728,2589,3361,3672]
["REMIND","Base","India","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","India","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0.0002,3.3E-3,0.0032,0.0024,0.0097]
["REMIND","Base","India","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","Base","India","Water Consumption|Electricity|Solar|PV","km3/yr",1E-4,0.0017,0.0098,0.0376,0.097]
["REMIND","Base","Japan","Capacity|Electricity|Solar|CSP","GW",0,1E-3,2E-3,0.0027,0.0029]
["REMIND","Base","Japan","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",122.6,112.2,63.02,27.63,19.67]
["REMIND","Base","Japan","Primary Energy|Biomass|Gases","EJ/yr",0.1529,0.1496,0.1352,0.0959,0.0246]
["REMIND","Base","Japan","Primary Energy|Fossil","EJ/yr",18.1,18.99,17.38,15.84,14.54]
["REMIND","Base","Japan","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",0.3332,0.4216,0.5648,0.6889,0.774]
["REMIND","Base","Japan","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","Base","Japan","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["REMIND","Base","LA","Capacity|Electricity|Coal|w/o CCS","GW",9.425,8.696,7.388,6.962,8.608]
["REMIND","Base","LA","Price|Primary Energy|Gas","US$2010/GJ",2.9743,3.6489,4.5606,5.5586,6.6885]
["REMIND","Base","LA","Primary Energy|Coal","EJ/yr",1.223,1.748,1.758,2.067,3.147]
["REMIND","Base","LA","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","LA","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",1.099,1.569,1.845,1.835,1.618]
["REMIND","Base","LA","Water Withdrawal|Electricity|Oil","km3/yr",3.285,1.646,0.3836,1E-4,1E-4]
["REMIND","Base","LAM","Capacity Additions|Electricity|Solar|PV","GW/yr",0.1517,0.9522,3.14,10.12,20.95]
["REMIND","Base","LAM","Policy Cost|Consumption Loss","billion US$2010/yr",0,0,0,0,0]
["REMIND","Base","LAM","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","LAM","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","LAM","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","Base","LAM","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","Base","MAF","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0.0478,0.2986,1.126,4.148,9.435]
["REMIND","Base","MAF","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",474.61,566.94,865.7,1412.3,1842.2]
["REMIND","Base","MAF","Primary Energy|Coal|w/o CCS","EJ/yr",1.938,2.4468,5.143,11.1422,20.188]
["REMIND","Base","MAF","Resource|Cumulative Extraction|Coal","EJ",12.443,71.92,162.84,249.24,334]
["REMIND","Base","MAF","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0,0,0,0]
["REMIND","Base","MAF","Water Consumption|Electricity|Nuclear","km3/yr",0.0153,0.1078,0.1402,0.1312,0.1053]
["REMIND","Base","OECD90","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["REMIND","Base","OECD90","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0,0,0,0]
["REMIND","Base","OECD90","Primary Energy|Biomass|w/o CCS","EJ/yr",13.9912,18.2525,16.8619,16.9793,17.3521]
["REMIND","Base","OECD90","Secondary Energy|Electricity|Fossil","EJ/yr",23.493,24.57,26.875,28.901,30.486]
["REMIND","Base","OECD90","Secondary Energy|Gases","EJ/yr",34.645,34.232,29.2324,25.883,25.33]
["REMIND","Base","OECD90","Water Withdrawal|Electricity","km3/yr",283.888,232.774,151.74,88.352,43.377]
["REMIND","Base","PAC","Capacity Additions|Electricity|Solar|CSP","GW/yr",0.004,0.0002,0.0002,0.0002,0.0184]
["REMIND","Base","PAC","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0,0,0,0]
["REMIND","Base","PAC","Policy Cost|Consumption Loss","billion US$2010/yr",0,0,0,0,0]
["REMIND","Base","PAC","Secondary Energy|Electricity|Biomass","EJ/yr",0.02,0.0243,0.0253,0.0568,0.1195]
["REMIND","Base","PAC","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.526,0.2504,0.0575,0.004,0.0032]
["REMIND","Base","PAC","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","Base","REF","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["REMIND","Base","REF","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["REMIND","Base","REF","Final Energy|Solids|Biomass","EJ/yr",0.2348,0.2009,0.1497,0.095,0.0499]
["REMIND","Base","REF","Primary Energy|Wind","EJ/yr",0.0002,0.0004,0.0005,0.0005,0.008]
["REMIND","Base","REF","Secondary Energy|Hydrogen","EJ/yr",0.0359,0.034,0.0345,0.0466,0.0648]
["REMIND","Base","REF","Secondary Energy|Solids","EJ/yr",1.142,1.021,1.285,1.285,1.046]
["REMIND","Base","REF","Water Withdrawal|Electricity|Solar","km3/yr",0,0.0003,0.0003,0.0002,1E-4]
["REMIND","Base","RER","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,0,0,0,0]
["REMIND","Base","RER","Final Energy|Electricity","EJ/yr",10.02,10.63,11.62,13.35,16.03]
["REMIND","Base","RER","Primary Energy|Biomass|w/o CCS","EJ/yr",6.095,7.803,7.258,6.459,5.67]
["REMIND","Base","RER","Primary Energy|Hydro","EJ/yr",1.176,1.08,1.075,1.08,1.065]
["REMIND","Base","RER","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0.0211,0.0104,0.0026,0.0005,0]
["REMIND","Base","RER","Water Withdrawal|Electricity","km3/yr",80.21,64.06,41.58,24.97,13.41]
["REMIND","Base","RER","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.1684,0.2101,0.412,0.484,0.4946]
["REMIND","Base","Russia","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",331.5,332,360,368.5,457.9]
["REMIND","Base","Russia","Primary Energy|Biomass|Liquids","EJ/yr",0,1E-4,1E-4,1E-4,1E-4]
["REMIND","Base","Russia","Primary Energy|Gas","EJ/yr",14.94,16.79,17.26,18.32,18.1]
["REMIND","Base","Russia","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.0694,0.1322,0.1038,0,0]
["REMIND","Base","Russia","Water Consumption|Electricity|Once Through","km3/yr",0.1852,0.2269,0.1841,0.1291,0.0848]
["REMIND","Base","Russia","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",19.79,20.5,15.84,9.533,6.007]
["REMIND","Base","US","Capacity|Electricity|Nuclear","GW",117.6,97.02,68.1,46.07,28.49]
["REMIND","Base","US","Primary Energy|Biomass","EJ/yr",4.175,7.122,6.863,7.917,8.759]
["REMIND","Base","US","Primary Energy|Wind","EJ/yr",0.391,1.395,2.095,2.535,3.235]
["REMIND","Base","US","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",3.815,6.115,7.305,5.846,3.667]
["REMIND","Base","US","Water Consumption|Electricity|Hydro","km3/yr",5.112,5.699,5.808,5.808,5.808]
["REMIND","Base","US","Water Withdrawal|Electricity|Solar","km3/yr",3.3E-3,0.0253,0.036,0.0552,0.0807]
["REMIND","Base","USA","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0,0,0]
["REMIND","Base","USA","Population","million",310.4,335.8,361,383.2,402.3]
["REMIND","Base","USA","Primary Energy|Geothermal","EJ/yr",0.0953,0.0896,0.0962,0.1,0.112]
["REMIND","Base","USA","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","Base","USA","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0.0211,0.0148,0.0075,0.0006,0]
["REMIND","Base","USA","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","Base","World","Capacity Additions|Electricity|Hydro","GW/yr",14.94,12.7,11.75,11.74,19.46]
["REMIND","Base","World","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",11800,16240,19120,19840,20210]
["REMIND","Base","World","Primary Energy|Fossil|w/o CCS","EJ/yr",429.8,532.3,598.6,639.9,672.4]
["REMIND","Base","World","Secondary Energy|Electricity|Oil","EJ/yr",3.437,1.89,0.6916,0.1446,0.0326]
["REMIND","Base","World","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0909,0.0699,0.2146,0.6174,1.425]
["REMIND","Base","World","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","FullTech","AME","Capacity|Electricity|Hydro","GW",46.09,70.97,131.89,167.74,167.34]
["REMIND","FullTech","AME","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0.0029,0.0046,4.3E-3,0.0049]
["REMIND","FullTech","AME","Primary Energy|Coal|Hydrogen","EJ/yr",0.0238,0.0102,2.3E-3,0.0005,0.0002]
["REMIND","FullTech","AME","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0.0439,0.8482,4.572,8.154]
["REMIND","FullTech","AME","Secondary Energy|Gases|Other","EJ/yr",0,0.2434,0.4434,0.6686,0.9437]
["REMIND","FullTech","AME","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.1421,0.0777,0.0255,0.0025,0.0003]
["REMIND","FullTech","AS","Capacity Additions|Electricity|Wind|Onshore","GW/yr",0.3689,6.416,18.28,24.45,31.02]
["REMIND","FullTech","AS","Consumption","billion US$2010/yr",2209.9413,3295.5265,4668.0164,6115.8325,7654.483]
["REMIND","FullTech","AS","Population","million",1107,1240,1355,1440,1493]
["REMIND","FullTech","AS","Secondary Energy|Electricity|Coal","EJ/yr",1.666,0.9074,0.2395,0.0121,0.0104]
["REMIND","FullTech","AS","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.007,0.4324,1.64,3.722,6.536]
["REMIND","FullTech","AS","Water Consumption|Electricity|Dry Cooling","km3/yr",0.0173,0.018,0.0204,0.0213,0.0311]
["REMIND","FullTech","ASIA","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",17.7112,85.1539,27.184,36.498,34.194]
["REMIND","FullTech","ASIA","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",332.5315,270.7279,162.4017,85.0367,17.9227]
["REMIND","FullTech","ASIA","Final Energy|Transportation","EJ/yr",17.488,26.99,40.847,47.98,55.25]
["REMIND","FullTech","ASIA","Resource|Cumulative Extraction|Oil","EJ",15.616,16.4223,18.7741,18.5374,16.692]
["REMIND","FullTech","ASIA","Secondary Energy","EJ/yr",128.23,155.77,177.86,187.16,198.15]
["REMIND","FullTech","ASIA","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0.0036,0.1355,0.6942,0.8927]
["REMIND","FullTech","ASIA","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0.0003,0.0088,0.0228,0.0227]
["REMIND","FullTech","China","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0.0116,0.5104,2.383,3.48]
["REMIND","FullTech","China","Final Energy|Liquids","EJ/yr",13.33,23.9,33.89,32.69,30.52]
["REMIND","FullTech","China","Primary Energy|Coal|Hydrogen","EJ/yr",0.0132,0.0085,0.0158,0.0168,0.0148]
["REMIND","FullTech","China","Primary Energy|Oil|w/o CCS","EJ/yr",16.92,28.66,39.08,34.95,26.14]
["REMIND","FullTech","China","Secondary Energy|Heat","EJ/yr",2.472,2.066,1.367,0.8663,0.5611]
["REMIND","FullTech","China","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",0.0428,0.3468,0.3992,0.377,0.2929]
["REMIND","FullTech","China","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",1.68,1.387,0.7374,0.1664,0]
["REMIND","FullTech","CN","Consumption","billion US$2010/yr",4226.0281,5831.1434,7572.5106,9065.7442,10326.35]
["REMIND","FullTech","CN","Primary Energy|Biomass|Other Carrier","EJ/yr",9.18,8.187,6.893,5.644,3.809]
["REMIND","FullTech","CN","Primary Energy|Gas|w/ CCS","EJ/yr",0,6.6E-3,0.0141,0.0133,0.0103]
["REMIND","FullTech","CN","Secondary Energy|Electricity|Solar|PV","EJ/yr",5.3E-3,0.5823,3.815,9.447,14.67]
["REMIND","FullTech","CN","Water Consumption|Electricity|Solar|PV","km3/yr",1E-4,0.0158,0.0999,0.2237,0.3269]
["REMIND","FullTech","EIT","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",4.162,0.5651,1.359,2.781,1E-4]
["REMIND","FullTech","EIT","Capacity|Electricity|Solar|PV","GW",0,2.123,2.901,8.069,31.45]
["REMIND","FullTech","EIT","Primary Energy|Biomass|Gases","EJ/yr",0.7165,0.6988,0.6257,0.4303,0.1021]
["REMIND","FullTech","EIT","Resource|Cumulative Extraction|Oil","EJ",17.59,20.06,22.43,24.03,23.13]
["REMIND","FullTech","EIT","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",0.4747,0.4863,0.7311,1.311,1.993]
["REMIND","FullTech","EIT","Water Consumption|Electricity|Nuclear","km3/yr",0.3149,0.6475,0.7179,0.6333,0.4763]
["REMIND","FullTech","EIT","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","FullTech","EU","Capacity|Electricity|Gas|w/ CCS","GW",0,1E-3,2E-3,0.0024,2E-3]
["REMIND","FullTech","EU","Final Energy|Liquids","EJ/yr",25.36,27.38,30.92,30.25,27.36]
["REMIND","FullTech","EU","Primary Energy|Oil","EJ/yr",30.81,31.16,34.26,32.48,27.87]
["REMIND","FullTech","EU","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",6.227,4.204,2.622,1.092,0.5063]
["REMIND","FullTech","EU","Water Consumption|Electricity|Coal","km3/yr",1.311,0.568,0.1639,0.0312,3.3E-3]
["REMIND","FullTech","EU","Water Withdrawal|Electricity|Oil","km3/yr",2.949,1.481,0.3459,0,0]
["REMIND","FullTech","IN","Capacity Additions|Electricity|Solar|PV","GW/yr",0.1705,7.886,43.5,77.17,101.7]
["REMIND","FullTech","IN","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",994.6,1303,960.4,186.4,-336.2]
["REMIND","FullTech","IN","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,1E-4,1E-4,1E-4]
["REMIND","FullTech","IN","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0.0002,0.0048,0.0241,0.1406,0.6669]
["REMIND","FullTech","IN","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","FullTech","IN","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","FullTech","India","Capacity|Electricity|Solar|CSP","GW",0.01,0.2626,1.324,8.156,43.89]
["REMIND","FullTech","India","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",37.11,37.79,50.92,77.55,119.9]
["REMIND","FullTech","India","Primary Energy|Biomass|Gases","EJ/yr",0.1166,0.3006,0.558,0.5164,0.4086]
["REMIND","FullTech","India","Secondary Energy|Electricity|Hydro","EJ/yr",0.3898,0.3513,0.3125,0.2804,0.2844]
["REMIND","FullTech","India","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,1E-4,0.031,0.2164,0.5894]
["REMIND","FullTech","India","Water Consumption|Electricity|Nuclear","km3/yr",0.0366,0.2418,1.418,3.972,6.992]
["REMIND","FullTech","Japan","Capacity|Electricity|Coal|w/o CCS","GW",43.77,37.61,18.54,4.7,0.0791]
["REMIND","FullTech","Japan","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",416.9,338.5,178.1,59.18,24.9]
["REMIND","FullTech","Japan","Price|Primary Energy|Oil","US$2010/GJ",6.3595,7.2834,8.9727,10.4715,11.875]
["REMIND","FullTech","Japan","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,1E-4,0.0005,1.4E-3,1.5E-3]
["REMIND","FullTech","Japan","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",2.484,2.047,1.127,0.3863,0.1922]
["REMIND","FullTech","Japan","Water Consumption|Electricity|Solar|CSP","km3/yr",0,0,0,0,0]
["REMIND","FullTech","Japan","Water Withdrawal|Electricity|Biomass","km3/yr",0.0008,0.0026,0.0025,2.3E-3,1.9E-3]
["REMIND","FullTech","LA","Capacity Additions|Electricity|Solar|PV","GW/yr",0.1517,3.243,15.1,23.4,27.63]
["REMIND","FullTech","LA","Policy Cost|Consumption Loss","billion US$2010/yr",0,-77.6969,-60.4272,-31.0721,-4.0133]
["REMIND","FullTech","LA","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0.011,0.2695,2.342,8.985]
["REMIND","FullTech","LA","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0.0009,0.0293,0.2375,0.8008]
["REMIND","FullTech","LA","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","FullTech","LA","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0.052,0.477,2.08,3.543]
["REMIND","FullTech","LAM","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0.2412,0,0,0,0]
["REMIND","FullTech","LAM","Final Energy|Solids|Biomass","EJ/yr",4.408,4.344,3.727,2.814,1.751]
["REMIND","FullTech","LAM","Primary Energy|Coal|w/o CCS","EJ/yr",1.223,0.7789,0.24,0.016,0.0037]
["REMIND","FullTech","LAM","Resource|Cumulative Extraction|Coal","EJ",17.13,51.85,77.87,94.48,97.03]
["REMIND","FullTech","LAM","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0,0.0031,0.0511,0.2493]
["REMIND","FullTech","LAM","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0.0157,0.0148,0.0112,0.0092,0.0099]
["REMIND","FullTech","LAM","Water Withdrawal|Electricity|Solar|PV","km3/yr",1E-4,2.3E-3,0.0175,0.0467,0.0777]
["REMIND","FullTech","MAF","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",799.12,573.77,384.2,218.09,127.79]
["REMIND","FullTech","MAF","Primary Energy|Coal","EJ/yr",1.938,1.1332,0.3366,0.0932,0.0258]
["REMIND","FullTech","MAF","Primary Energy|Non-Biomass Renewables","EJ/yr",0.7405,1.4663,4.3,9.602,18.872]
["REMIND","FullTech","MAF","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,1E-4,2.8E-3]
["REMIND","FullTech","MAF","Water Withdrawal|Electricity","km3/yr",15.2686,12.358,10.186,9.294,11.499]
["REMIND","FullTech","OECD90","Capacity Additions|Electricity|Solar|CSP","GW/yr",0.2,0.0004,0.5904,5.0008,19.1791]
["REMIND","FullTech","OECD90","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0.0879,6.7929,48.2319,163.574]
["REMIND","FullTech","OECD90","Primary Energy|Biomass|Liquids","EJ/yr",0.185,4.3202,4.6778,7.5289,18.3887]
["REMIND","FullTech","OECD90","Secondary Energy|Electricity|Biomass","EJ/yr",0.5489,0.8199,1.0265,1.155,1.6698]
["REMIND","FullTech","OECD90","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",1.1751,0.5595,0.124,0,0]
["REMIND","FullTech","OECD90","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0.0031,0.0139,0.0191]
["REMIND","FullTech","PAC","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0.0007,0,0.0006,0]
["REMIND","FullTech","PAC","Capacity|Electricity|Nuclear","GW",75.01,89.29,116.4,138.71,148.84]
["REMIND","FullTech","PAC","Final Energy|Solids|Biomass","EJ/yr",2.7072,2.4109,1.8712,1.59,1.4622]
["REMIND","FullTech","PAC","Primary Energy|Wind","EJ/yr",0.079,0.5561,1.5115,2.5016,3.3391]
["REMIND","FullTech","PAC","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",2.338,4.0304,4.1718,2.5622,1.1238]
["REMIND","FullTech","PAC","Secondary Energy|Solids|Coal","EJ/yr",4.633,2.6932,1.939,1.3655,0.9596]
["REMIND","FullTech","PAC","Water Withdrawal|Electricity|Solar|CSP","km3/yr",1E-4,0.0026,0.0047,0.0496,0.3201]
["REMIND","FullTech","REF","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0.0065,0.0132,1.096,15.93]
["REMIND","FullTech","REF","Final Energy|Gases","EJ/yr",6.81,6.894,5.39,4.108,3.024]
["REMIND","FullTech","REF","Primary Energy|Hydro","EJ/yr",0.4728,0.4563,0.6208,1.066,1.496]
["REMIND","FullTech","REF","Secondary Energy|Gases","EJ/yr",7.612,7.803,6.179,4.77,3.557]
["REMIND","FullTech","REF","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0.0084,0.0032,0.0006,1E-4,0]
["REMIND","FullTech","REF","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","FullTech","RER","Capacity|Electricity|Wind|Onshore","GW",84,226,375.9,501.8,617.7]
["REMIND","FullTech","RER","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",1963,2075,2305,2178,1800]
["REMIND","FullTech","RER","Primary Energy|Biomass|Liquids","EJ/yr",0.0254,1.495,1.507,1.795,3.314]
["REMIND","FullTech","RER","Secondary Energy|Electricity|Oil","EJ/yr",0.2812,0.1339,0.0297,0,0]
["REMIND","FullTech","RER","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0084,0.0054,0.006,0.0109,0.0098]
["REMIND","FullTech","RER","Water Consumption|Electricity|Once Through","km3/yr",0.4816,0.3417,0.1951,0.1059,0.0589]
["REMIND","FullTech","RER","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",36.66,20.62,9.699,2.53,0.0681]
["REMIND","FullTech","Russia","Capacity|Electricity|Nuclear","GW",23.22,45.9,49,42.87,31.77]
["REMIND","FullTech","Russia","Primary Energy|Biomass","EJ/yr",1.16,1.422,2.569,4.011,3.858]
["REMIND","FullTech","Russia","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","FullTech","Russia","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",1.385,1.368,1.014,0.5674,0.1538]
["REMIND","FullTech","Russia","Water Consumption|Electricity|Geothermal","km3/yr",0.0064,0.006,0.0042,0.0046,0.0939]
["REMIND","FullTech","Russia","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0.0005,0.0005,0.0005,0.0004]
["REMIND","FullTech","US","Capacity|Electricity|Biomass|w/o CCS","GW",12.02,11.71,10.46,7.118,1.644]
["REMIND","FullTech","US","Price|Carbon","US$2010/tCO2",0,37.2201,60.6266,98.755,160.8438]
["REMIND","FullTech","US","Primary Energy|Hydro","EJ/yr",1.083,1.209,1.23,1.23,1.23]
["REMIND","FullTech","US","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",6.768,4.336,1.324,0.0074,1.4E-3]
["REMIND","FullTech","US","Water Consumption|Electricity|Cooling Pond","km3/yr",0.9585,0.6708,0.3471,0.193,0.1374]
["REMIND","FullTech","US","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","FullTech","USA","Capacity Additions|Electricity|Hydro","GW/yr",1.927,1.594,0.9976,1.02,1.062]
["REMIND","FullTech","USA","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",2621,2802,3156,2954,2017]
["REMIND","FullTech","USA","Primary Energy|Fossil|w/o CCS","EJ/yr",82.89,79.55,73.96,61.71,46.53]
["REMIND","FullTech","USA","Secondary Energy","EJ/yr",70.43,73.43,75.82,73.91,70.59]
["REMIND","FullTech","USA","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0084,0.0054,0.0082,0.0156,0.0144]
["REMIND","FullTech","USA","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0.0171,0.0868,0.3315,0.5473]
["REMIND","FullTech","World","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0.1607,3.704,10.43,14.13]
["REMIND","FullTech","World","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0.0156,0.8453,3.187,4.113]
["REMIND","FullTech","World","Primary Energy|Coal|Hydrogen","EJ/yr",0.1425,0.0803,0.0873,0.147,0.1405]
["REMIND","FullTech","World","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0.1187,1.729,8.85,16.41]
["REMIND","FullTech","World","Secondary Energy|Gases|Other","EJ/yr",0.6802,2.449,3.796,4.831,5.874]
["REMIND","FullTech","World","Water Withdrawal|Electricity|Coal","km3/yr",290.3,211.9,93.14,17.34,0.7081]
["REMIND","Conv","AME","Capacity|Electricity|Biomass|w/ CCS","GW",0,0.011,0.5013,4.6038,21.717]
["REMIND","Conv","AME","Emissions|CO2","Mt CO2/yr",4690,4699.7,4184.3,4031,3504.4]
["REMIND","Conv","AME","Primary Energy|Biomass|Traditional","EJ/yr",13.0694,12.8085,10.9282,8.2103,5.0845]
["REMIND","Conv","AME","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0.0002,0.0002,0.0002,0.0003]
["REMIND","Conv","AME","Secondary Energy|Electricity|Wind","EJ/yr",0.01,0.1244,0.6071,1.4443,2.364]
["REMIND","Conv","AME","Secondary Energy|Solids","EJ/yr",0.5116,0.438,0.165,0.1089,0.0281]
["REMIND","Conv","AS","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",5.271,9.076,9.95,10.04,10.14]
["REMIND","Conv","AS","Capacity|Electricity|Solar|PV","GW",1.13,37.71,36.18,27.78,3.779]
["REMIND","Conv","AS","Final Energy|Transportation","EJ/yr",8.414,8.781,11.31,13.22,13.87]
["REMIND","Conv","AS","Resource|Cumulative Extraction|Oil","EJ",4.702,3.727,4.361,4.575,4.289]
["REMIND","Conv","AS","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0,0,0,0]
["REMIND","Conv","AS","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0.0004,0.0137,0.0996,0.2633]
["REMIND","Conv","AS","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","Conv","ASIA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",0,0,0,0,0]
["REMIND","Conv","ASIA","Final Energy|Liquids","EJ/yr",32.256,52.85,76.08,83.03,83.92]
["REMIND","Conv","ASIA","Primary Energy|Oil","EJ/yr",41.585,64.27,88.75,92.07,84.37]
["REMIND","Conv","ASIA","Secondary Energy|Gases|Natural Gas","EJ/yr",8.894,10.165,7.982,7.377,8.035]
["REMIND","Conv","ASIA","Secondary Energy|Liquids|Oil","EJ/yr",35.998,57.2,79.99,83.45,76.73]
["REMIND","Conv","ASIA","Water Withdrawal|Electricity|Coal","km3/yr",146.907,133.866,71.122,17.4243,1.5972]
["REMIND","Conv","ASIA","Water Withdrawal|Electricity|Once Through","km3/yr",142.76,153.41,104.2,66.27,63.166]
["REMIND","Conv","China","Emissions|CO2|Land Use","Mt CO2/yr",39.05,-0.1819,-18.19,-15.25,-14.38]
["REMIND","Conv","China","Primary Energy|Biomass|Traditional","EJ/yr",9.101,7.762,5.768,3.649,1.913]
["REMIND","Conv","China","Primary Energy|Gas|w/o CCS","EJ/yr",4.82,19,31.76,27.01,16.11]
["REMIND","Conv","China","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0,0.0119,0.0115,0.009,0.0036]
["REMIND","Conv","China","Water Consumption|Electricity|Solar|PV","km3/yr",1E-4,0.0061,0.0059,0.0045,0.0006]
["REMIND","Conv","China","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",1.908,14.68,16.79,11.89,3.669]
["REMIND","Conv","CN","Capacity|Electricity|Solar|PV","GW",0.9,38.15,36.65,28.23,4.038]
["REMIND","Conv","CN","Primary Energy|Biomass|Gases","EJ/yr",0.1959,0.1923,0.1755,0.1279,0.0349]
["REMIND","Conv","CN","Primary Energy|Fossil","EJ/yr",83.77,93.82,94.28,70.75,46.32]
["REMIND","Conv","CN","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",2.053,3.821,4.982,5.36,5.648]
["REMIND","Conv","CN","Water Consumption|Electricity|Nuclear","km3/yr",0.1596,0.9159,3.077,6.895,10.78]
["REMIND","Conv","CN","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","Conv","EIT","Capacity|Electricity|Gas|w/ CCS","GW",0,1E-3,0.319,3.028,15.4]
["REMIND","Conv","EIT","Price|Primary Energy|Oil","US$2010/GJ",5.5874,6.4792,8.0643,9.5775,11.1328]
["REMIND","Conv","EIT","Primary Energy|Oil","EJ/yr",5.229,5.572,6.198,5.44,4.401]
["REMIND","Conv","EIT","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",1.84,1.6,1.072,0.4401,0.1126]
["REMIND","Conv","EIT","Water Consumption|Electricity|Gas","km3/yr",0.6888,0.5281,0.3087,0.11,0.0792]
["REMIND","Conv","EIT","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",1.956,3.315,2.329,1E-4,1E-4]
["REMIND","Conv","EU","Capacity Additions|Electricity|Wind","GW/yr",17.25,1E-4,2.27,11.89,6.188]
["REMIND","Conv","EU","Emissions|CO2|Land Use","Mt CO2/yr",-12.37,-11.41,-12.27,-12.84,-12.87]
["REMIND","Conv","EU","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.0561,0.5405,2.054,2.922]
["REMIND","Conv","EU","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.3332,0.6578,1.034,1.357,1.428]
["REMIND","Conv","EU","Secondary Energy|Liquids|Coal","EJ/yr",0,0,1E-4,1E-4,1E-4]
["REMIND","Conv","EU","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0.0469,0.1455,0.4399,0.5951]
["REMIND","Conv","IN","Capacity|Electricity|Solar|CSP","GW",0.01,0.18,0.1731,0.1414,0.1118]
["REMIND","Conv","IN","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",37.11,46.08,109.8,147.7,165.7]
["REMIND","Conv","IN","Primary Energy|Coal|w/o CCS","EJ/yr",11.49,13.67,9.287,3.652,0.1064]
["REMIND","Conv","IN","Secondary Energy|Electricity|Hydro","EJ/yr",0.3898,0.3513,0.3125,0.2804,0.2844]
["REMIND","Conv","IN","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0,0.0249,0.1601,0.4424]
["REMIND","Conv","IN","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,0,0,0,0]
["REMIND","Conv","India","Capacity|Electricity|Coal|w/o CCS","GW",99.96,148.1,118.3,48.33,0.2001]
["REMIND","Conv","India","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",864,1151,893,130.2,-337.1]
["REMIND","Conv","India","Price|Primary Energy|Oil","US$2010/GJ",6.4758,7.4584,9.264,10.8614,12.4399]
["REMIND","Conv","India","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,1E-4,0.0268,0.0713,0.0692]
["REMIND","Conv","India","Secondary Energy|Gases|Biomass","EJ/yr",0.0641,0.1414,0.1712,0.1509,0.1036]
["REMIND","Conv","India","Water Consumption|Electricity|Gas","km3/yr",0.0815,0.1073,0.2346,0.1815,0.0661]
["REMIND","Conv","Japan","Capacity Additions|Electricity|Solar|PV","GW/yr",1.439,1E-4,1E-4,1E-4,0.0163]
["REMIND","Conv","Japan","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,1.969,24.23,78.44,88.88]
["REMIND","Conv","Japan","Policy Cost|GDP Loss","billion US$2010/yr",0,23.8053,45.1736,76.4119,108.6693]
["REMIND","Conv","Japan","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0,0.0092,0.1061,0.4313]
["REMIND","Conv","Japan","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","Conv","Japan","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",0.0305,0.0292,0.0166,0.0027,0]
["REMIND","Conv","LA","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0.0008,0.0189,0.0259,0.0044]
["REMIND","Conv","LA","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0.2412,0,0,0,0]
["REMIND","Conv","LA","Final Energy|Solids|Biomass","EJ/yr",4.408,4.344,3.727,2.814,1.751]
["REMIND","Conv","LA","Primary Energy|Coal|w/o CCS","EJ/yr",1.223,0.6828,0.1717,0.0246,0.0055]
["REMIND","Conv","LA","Resource|Cumulative Extraction|Coal","EJ",17.13,45.87,64,79.84,91.68]
["REMIND","Conv","LA","Secondary Energy|Solids|Coal","EJ/yr",0.5845,0.3583,0.0895,0.0189,0.004]
["REMIND","Conv","LA","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0.0157,0.0138,0.0116,0.0148,0.0251]
["REMIND","Conv","LA","Water Withdrawal|Electricity|Solar|PV","km3/yr",1E-4,0.0009,0.0009,0.0007,1E-4]
["REMIND","Conv","LAM","Final Energy|Gases","EJ/yr",4.575,5.467,3.498,2.666,1.914]
["REMIND","Conv","LAM","Primary Energy|Coal","EJ/yr",1.223,0.683,0.1769,0.0469,0.0361]
["REMIND","Conv","LAM","Primary Energy|Non-Biomass Renewables","EJ/yr",2.757,3.696,4.526,4.885,5.227]
["REMIND","Conv","LAM","Secondary Energy|Gases|Biomass","EJ/yr",0.2892,0.2827,0.255,0.1794,0.0451]
["REMIND","Conv","LAM","Water Withdrawal|Electricity|Biomass","km3/yr",0,0.0375,0.5702,4.218,10.62]
["REMIND","Conv","LAM","Water Withdrawal|Electricity|Nuclear","km3/yr",0.7508,0.8759,0.7111,0.5473,0.3679]
["REMIND","Conv","MAF","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0.0266,0.0559,0.0547,0.0591]
["REMIND","Conv","MAF","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0.0055,0.2189,2.1798,10.338]
["REMIND","Conv","MAF","Primary Energy|Gas|Electricity","EJ/yr",8.4606,7.513,8.988,18.413,31.718]
["REMIND","Conv","MAF","Secondary Energy|Liquids","EJ/yr",25.433,44.856,46.479,49.3,50.64]
["REMIND","Conv","MAF","Water Consumption|Electricity|Once Through","km3/yr",0.0933,0.0752,0.0656,0.0815,0.1413]
["REMIND","Conv","OECD90","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0.7284,4.8645,4.0002,0]
["REMIND","Conv","OECD90","Capacity|Electricity|Nuclear","GW",333.51,313.26,328.56,404.57,506.94]
["REMIND","Conv","OECD90","Primary Energy|Biomass","EJ/yr",13.9912,18.4858,18.6082,23.5152,39.366]
["REMIND","Conv","OECD90","Primary Energy|Wind","EJ/yr",1.2843,2.0911,3.0397,3.685,5.082]
["REMIND","Conv","OECD90","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",9.039,13.5891,16.4819,10.9689,4.7538]
["REMIND","Conv","OECD90","Secondary Energy|Solids|Coal","EJ/yr",7.845,4.7111,3.379,2.9321,2.7728]
["REMIND","Conv","OECD90","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.006,0.0276,0.0264,0.0266,0.0047]
["REMIND","Conv","PAC","Capacity|Electricity|Biomass|w/o CCS","GW",0.694,0.8911,0.8251,0.6328,0.2734]
["REMIND","Conv","PAC","Final Energy|Gases","EJ/yr",7.556,7.638,6.2547,4.6718,3.2184]
["REMIND","Conv","PAC","Primary Energy|Hydro","EJ/yr",2.817,2.9763,3.2297,3.2265,3.1998]
["REMIND","Conv","PAC","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",3.452,1.9865,0.8227,0.1962,0.0165]
["REMIND","Conv","PAC","Secondary Energy|Liquids","EJ/yr",19.143,21.869,24.25,23.822,20.965]
["REMIND","Conv","PAC","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.1415,0.2959,0.7597,0.8612,0.8631]
["REMIND","Conv","REF","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0.003,0.0062,0.1207,3.596]
["REMIND","Conv","REF","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",331.5,338.7,391.2,366.2,289.1]
["REMIND","Conv","REF","Primary Energy|Gas","EJ/yr",14.94,12.22,8.304,5.285,4.103]
["REMIND","Conv","REF","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.0694,0.1322,0.1038,0,0]
["REMIND","Conv","REF","Secondary Energy|Gases|Natural Gas","EJ/yr",7.218,6.461,4.986,3.915,3.147]
["REMIND","Conv","REF","Water Consumption|Electricity|Once Through","km3/yr",0.1852,0.1981,0.1504,0.0974,0.0634]
["REMIND","Conv","RER","Capacity|Electricity|Hydro","GW",82.48,73.8,73.8,73.8,72.99]
["REMIND","Conv","RER","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,1.566,14.86,42.64,45.89]
["REMIND","Conv","RER","Primary Energy|Biomass","EJ/yr",6.095,7.959,7.98,7.72,8.019]
["REMIND","Conv","RER","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0.0288,0.2829,1.103,1.582]
["REMIND","Conv","RER","Secondary Energy|Gases|Other","EJ/yr",0.2557,0.476,0.601,0.7456,0.8483]
["REMIND","Conv","RER","Water Consumption|Electricity|Geothermal","km3/yr",0.1607,0.267,0.431,0.431,0.431]
["REMIND","Conv","Russia","Capacity|Electricity|Biomass|w/ CCS","GW",0,0.0006,0.0011,0.0375,0.7884]
["REMIND","Conv","Russia","Capacity|Electricity|Biomass|w/o CCS","GW",0.1999,1.499,8.298,18.61,20.05]
["REMIND","Conv","Russia","Price|Carbon","US$2010/tCO2",0,51.5099,83.9002,136.6951,222.6557]
["REMIND","Conv","Russia","Primary Energy|Biomass|w/ CCS","EJ/yr",0,1E-4,0.0002,0.0244,0.3215]
["REMIND","Conv","Russia","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",0.3856,0.1547,0.0235,0.0009,0.0002]
["REMIND","Conv","Russia","Water Consumption|Electricity|Fossil","km3/yr",0.9167,0.7312,0.4256,0.1102,0.0793]
["REMIND","Conv","Russia","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","Conv","US","Capacity Additions|Electricity|Nuclear","GW/yr",1.476,2.36,2.382,2.86,4.449]
["REMIND","Conv","US","GDP|MER","billion US$2010/yr",14389.5426,18798.3478,23207.153,26829.4628,29931.13]
["REMIND","Conv","US","Primary Energy|Gas","EJ/yr",21.51,24.16,25.59,22.57,18.2]
["REMIND","Conv","US","Secondary Energy|Electricity","EJ/yr",15.7,16.53,16.62,16.51,18.52]
["REMIND","Conv","US","Secondary Energy|Solids|Biomass","EJ/yr",0.1015,0.689,1.158,1.404,1.536]
["REMIND","Conv","US","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0.0599,0.2471,0.8102,1.297]
["REMIND","Conv","USA","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0.191,2.222,10.82,13.3]
["REMIND","Conv","USA","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,1.4E-3,0.1508,0.2947,0.2835]
["REMIND","Conv","USA","Primary Energy|Coal|Hydrogen","EJ/yr",0.0132,0.0085,0.0169,0.0188,0.0165]
["REMIND","Conv","USA","Primary Energy|Oil|w/o CCS","EJ/yr",41.92,42.05,47.45,46.87,40.55]
["REMIND","Conv","USA","Secondary Energy|Gases|Other","EJ/yr",0.3916,0.7327,0.8722,0.9939,1.106]
["REMIND","Conv","USA","Water Withdrawal|Electricity|Coal","km3/yr",82.16,51.65,15.49,0.0856,0.0179]
["REMIND","Conv","USA","Water Withdrawal|Electricity|Once Through","km3/yr",122.1,84.63,36.87,12.68,4.779]
["REMIND","Conv","World","Emissions|CO2","Mt CO2/yr",37050,35810,31480,24310,16390]
["REMIND","Conv","World","Primary Energy|Biomass|Traditional","EJ/yr",49.44,46.4,38.1,27.41,16.37]
["REMIND","Conv","World","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0.0774,0.9231,3.083,3.434]
["REMIND","Conv","World","Secondary Energy|Electricity|Wind","EJ/yr",1.743,4.839,8.689,12.1,16.54]
["REMIND","Conv","World","Water Consumption|Electricity|Wet Tower","km3/yr",23.52,25.07,28.8,35.13,46.4]
["REMIND","NewRE","AME","Capacity Additions|Electricity|Hydro","GW/yr",1.1811,5.517,7.141,0.5332,0.6579]
["REMIND","NewRE","AME","Capacity|Electricity|Wind","GW",1.02,24.613,160.77,473.5,897.6]
["REMIND","NewRE","AME","GDP|MER","billion US$2010/yr",2862.8432,4586.0436,7152.6772,10648.7046,15219.24]
["REMIND","NewRE","AME","Secondary Energy","EJ/yr",53.08,67.22,68.82,78.67,90.69]
["REMIND","NewRE","AME","Secondary Energy|Gases|Biomass","EJ/yr",0.5801,0.5678,0.5136,0.3649,0.094]
["REMIND","NewRE","AME","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","AME","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","NewRE","AS","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["REMIND","NewRE","AS","Final Energy|Liquids","EJ/yr",13.9,18.15,23.38,25.75,25.36]
["REMIND","NewRE","AS","Primary Energy|Oil","EJ/yr",18.01,22.16,27.2,28.88,27.02]
["REMIND","NewRE","AS","Secondary Energy|Gases|Natural Gas","EJ/yr",4.104,4.012,2.837,2.172,1.938]
["REMIND","NewRE","AS","Secondary Energy|Liquids|Oil","EJ/yr",15.36,19.66,24.63,26.29,24.59]
["REMIND","NewRE","AS","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",1.097,0.576,0.1409,0,0]
["REMIND","NewRE","ASIA","Consumption","billion US$2010/yr",7867.1695,11234.6991,15199.3005,19052.0203,22858.217]
["REMIND","NewRE","ASIA","Emissions|CO2|Land Use","Mt CO2/yr",993.92,503.3891,4.099,-27.276,-26.462]
["REMIND","NewRE","ASIA","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.0016,1.8E-3,0.0016,0.0009]
["REMIND","NewRE","ASIA","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.0149,1.348,9.022,24.266,41.849]
["REMIND","NewRE","ASIA","Secondary Energy|Hydrogen|Gas","EJ/yr",0.0804,0.0708,0.036,0.006,0.0008]
["REMIND","NewRE","ASIA","Water Consumption|Electricity|Wet Tower","km3/yr",8.818,9.57,9.76,10.847,16.088]
["REMIND","NewRE","China","Capacity|Electricity|Solar|PV","GW",0.9,110.1,830.3,2179,3420]
["REMIND","NewRE","China","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",195.1,267.4,234.5,272.5,245.4]
["REMIND","NewRE","China","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0,0.0701,0.5008,1.275]
["REMIND","NewRE","China","Primary Energy|Fossil|w/ CCS","EJ/yr",0,1.5E-3,0.0024,2.3E-3,0.0017]
["REMIND","NewRE","China","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",2.053,5.301,14.16,28.11,42.1]
["REMIND","NewRE","China","Water Consumption|Electricity|Nuclear","km3/yr",0.1596,0.1736,0.1324,0.0992,0.0557]
["REMIND","NewRE","China","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0,0.0134,0.032,0.0722,0.1477]
["REMIND","NewRE","CN","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["REMIND","NewRE","CN","Price|Primary Energy|Oil","US$2010/GJ",6.7993,7.5559,9.1278,10.4205,11.5094]
["REMIND","NewRE","CN","Primary Energy|Coal|Electricity","EJ/yr",29.35,21.77,8.94,0.8884,0.0122]
["REMIND","NewRE","CN","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",10.88,16.49,18.76,11.83,4.358]
["REMIND","NewRE","CN","Water Consumption|Electricity|Gas","km3/yr",0.1533,1.893,3.23,2.367,0.8465]
["REMIND","NewRE","CN","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",1.68,1.072,0.4336,0,0]
["REMIND","NewRE","EIT","Capacity Additions|Electricity|Wind","GW/yr",0.0068,0.741,1.376,1.171,4.475]
["REMIND","NewRE","EIT","Policy Cost|GDP Loss","billion US$2010/yr",0,38.926,60.0727,80.4884,133.4827]
["REMIND","NewRE","EIT","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.0093,0.053,0.0964,0.0903]
["REMIND","NewRE","EIT","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.0131,0.1118,0.5985,1.306,1.39]
["REMIND","NewRE","EIT","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",0.1345,0.0449,0.0058,0.0002,0]
["REMIND","NewRE","EIT","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",14.46,11.94,7.109,2.067,0.1808]
["REMIND","NewRE","EU","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["REMIND","NewRE","EU","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",577.2,313.6,137.9,102.2,85.99]
["REMIND","NewRE","EU","Primary Energy|Fossil","EJ/yr",58.65,47.43,42.91,36.84,29.8]
["REMIND","NewRE","EU","Resource|Cumulative Extraction|Gas","EJ",11.04,9.161,7.642,4.819,2.722]
["REMIND","NewRE","EU","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0084,4.3E-3,2E-3,0.0005,0.0003]
["REMIND","NewRE","EU","Water Withdrawal|Electricity|Cooling Pond","km3/yr",0,-0.0099,-0.0374,-0.0349,-0.0222]
["REMIND","NewRE","IN","Capacity|Electricity|Coal|w/o CCS","GW",99.96,130.4,81.17,26.98,0.1628]
["REMIND","NewRE","IN","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",864,1044,729.1,296.5,25.31]
["REMIND","NewRE","IN","Primary Energy|Coal","EJ/yr",11.49,12.52,6.803,2.049,0.0255]
["REMIND","NewRE","IN","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","IN","Secondary Energy|Gases|Biomass","EJ/yr",0.0641,0.1775,0.36,0.336,0.2716]
["REMIND","NewRE","IN","Water Withdrawal|Electricity|Biomass","km3/yr",0,0.2162,0.3636,0.3488,0.2952]
["REMIND","NewRE","India","Capacity Additions|Electricity|Solar|PV","GW/yr",0.1705,10.78,61.81,110.1,151.5]
["REMIND","NewRE","India","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0.0002,0.0004,0.0004,0.0003]
["REMIND","NewRE","India","Policy Cost|GDP Loss","billion US$2010/yr",0,70.4523,186.9865,295.4343,453.5088]
["REMIND","NewRE","India","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0.0011,0.0305,0.1937,0.4415]
["REMIND","NewRE","India","Secondary Energy|Electricity|Solar","EJ/yr",2.8E-3,0.3218,3.09,10.68,21.58]
["REMIND","NewRE","India","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",1.616,1.901,1.15,0.3699,0.0016]
["REMIND","NewRE","Japan","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",1.803,0,0,0,0]
["REMIND","NewRE","Japan","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",122.6,130.4,164,157.6,126]
["REMIND","NewRE","Japan","Final Energy|Solids|Biomass|Traditional","EJ/yr",0.3092,0.2637,0.196,0.1241,0.065]
["REMIND","NewRE","Japan","Resource|Cumulative Extraction|Coal","EJ",0.1323,0.2552,0.2555,0.2559,0.2562]
["REMIND","NewRE","Japan","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0172,0.0537,0.112,0.111,0.112]
["REMIND","NewRE","Japan","Secondary Energy|Solids|Coal","EJ/yr",2.217,1.626,1.217,0.7397,0.4709]
["REMIND","NewRE","Japan","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0,0,0,1E-4,0.0008]
["REMIND","NewRE","LA","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,0.9459,26.08,214,650.3]
["REMIND","NewRE","LA","Final Energy|Gases","EJ/yr",4.575,5.49,3.811,2.926,2.203]
["REMIND","NewRE","LA","Primary Energy|Coal","EJ/yr",1.223,0.6776,0.1669,6.6E-3,2E-3]
["REMIND","NewRE","LA","Primary Energy|Non-Biomass Renewables","EJ/yr",2.757,3.959,6.422,9.965,13.95]
["REMIND","NewRE","LA","Secondary Energy|Liquids","EJ/yr",12.34,15.53,19.16,19.42,19.13]
["REMIND","NewRE","LA","Water Withdrawal|Electricity|Biomass","km3/yr",0,0.0186,0.0236,0.0223,0.0183]
["REMIND","NewRE","LA","Water Withdrawal|Electricity|Nuclear","km3/yr",0.7508,0.6023,0.3624,0.2158,0.0964]
["REMIND","NewRE","LAM","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",909,1052,1285,1033,396]
["REMIND","NewRE","LAM","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0.0189,0.4828,3.92,11.74]
["REMIND","NewRE","LAM","Primary Energy|Gas|Electricity","EJ/yr",3.189,5.5,5.083,2.084,0.2293]
["REMIND","NewRE","LAM","Secondary Energy|Electricity|Solar","EJ/yr",0.0027,0.1282,1.107,3.646,7.114]
["REMIND","NewRE","LAM","Water Consumption|Electricity|Solar","km3/yr",1E-4,0.0233,0.2528,1.061,2.371]
["REMIND","NewRE","LAM","Water Withdrawal|Electricity|Gas","km3/yr",4.874,8.182,7.219,2.837,0.2802]
["REMIND","NewRE","MAF","Capacity|Electricity|Oil|w/o CCS","GW",75.967,36.175,8.0091,0.0022,2E-3]
["REMIND","NewRE","MAF","Primary Energy|Biomass|Electricity","EJ/yr",0,0.0354,0.1341,0.6153,2.3932]
["REMIND","NewRE","MAF","Resource|Cumulative Extraction|Coal","EJ",12.443,32.034,40.02,42.8,44.21]
["REMIND","NewRE","MAF","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,0.0064,0.0624,0.2573]
["REMIND","NewRE","MAF","Water Consumption|Electricity|Geothermal","km3/yr",0.0198,0.1134,0.5842,0.862,0.8611]
["REMIND","NewRE","MAF","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.0003,0.0514,0.6164,3.037,8.123]
["REMIND","NewRE","OECD90","Capacity|Electricity|Biomass|w/o CCS","GW",22.53,32.1579,39.371,34.2415,21.3729]
["REMIND","NewRE","OECD90","Price|Carbon","US$2010/tCO2",0,192.3036,313.2244,510.4464,831.248]
["REMIND","NewRE","OECD90","Primary Energy|Hydro","EJ/yr",5.076,5.2693,5.5407,5.5365,5.4988]
["REMIND","NewRE","OECD90","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",13.28,6.4565,1.5654,0.2554,0.0058]
["REMIND","NewRE","OECD90","Secondary Energy|Liquids","EJ/yr",83.773,90.822,101.339,96.906,85.62]
["REMIND","NewRE","OECD90","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.6799,1.0586,2.6358,5.7307,10.7905]
["REMIND","NewRE","PAC","Capacity Additions|Electricity|Nuclear","GW/yr",1.7503,0,0,0,0]
["REMIND","NewRE","PAC","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",1418.7,1636.5,1806.2,1735,1332.8]
["REMIND","NewRE","PAC","Primary Energy|Gas","EJ/yr",14.81,18.085,17.604,12.877,7.622]
["REMIND","NewRE","PAC","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.526,0.2523,0.0861,0.0404,0.026]
["REMIND","NewRE","PAC","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0.0004,0.0084,0.0171,0.0161]
["REMIND","NewRE","PAC","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",45.724,35.746,21.453,10.3061,2.771]
["REMIND","NewRE","REF","Capacity|Electricity|Nuclear","GW",23.22,25.92,20.07,15.22,8.626]
["REMIND","NewRE","REF","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",66.45,23.48,3.196,0.1071,0.0277]
["REMIND","NewRE","REF","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","REF","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",1.385,1.444,1.095,0.4518,0.0876]
["REMIND","NewRE","REF","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.0694,0.1322,0.1038,0,0]
["REMIND","NewRE","REF","Water Consumption|Electricity|Geothermal","km3/yr",0.0064,0.006,0.0268,0.1142,0.3072]
["REMIND","NewRE","RER","Capacity|Electricity|Biomass|w/ CCS","GW",0,0,0.0456,0.9067,4.695]
["REMIND","NewRE","RER","Emissions|CO2","Mt CO2/yr",4096,3306,2945,2518,1941]
["REMIND","NewRE","RER","Price|Carbon","US$2010/tCO2",0,48.0759,78.3061,127.6116,207.812]
["REMIND","NewRE","RER","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","RER","Secondary Energy|Electricity|Wind","EJ/yr",0.8143,2.25,3.892,5.591,7.233]
["REMIND","NewRE","RER","Water Consumption|Electricity|Fossil","km3/yr",2.271,1.33,0.6741,0.3037,0.0647]
["REMIND","NewRE","Russia","Capacity Additions|Electricity|Hydro","GW/yr",0.047,1.325,4.478,3.83,0.5178]
["REMIND","NewRE","Russia","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",331.5,348.8,417.5,374.2,279.8]
["REMIND","NewRE","Russia","GDP|MER","billion US$2010/yr",1001.2862,1322.6416,1777.9227,2182.2478,2435.92]
["REMIND","NewRE","Russia","Secondary Energy","EJ/yr",21.59,18.68,18.14,18.09,16.59]
["REMIND","NewRE","Russia","Secondary Energy|Electricity","EJ/yr",2.914,3.036,3.378,4.017,3.968]
["REMIND","NewRE","Russia","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.0091,0.0565,0.2299,0.369,0.2915]
["REMIND","NewRE","Russia","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",19.79,16.37,9.582,2.072,0.1818]
["REMIND","NewRE","US","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0,0.0002,0,0,0.0002]
["REMIND","NewRE","US","Final Energy|Other Sector","EJ/yr",37.62,40.66,41.69,39.83,39.38]
["REMIND","NewRE","US","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,1E-4,1E-4,1E-4]
["REMIND","NewRE","US","Primary Energy|Solar","EJ/yr",0.0198,0.4394,2.84,7.337,12.51]
["REMIND","NewRE","US","Secondary Energy|Gases|Coal","EJ/yr",0,1E-4,1E-4,0,0]
["REMIND","NewRE","US","Secondary Energy|Gases|Natural Gas","EJ/yr",13.12,12.02,8.346,6.506,5.095]
["REMIND","NewRE","US","Secondary Energy|Gases|Other","EJ/yr",0.3916,0.7327,0.8722,0.9939,1.106]
["REMIND","NewRE","US","Secondary Energy|Heat","EJ/yr",0.198,0.1135,0.0372,0.0154,0.0188]
["REMIND","NewRE","US","Secondary Energy|Hydrogen","EJ/yr",0.0295,0.0217,0.0155,0.02,0.0828]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0,1E-4,0.0118,0.0764]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,1E-4,0.0118,0.0764]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0084,3.3E-3,0.0006,0.0002,1E-4]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,1E-4,1E-4,0]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0.0084,0.0032,0.0006,1E-4,0]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Gas","EJ/yr",0.0211,0.0184,0.0148,0.0081,0.0062]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,2E-3,0.0078,0.0075,0.0062]
["REMIND","NewRE","US","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0.0211,0.0164,0.007,0.0006,0]
["REMIND","NewRE","US","Secondary Energy|Liquids","EJ/yr",37.31,39.64,44.67,42.39,37.51]
["REMIND","NewRE","US","Secondary Energy|Liquids|Biomass","EJ/yr",0.0878,1.643,1.937,3.996,9.73]
["REMIND","NewRE","US","Secondary Energy|Liquids|Coal","EJ/yr",0,0,1E-4,1E-4,1E-4]
["REMIND","NewRE","US","Secondary Energy|Liquids|Oil","EJ/yr",37.22,38,42.73,38.39,27.78]
["REMIND","NewRE","US","Secondary Energy|Solids","EJ/yr",1.372,1.922,2.392,2.354,2.471]
["REMIND","NewRE","US","Secondary Energy|Solids|Biomass","EJ/yr",0.1015,0.6927,1.196,1.177,1.235]
["REMIND","NewRE","US","Secondary Energy|Solids|Coal","EJ/yr",1.27,1.229,1.196,1.177,1.235]
["REMIND","NewRE","US","Water Consumption|Electricity","km3/yr",11.53,10.48,9.188,9.303,10.9]
["REMIND","NewRE","US","Water Consumption|Electricity|Biomass","km3/yr",0.035,0.0307,0.0247,0.0152,0.0032]
["REMIND","NewRE","US","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.035,0.0307,0.0247,0.0152,0.0032]
["REMIND","NewRE","US","Water Consumption|Electricity|Coal","km3/yr",3.205,1.368,0.2009,1.8E-3,0.0003]
["REMIND","NewRE","US","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",3.205,1.368,0.2009,1.8E-3,0.0003]
["REMIND","NewRE","US","Water Consumption|Electricity|Cooling Pond","km3/yr",0.9585,0.5524,0.2224,0.0893,0.0252]
["REMIND","NewRE","US","Water Consumption|Electricity|Dry Cooling","km3/yr",0.0175,0.02,0.0334,0.0661,0.1217]
["REMIND","NewRE","US","Water Consumption|Electricity|Fossil","km3/yr",4.524,3.239,1.855,0.7735,0.1531]
["REMIND","NewRE","US","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",4.524,3.239,1.855,0.7735,0.1531]
["REMIND","NewRE","US","Water Consumption|Electricity|Gas","km3/yr",1.144,1.782,1.632,0.7717,0.1527]
["REMIND","NewRE","US","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",1.144,1.782,1.632,0.7717,0.1527]
["REMIND","NewRE","US","Water Consumption|Electricity|Geothermal","km3/yr",0.3667,0.3755,0.431,0.4217,0.431]
["REMIND","NewRE","US","Water Consumption|Electricity|Hydro","km3/yr",5.112,5.726,5.808,5.808,5.808]
["REMIND","NewRE","US","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",5.482,6.163,6.767,8.256,10.67]
["REMIND","NewRE","US","Water Consumption|Electricity|Nuclear","km3/yr",1.486,1.048,0.5422,0.2581,0.0793]
["REMIND","NewRE","US","Water Consumption|Electricity|Oil","km3/yr",0.1748,0.0893,0.0212,0,0]
["REMIND","NewRE","US","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.1748,0.0893,0.0212,0,0]
["REMIND","NewRE","US","Water Consumption|Electricity|Once Through","km3/yr",0.8124,0.4609,0.1733,0.0643,0.0162]
["REMIND","NewRE","US","Water Consumption|Electricity|Solar","km3/yr",3.3E-3,0.0612,0.5276,2.026,4.429]
["REMIND","NewRE","US","Water Consumption|Electricity|Solar|CSP","km3/yr",0.0029,0.0513,0.4688,1.902,4.257]
["REMIND","NewRE","US","Water Consumption|Electricity|Solar|PV","km3/yr",0.0004,0.0099,0.0588,0.1246,0.1723]
["REMIND","NewRE","US","Water Consumption|Electricity|Wet Tower","km3/yr",4.612,3.694,2.852,3.036,4.524]
["REMIND","NewRE","US","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity","km3/yr",144,82.68,32.79,14.59,7.974]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Biomass","km3/yr",1.694,1.484,1.193,0.733,0.1528]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",1.694,1.484,1.193,0.733,0.1528]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Coal","km3/yr",82.16,35.06,5.15,0.045,0.008]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",82.16,35.06,5.15,0.045,0.008]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Cooling Pond","km3/yr",15.24,8.062,2.766,1.035,0.2909]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.0175,0.02,0.0334,0.0661,0.1217]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Fossil","km3/yr",99.52,50.83,15.16,4.044,0.6979]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",99.52,50.83,15.16,4.044,0.6979]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Gas","km3/yr",11.36,12.7,9.277,3.999,0.6898]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",11.36,12.7,9.277,3.999,0.6898]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Geothermal","km3/yr",0.3667,0.3755,0.431,0.4217,0.431]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.37,0.4367,0.9586,2.448,4.86]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Nuclear","km3/yr",42.43,29.92,15.48,7.368,2.264]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Oil","km3/yr",6.006,3.068,0.7295,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",6.006,3.068,0.7295,0,0]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Once Through","km3/yr",122.1,69.33,26.14,9.823,2.54]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Solar","km3/yr",3.3E-3,0.0612,0.5276,2.026,4.429]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.0029,0.0513,0.4688,1.902,4.257]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Solar|PV","km3/yr",0.0004,0.0099,0.0588,0.1246,0.1723]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Wet Tower","km3/yr",6.689,5.234,3.75,3.431,4.613]
["REMIND","NewRE","US","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0.0236,0.2915,1.667,2.941]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",0,0.0002,0,0,0.0002]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",0,0,0,0,0.1077]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",12.56,24.51,4.861,0.6975,1.526]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Hydro","GW/yr",1.927,1.499,1.018,1.041,1.083]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Nuclear","GW/yr",1.476,0,0,0,0]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Solar|CSP","GW/yr",0.088,0.9502,6.407,17.84,24.66]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Solar|PV","GW/yr",0.9903,13.63,47.44,56.94,51.84]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Wind","GW/yr",11.94,25.34,34.96,40.22,40.69]
["REMIND","NewRE","USA","Capacity Additions|Electricity|Wind|Onshore","GW/yr",11.94,25.34,34.96,40.22,40.69]
["REMIND","NewRE","USA","Capacity|Electricity|Biomass|w/ CCS","GW",0,0.059,1.317,10.13,34.6]
["REMIND","NewRE","USA","Capacity|Electricity|Biomass|w/o CCS","GW",12.02,11.71,10.46,7.118,1.644]
["REMIND","NewRE","USA","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["REMIND","NewRE","USA","Capacity|Electricity|Coal|w/o CCS","GW",286.6,126.5,19.1,0.1858,0.0358]
["REMIND","NewRE","USA","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["REMIND","NewRE","USA","Capacity|Electricity|Gas|w/o CCS","GW",270.1,430.1,468.8,275.9,107.9]
["REMIND","NewRE","USA","Capacity|Electricity|Hydro","GW",75.77,84.94,86.16,86.16,86.16]
["REMIND","NewRE","USA","Capacity|Electricity|Nuclear","GW",117.6,82.95,42.91,20.43,6.275]
["REMIND","NewRE","USA","Capacity|Electricity|Oil|w/o CCS","GW",29.16,13.89,3.075,1E-3,1E-3]
["REMIND","NewRE","USA","Capacity|Electricity|Solar|CSP","GW",0.22,3.931,35.98,154.1,358.7]
["REMIND","NewRE","USA","Capacity|Electricity|Solar|PV","GW",2.49,58.14,363.6,878.8,1305]
["REMIND","NewRE","USA","Capacity|Electricity|Wind","GW",40,224.6,501.6,752.4,885.2]
["REMIND","NewRE","USA","Capacity|Electricity|Wind|Onshore","GW",40,224.6,501.6,752.4,885.2]
["REMIND","NewRE","USA","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0.1816,4.056,31.19,106.6]
["REMIND","NewRE","USA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,0.0002,0.0004,0.0005,0.0004]
["REMIND","NewRE","USA","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Consumption","billion US$2010/yr",7912.5868,11586.9604,16095.4622,21002.7504,26541.45]
["REMIND","NewRE","USA","Emissions|CO2","Mt CO2/yr",5951,5183,4648,3513,1731]
["REMIND","NewRE","USA","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,1.627,33.61,256.3,879.6]
["REMIND","NewRE","USA","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,1.479,33.04,255.7,879.1]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",2243,1525,899.9,388.5,11.25]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,-0.1816,-4.056,-31.19,-106.6]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0,0,1E-4,0]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",1726,746,110.4,1.037,0.1951]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",450.9,744.9,785.6,418.7,117.6]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",736.3,674.2,468.2,365,285.8]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",24.47,11.54,1.83,0.0667,6.6E-3]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",2621,2816,3139,2623,1298]
["REMIND","NewRE","USA","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",2621,2816,3139,2623,1298]
["REMIND","NewRE","USA","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",5800,5200,4682,3549,1767]
["REMIND","NewRE","USA","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",2615,2037,1405,701.6,-176.2]
["REMIND","NewRE","USA","Emissions|CO2|Land Use","Mt CO2/yr",151.2,-17.16,-34.09,-35.89,-35.89]
["REMIND","NewRE","USA","Final Energy","EJ/yr",64.55,67.04,70.85,69.26,67.05]
["REMIND","NewRE","USA","Final Energy|Electricity","EJ/yr",13.2,13.88,15.67,17.96,21.7]
["REMIND","NewRE","USA","Final Energy|Gases","EJ/yr",12.59,11.78,8.514,6.718,5.293]
["REMIND","NewRE","USA","Final Energy|Heat","EJ/yr",0.1111,0.0747,0.0281,0.0131,0.0178]
["REMIND","NewRE","USA","Final Energy|Hydrogen","EJ/yr",0.0295,0.0217,0.0155,0.02,0.0828]
["REMIND","NewRE","USA","Final Energy|Liquids","EJ/yr",35.34,37.73,43.01,41.42,37.09]
["REMIND","NewRE","USA","Final Energy|Other Sector","EJ/yr",37.62,40.66,41.69,39.83,39.38]
["REMIND","NewRE","USA","Final Energy|Solids","EJ/yr",3.288,3.556,3.607,3.123,2.875]
["REMIND","NewRE","USA","Final Energy|Solids|Biomass","EJ/yr",2.02,2.329,2.412,1.947,1.639]
["REMIND","NewRE","USA","Final Energy|Solids|Biomass|Traditional","EJ/yr",1.918,1.637,1.217,0.7702,0.404]
["REMIND","NewRE","USA","Final Energy|Solids|Coal","EJ/yr",1.268,1.228,1.195,1.177,1.235]
["REMIND","NewRE","USA","Final Energy|Transportation","EJ/yr",26.93,26.39,29.16,29.43,27.67]
["REMIND","NewRE","USA","GDP|MER","billion US$2010/yr",14389.5426,18809.4252,23273.6174,26907.0046,30008.68]
["REMIND","NewRE","USA","GDP|PPP","billion US$2010/yr",14389.5426,18809.4252,23273.6174,26907.0046,30008.68]
["REMIND","NewRE","USA","Policy Cost|Consumption Loss","billion US$2010/yr",0,-72.845,97.4479,336.6422,600.2843]
["REMIND","NewRE","USA","Policy Cost|GDP Loss","billion US$2010/yr",0,32.9331,122.1837,270.1778,473.7804]
["REMIND","NewRE","USA","Policy Cost|Other","billion US$2010/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Population","million",310.4,335.8,361,383.2,402.3]
["REMIND","NewRE","USA","Price|Carbon","US$2010/tCO2",0,48.0759,78.3061,127.6116,207.812]
["REMIND","NewRE","USA","Price|Primary Energy|Coal","US$2010/GJ",0.9116,0.8509,0.7702,0.754,0.7905]
["REMIND","NewRE","USA","Price|Primary Energy|Gas","US$2010/GJ",3.5625,4.1119,4.7234,4.9804,5.1599]
["REMIND","NewRE","USA","Price|Primary Energy|Oil","US$2010/GJ",6.8813,7.6379,9.2219,10.5224,11.6202]
["REMIND","NewRE","USA","Price|Secondary Energy|Electricity","US$2010/GJ",13.7471,18.322,18.7208,19.5738,17.9897]
["REMIND","NewRE","USA","Primary Energy","EJ/yr",91.62,89.86,88.97,84.13,84.51]
["REMIND","NewRE","USA","Primary Energy|Biomass","EJ/yr",4.175,7.122,7.678,11.57,24.58]
["REMIND","NewRE","USA","Primary Energy|Biomass|Electricity","EJ/yr",0.5145,0.4739,0.4868,0.9623,2.477]
["REMIND","NewRE","USA","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0.0041,0.0922,0.7088,2.422]
["REMIND","NewRE","USA","Primary Energy|Biomass|Gases","EJ/yr",1.404,1.341,1.125,0.6053,0.048]
["REMIND","NewRE","USA","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0,0.0002,0.0214,0.139]
["REMIND","NewRE","USA","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0,1E-4,0.0214,0.1389]
["REMIND","NewRE","USA","Primary Energy|Biomass|Liquids","EJ/yr",0.1596,2.841,3.47,7.875,20.14]
["REMIND","NewRE","USA","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0.0295,0.6585,5.063,17.3]
["REMIND","NewRE","USA","Primary Energy|Biomass|Modern","EJ/yr",2.254,5.483,6.46,10.8,24.18]
["REMIND","NewRE","USA","Primary Energy|Biomass|Other Carrier","EJ/yr",2.097,2.466,2.595,2.109,1.783]
["REMIND","NewRE","USA","Primary Energy|Biomass|Traditional","EJ/yr",1.922,1.639,1.218,0.7705,0.404]
["REMIND","NewRE","USA","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0.0336,0.7508,5.793,19.86]
["REMIND","NewRE","USA","Primary Energy|Biomass|w/o CCS","EJ/yr",4.175,7.088,6.927,5.781,4.726]
["REMIND","NewRE","USA","Primary Energy|Coal","EJ/yr",19.46,9.118,2.414,1.251,1.303]
["REMIND","NewRE","USA","Primary Energy|Coal|Electricity","EJ/yr",18.04,7.795,1.153,0.0108,2E-3]
["REMIND","NewRE","USA","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Primary Energy|Coal|Hydrogen","EJ/yr",0.0132,0.0051,1E-3,0.0003,1E-4]
["REMIND","NewRE","USA","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0,1E-4,1E-4,1E-4]
["REMIND","NewRE","USA","Primary Energy|Coal|w/ CCS","EJ/yr",0,1E-4,0.0002,0.0002,0.0002]
["REMIND","NewRE","USA","Primary Energy|Coal|w/o CCS","EJ/yr",19.46,9.118,2.414,1.25,1.303]
["REMIND","NewRE","USA","Primary Energy|Fossil","EJ/yr",82.89,76.86,71.88,57.42,39.03]
["REMIND","NewRE","USA","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0.0029,0.0113,0.0109,0.009]
["REMIND","NewRE","USA","Primary Energy|Fossil|w/o CCS","EJ/yr",82.89,76.86,71.87,57.41,39.02]
["REMIND","NewRE","USA","Primary Energy|Gas","EJ/yr",21.51,25.49,22.4,13.98,7.201]
["REMIND","NewRE","USA","Primary Energy|Gas|Electricity","EJ/yr",8.037,13.28,14,7.463,2.096]
["REMIND","NewRE","USA","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Primary Energy|Gas|w/ CCS","EJ/yr",0,2.8E-3,0.0111,0.0107,0.0089]
["REMIND","NewRE","USA","Primary Energy|Gas|w/o CCS","EJ/yr",21.51,25.48,22.39,13.97,7.192]
["REMIND","NewRE","USA","Primary Energy|Geothermal","EJ/yr",0.0953,0.0976,0.112,0.1103,0.1275]
["REMIND","NewRE","USA","Primary Energy|Hydro","EJ/yr",1.083,1.213,1.23,1.23,1.23]
["REMIND","NewRE","USA","Primary Energy|Non-Biomass Renewables","EJ/yr",1.589,3.783,8.328,14.62,20.74]
["REMIND","NewRE","USA","Primary Energy|Nuclear","EJ/yr",2.968,2.093,1.083,0.5153,0.1583]
["REMIND","NewRE","USA","Primary Energy|Oil","EJ/yr",41.92,42.26,47.07,42.19,30.53]
["REMIND","NewRE","USA","Primary Energy|Oil|w/o CCS","EJ/yr",41.92,42.26,47.07,42.19,30.53]
["REMIND","NewRE","USA","Primary Energy|Solar","EJ/yr",0.0198,0.4394,2.84,7.337,12.51]
["REMIND","NewRE","USA","Primary Energy|Wind","EJ/yr",0.391,2.034,4.146,5.942,6.866]
["REMIND","NewRE","USA","Resource|Cumulative Extraction|Coal","EJ",115.5,445.3,641.4,715.3,748.2]
["REMIND","NewRE","USA","Resource|Cumulative Extraction|Gas","EJ",21.66,25.48,22.51,14.23,7.523]
["REMIND","NewRE","USA","Resource|Cumulative Extraction|Oil","EJ",19.17,21.98,24.87,23.35,19.5]
["REMIND","NewRE","USA","Secondary Energy","EJ/yr",70.43,72.2,74.89,72.02,68.76]
["REMIND","NewRE","USA","Secondary Energy|Electricity","EJ/yr",15.7,16.11,17.6,19.63,23.15]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Biomass","EJ/yr",0.1957,0.1924,0.208,0.4064,1.02]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0.0017,0.0378,0.2906,0.9929]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.1957,0.1907,0.1702,0.1159,0.0268]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Coal","EJ/yr",6.768,2.989,0.4517,0.0044,0.0008]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",6.768,2.989,0.4517,0.0044,0.0008]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Fossil","EJ/yr",10.95,10.04,7.973,4.048,1.11]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",10.95,10.04,7.973,4.048,1.11]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Gas","EJ/yr",3.815,6.876,7.483,4.044,1.109]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",3.815,6.876,7.483,4.044,1.109]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Geothermal","EJ/yr",0.0953,0.0976,0.112,0.1096,0.112]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Hydro","EJ/yr",1.083,1.213,1.23,1.23,1.23]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",1.589,3.849,8.851,16.35,23.68]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Nuclear","EJ/yr",2.968,2.093,1.083,0.5153,0.1583]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Oil","EJ/yr",0.3679,0.1752,0.0388,0,0]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",0.3679,0.1752,0.0388,0,0]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Solar","EJ/yr",0.0198,0.4394,2.964,8.251,14.51]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0.0042,0.0745,0.682,2.83,6.488]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.0156,0.3649,2.282,5.421,8.025]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Wind","EJ/yr",0.391,2.1,4.545,6.76,7.828]
["REMIND","NewRE","USA","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",0.391,2.1,4.545,6.76,7.828]
["REMIND","NewRE","USA","Secondary Energy|Gases","EJ/yr",14.29,13.49,9.838,7.833,6.228]
["REMIND","NewRE","USA","Secondary Energy|Gases|Biomass","EJ/yr",0.7722,0.7374,0.6189,0.3329,0.0264]
["REMIND","NewRE","USA","Secondary Energy|Gases|Coal","EJ/yr",0,1E-4,1E-4,0,0]
["REMIND","NewRE","USA","Secondary Energy|Gases|Natural Gas","EJ/yr",13.12,12.02,8.346,6.506,5.095]
["REMIND","NewRE","USA","Secondary Energy|Gases|Other","EJ/yr",0.3916,0.7327,0.8722,0.9939,1.106]
["REMIND","NewRE","USA","Secondary Energy|Heat","EJ/yr",0.198,0.1135,0.0372,0.0154,0.0188]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen","EJ/yr",0.0295,0.0217,0.0155,0.02,0.0828]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,0,1E-4,0.0118,0.0764]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0,1E-4,0.0118,0.0764]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0084,3.3E-3,0.0006,0.0002,1E-4]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0,1E-4,1E-4,0]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0.0084,0.0032,0.0006,1E-4,0]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Gas","EJ/yr",0.0211,0.0184,0.0148,0.0081,0.0062]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,2E-3,0.0078,0.0075,0.0062]
["REMIND","NewRE","USA","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0.0211,0.0164,0.007,0.0006,0]
["REMIND","NewRE","USA","Secondary Energy|Liquids","EJ/yr",37.31,39.64,44.67,42.39,37.51]
["REMIND","NewRE","USA","Secondary Energy|Liquids|Biomass","EJ/yr",0.0878,1.643,1.937,3.996,9.73]
["REMIND","NewRE","USA","Secondary Energy|Liquids|Coal","EJ/yr",0,0,1E-4,1E-4,1E-4]
["REMIND","NewRE","USA","Secondary Energy|Liquids|Oil","EJ/yr",37.22,38,42.73,38.39,27.78]
["REMIND","NewRE","USA","Secondary Energy|Solids","EJ/yr",1.372,1.922,2.392,2.354,2.471]
["REMIND","NewRE","USA","Secondary Energy|Solids|Biomass","EJ/yr",0.1015,0.6927,1.196,1.177,1.235]
["REMIND","NewRE","USA","Secondary Energy|Solids|Coal","EJ/yr",1.27,1.229,1.196,1.177,1.235]
["REMIND","NewRE","USA","Water Consumption|Electricity","km3/yr",11.53,10.48,9.188,9.303,10.9]
["REMIND","NewRE","USA","Water Consumption|Electricity|Biomass","km3/yr",0.035,0.0307,0.0247,0.0152,0.0032]
["REMIND","NewRE","USA","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.035,0.0307,0.0247,0.0152,0.0032]
["REMIND","NewRE","USA","Water Consumption|Electricity|Coal","km3/yr",3.205,1.368,0.2009,1.8E-3,0.0003]
["REMIND","NewRE","USA","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",3.205,1.368,0.2009,1.8E-3,0.0003]
["REMIND","NewRE","USA","Water Consumption|Electricity|Cooling Pond","km3/yr",0.9585,0.5524,0.2224,0.0893,0.0252]
["REMIND","NewRE","USA","Water Consumption|Electricity|Dry Cooling","km3/yr",0.0175,0.02,0.0334,0.0661,0.1217]
["REMIND","NewRE","USA","Water Consumption|Electricity|Fossil","km3/yr",4.524,3.239,1.855,0.7735,0.1531]
["REMIND","NewRE","USA","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",4.524,3.239,1.855,0.7735,0.1531]
["REMIND","NewRE","USA","Water Consumption|Electricity|Gas","km3/yr",1.144,1.782,1.632,0.7717,0.1527]
["REMIND","NewRE","USA","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",1.144,1.782,1.632,0.7717,0.1527]
["REMIND","NewRE","USA","Water Consumption|Electricity|Geothermal","km3/yr",0.3667,0.3755,0.431,0.4217,0.431]
["REMIND","NewRE","USA","Water Consumption|Electricity|Hydro","km3/yr",5.112,5.726,5.808,5.808,5.808]
["REMIND","NewRE","USA","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",5.482,6.163,6.767,8.256,10.67]
["REMIND","NewRE","USA","Water Consumption|Electricity|Nuclear","km3/yr",1.486,1.048,0.5422,0.2581,0.0793]
["REMIND","NewRE","USA","Water Consumption|Electricity|Oil","km3/yr",0.1748,0.0893,0.0212,0,0]
["REMIND","NewRE","USA","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",0.1748,0.0893,0.0212,0,0]
["REMIND","NewRE","USA","Water Consumption|Electricity|Once Through","km3/yr",0.8124,0.4609,0.1733,0.0643,0.0162]
["REMIND","NewRE","USA","Water Consumption|Electricity|Solar","km3/yr",3.3E-3,0.0612,0.5276,2.026,4.429]
["REMIND","NewRE","USA","Water Consumption|Electricity|Solar|CSP","km3/yr",0.0029,0.0513,0.4688,1.902,4.257]
["REMIND","NewRE","USA","Water Consumption|Electricity|Solar|PV","km3/yr",0.0004,0.0099,0.0588,0.1246,0.1723]
["REMIND","NewRE","USA","Water Consumption|Electricity|Wet Tower","km3/yr",4.612,3.694,2.852,3.036,4.524]
["REMIND","NewRE","USA","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity","km3/yr",144,82.68,32.79,14.59,7.974]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Biomass","km3/yr",1.694,1.484,1.193,0.733,0.1528]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",1.694,1.484,1.193,0.733,0.1528]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Coal","km3/yr",82.16,35.06,5.15,0.045,0.008]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",82.16,35.06,5.15,0.045,0.008]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Cooling Pond","km3/yr",15.24,8.062,2.766,1.035,0.2909]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.0175,0.02,0.0334,0.0661,0.1217]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Fossil","km3/yr",99.52,50.83,15.16,4.044,0.6979]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",99.52,50.83,15.16,4.044,0.6979]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Gas","km3/yr",11.36,12.7,9.277,3.999,0.6898]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",11.36,12.7,9.277,3.999,0.6898]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Geothermal","km3/yr",0.3667,0.3755,0.431,0.4217,0.431]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",0.37,0.4367,0.9586,2.448,4.86]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Nuclear","km3/yr",42.43,29.92,15.48,7.368,2.264]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Oil","km3/yr",6.006,3.068,0.7295,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",6.006,3.068,0.7295,0,0]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Once Through","km3/yr",122.1,69.33,26.14,9.823,2.54]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Solar","km3/yr",3.3E-3,0.0612,0.5276,2.026,4.429]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.0029,0.0513,0.4688,1.902,4.257]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Solar|PV","km3/yr",0.0004,0.0099,0.0588,0.1246,0.1723]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Wet Tower","km3/yr",6.689,5.234,3.75,3.431,4.613]
["REMIND","NewRE","USA","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Capacity Additions|Electricity|Biomass|w/ CCS","GW/yr",0,0.0947,1.436,7.959,14.51]
["REMIND","NewRE","World","Capacity Additions|Electricity|Biomass|w/o CCS","GW/yr",1.258,6.023,4.62,0.8793,0.0008]
["REMIND","NewRE","World","Capacity Additions|Electricity|Coal|w/ CCS","GW/yr",0,0,0,0,0]
["REMIND","NewRE","World","Capacity Additions|Electricity|Coal|w/o CCS","GW/yr",44.5,1.472,0,0,0.2999]
["REMIND","NewRE","World","Capacity Additions|Electricity|Gas|w/ CCS","GW/yr",0,0,0,0,0]
["REMIND","NewRE","World","Capacity Additions|Electricity|Gas|w/o CCS","GW/yr",57.39,151.2,37.96,17.16,22.96]
["REMIND","NewRE","World","Capacity Additions|Electricity|Hydro","GW/yr",14.94,23.34,20.31,12.38,15.51]
["REMIND","NewRE","World","Capacity Additions|Electricity|Nuclear","GW/yr",11.57,0,0,0,0]
["REMIND","NewRE","World","Capacity Additions|Electricity|Solar|CSP","GW/yr",0.212,6.163,49.06,152.9,242.9]
["REMIND","NewRE","World","Capacity Additions|Electricity|Solar|PV","GW/yr",14.9,106.7,379.6,577.8,672.4]
["REMIND","NewRE","World","Capacity Additions|Electricity|Wind","GW/yr",48.65,141.7,259.3,353.6,410.6]
["REMIND","NewRE","World","Capacity Additions|Electricity|Wind|Onshore","GW/yr",48.65,141.7,259.3,353.6,410.6]
["REMIND","NewRE","World","Capacity|Electricity|Biomass|w/ CCS","GW",0,0.2367,6.182,49.22,165.6]
["REMIND","NewRE","World","Capacity|Electricity|Biomass|w/o CCS","GW",23.45,56.6,122,134.9,115.4]
["REMIND","NewRE","World","Capacity|Electricity|Coal|w/ CCS","GW",0,0,0,0,0]
["REMIND","NewRE","World","Capacity|Electricity|Coal|w/o CCS","GW",1211,816.5,322.8,64,0.7634]
["REMIND","NewRE","World","Capacity|Electricity|Gas|w/ CCS","GW",0,0,0,0,0]
["REMIND","NewRE","World","Capacity|Electricity|Gas|w/o CCS","GW",1243,2062,2657,1886,960.7]
["REMIND","NewRE","World","Capacity|Electricity|Hydro","GW",767.5,875.2,1007,1075,1103]
["REMIND","NewRE","World","Capacity|Electricity|Nuclear","GW",404.4,306.8,173.8,95.56,38.3]
["REMIND","NewRE","World","Capacity|Electricity|Oil|w/o CCS","GW",272.5,144.4,48.51,8.447,2.839]
["REMIND","NewRE","World","Capacity|Electricity|Solar|CSP","GW",0.53,23.37,258.2,1234,3146]
["REMIND","NewRE","World","Capacity|Electricity|Solar|PV","GW",38.82,544.3,2891,7526,12860]
["REMIND","NewRE","World","Capacity|Electricity|Wind","GW",180.4,1065,2945,5403,7642]
["REMIND","NewRE","World","Capacity|Electricity|Wind|Onshore","GW",180.4,1065,2945,5403,7642]
["REMIND","NewRE","World","Carbon Sequestration|CCS|Fossil|Biomass|Supply|Electricity","Mt CO2/yr",0,0.729,19.04,151.6,509.9]
["REMIND","NewRE","World","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Coal","Mt CO2/yr",0,5.3E-3,0.0796,0.1522,0.1428]
["REMIND","NewRE","World","Carbon Sequestration|CCS|Fossil|Energy|Supply|Electricity|Gas","Mt CO2/yr",0,0,0,0,0]
["REMIND","NewRE","World","Consumption","billion US$2010/yr",36932.0516,52750.5788,71637.5458,91211.3116,112324.8]
["REMIND","NewRE","World","Emissions|CO2","Mt CO2/yr",37050,34960,29930,23080,14280]
["REMIND","NewRE","World","Emissions|CO2|Carbon Capture and Storage","Mt CO2/yr",0,9.966,213.9,1503,4767]
["REMIND","NewRE","World","Emissions|CO2|Carbon Capture and Storage|Biomass","Mt CO2/yr",0,6.681,181.3,1416,4676]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity","Mt CO2/yr",10370,8875,6394,3035,580.9]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/ CCS","Mt CO2/yr",0,-0.729,-19.04,-151.6,-509.9]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Biomass|w/o CCS","Mt CO2/yr",0,0,0,0,0]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Coal|w/ CCS","MtCO2/yr",0,0.0006,0.0088,0.0168,0.0158]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Coal|w/o CCS","MtCO2/yr",7568,4923,1866,324.6,3.69]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Gas|w/ CCS","MtCO2/yr",0,0,0,0,0]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Electricity|Gas|w/o CCS","MtCO2/yr",2152,3584,4416,2840,1079]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Gases","Mt CO2/yr",3491,2970,2034,1707,1544]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Heat","Mt CO2/yr",1155,797.8,403.4,169,40.6]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Liquids","Mt CO2/yr",11800,15570,18020,16520,11030]
["REMIND","NewRE","World","Emissions|CO2|Energy|Supply|Solids","Mt CO2/yr",11800,15570,18020,16520,11030]
["REMIND","NewRE","World","Emissions|CO2|Fossil Fuels and Industry","Mt CO2/yr",32610,32500,29530,23260,14460]
["REMIND","NewRE","World","Emissions|CO2|Fossil Fuels and Industry|Energy Supply","Mt CO2/yr",14520,13130,9886,4614,-1535]
["REMIND","NewRE","World","Emissions|CO2|Land Use","Mt CO2/yr",4437,2459,395.3,-178.5,-177.6]
["REMIND","NewRE","World","Final Energy","EJ/yr",368.8,409.2,441.5,462.3,486.8]
["REMIND","NewRE","World","Final Energy|Electricity","EJ/yr",60.37,75.47,102.8,134.3,180.8]
["REMIND","NewRE","World","Final Energy|Gases","EJ/yr",57.12,50.31,37.15,32.18,29.04]
["REMIND","NewRE","World","Final Energy|Heat","EJ/yr",10.77,9.682,9.425,9.699,8.726]
["REMIND","NewRE","World","Final Energy|Hydrogen","EJ/yr",0.3757,0.3164,0.7251,2.412,4.734]
["REMIND","NewRE","World","Final Energy|Liquids","EJ/yr",148.6,199.8,239,247.1,240]
["REMIND","NewRE","World","Final Energy|Other Sector","EJ/yr",277.1,302.1,307.6,316.2,334.2]
["REMIND","NewRE","World","Final Energy|Solids","EJ/yr",91.6,73.63,52.41,36.6,23.48]
["REMIND","NewRE","World","Final Energy|Solids|Biomass","EJ/yr",49.17,47.45,40.69,30.83,19.92]
["REMIND","NewRE","World","Final Energy|Solids|Biomass|Traditional","EJ/yr",48.96,46.1,37.95,27.37,16.37]
["REMIND","NewRE","World","Final Energy|Solids|Coal","EJ/yr",42.44,26.18,11.73,5.77,3.556]
["REMIND","NewRE","World","Final Energy|Transportation","EJ/yr",91.72,107.1,133.9,146.1,152.6]
["REMIND","NewRE","World","GDP|MER","billion US$2010/yr",56815.9846,78472.3016,104581.7334,130491.772,157520.6]
["REMIND","NewRE","World","GDP|PPP","billion US$2010/yr",74628.4438,110375.2136,155305.148,200500.94,248576.9]
["REMIND","NewRE","World","Policy Cost|Consumption Loss","billion US$2010/yr",0,173.5829,1144.2954,2392.7184,3708.714]
["REMIND","NewRE","World","Policy Cost|GDP Loss","billion US$2010/yr",0,698.4301,1515.3883,2586.5729,3617.879]
["REMIND","NewRE","World","Policy Cost|Other","billion US$2010/yr",0,0,0,0,0]
["REMIND","NewRE","World","Population","million",6894,7638,8288,8810,9187]
["REMIND","NewRE","World","Price|Carbon","US$2010/tCO2",0,0,0,0,0]
["REMIND","NewRE","World","Price|Primary Energy|Coal","US$2010/GJ",1.8156,1.6339,1.4877,1.3204,1.2097]
["REMIND","NewRE","World","Price|Primary Energy|Gas","US$2010/GJ",3.239,4.0421,5.1311,5.953,6.128]
["REMIND","NewRE","World","Price|Primary Energy|Oil","US$2010/GJ",6.4094,7.115,8.6847,9.9708,11.0419]
["REMIND","NewRE","World","Price|Secondary Energy|Electricity","US$2010/GJ",14.0794,20.2716,21.4348,22.4982,21.4237]
["REMIND","NewRE","World","Primary Energy","EJ/yr",513.4,545.9,556.2,552.6,581.9]
["REMIND","NewRE","World","Primary Energy|Biomass","EJ/yr",59.46,67.03,68.5,84.23,138.5]
["REMIND","NewRE","World","Primary Energy|Biomass|Electricity","EJ/yr",1.091,2.298,4.934,8.221,15.48]
["REMIND","NewRE","World","Primary Energy|Biomass|Electricity|w/ CCS","EJ/yr",0,0.0166,0.4327,3.445,11.59]
["REMIND","NewRE","World","Primary Energy|Biomass|Gases","EJ/yr",6.856,6.875,6.467,4.487,1.348]
["REMIND","NewRE","World","Primary Energy|Biomass|Hydrogen","EJ/yr",0,0.0095,0.3194,2.201,6.347]
["REMIND","NewRE","World","Primary Energy|Biomass|Hydrogen|w/ CCS","EJ/yr",0,0.009,0.3188,2.201,6.346]
["REMIND","NewRE","World","Primary Energy|Biomass|Liquids","EJ/yr",0.3133,6.822,9.795,31.32,89.54]
["REMIND","NewRE","World","Primary Energy|Biomass|Liquids|w/ CCS","EJ/yr",0,0.1183,3.091,24.61,82.78]
["REMIND","NewRE","World","Primary Energy|Biomass|Modern","EJ/yr",10.02,20.63,30.4,56.82,122.1]
["REMIND","NewRE","World","Primary Energy|Biomass|Other Carrier","EJ/yr",51.2,51.03,46.98,38,25.74]
["REMIND","NewRE","World","Primary Energy|Biomass|Traditional","EJ/yr",49.44,46.4,38.1,27.41,16.37]
["REMIND","NewRE","World","Primary Energy|Biomass|w/ CCS","EJ/yr",0,0.1439,3.843,30.25,100.7]
["REMIND","NewRE","World","Primary Energy|Biomass|w/o CCS","EJ/yr",59.46,66.89,64.66,53.98,37.75]
["REMIND","NewRE","World","Primary Energy|Coal","EJ/yr",131.6,83.82,33.8,10.19,3.824]
["REMIND","NewRE","World","Primary Energy|Coal|Electricity","EJ/yr",79.08,51.44,19.5,3.393,0.0402]
["REMIND","NewRE","World","Primary Energy|Coal|Electricity|w/ CCS","EJ/yr",0,1E-4,0.0009,1.8E-3,0.0017]
["REMIND","NewRE","World","Primary Energy|Coal|Hydrogen","EJ/yr",0.1425,0.0706,0.0406,0.0364,0.0311]
["REMIND","NewRE","World","Primary Energy|Coal|Hydrogen|w/ CCS","EJ/yr",0,0.0011,0.0171,0.0327,0.0307]
["REMIND","NewRE","World","Primary Energy|Coal|w/ CCS","EJ/yr",0,1.5E-3,0.0189,0.0353,0.0331]
["REMIND","NewRE","World","Primary Energy|Coal|w/o CCS","EJ/yr",131.6,83.82,33.78,10.16,3.791]
["REMIND","NewRE","World","Primary Energy|Fossil","EJ/yr",429.8,444.5,424.8,356.1,270.6]
["REMIND","NewRE","World","Primary Energy|Fossil|w/ CCS","EJ/yr",0,0.064,0.6297,1.705,1.782]
["REMIND","NewRE","World","Primary Energy|Fossil|w/o CCS","EJ/yr",429.8,444.4,424.1,354.4,268.8]
["REMIND","NewRE","World","Primary Energy|Gas","EJ/yr",110.7,124.4,120,84.63,49.22]
["REMIND","NewRE","World","Primary Energy|Gas|Electricity","EJ/yr",38.35,63.89,78.71,50.62,19.23]
["REMIND","NewRE","World","Primary Energy|Gas|Electricity|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","World","Primary Energy|Gas|w/ CCS","EJ/yr",0,0.0624,0.6108,1.67,1.749]
["REMIND","NewRE","World","Primary Energy|Gas|w/o CCS","EJ/yr",110.7,124.3,119.4,82.96,47.47]
["REMIND","NewRE","World","Primary Energy|Geothermal","EJ/yr",0.3321,0.5441,1.014,1.211,1.89]
["REMIND","NewRE","World","Primary Energy|Hydro","EJ/yr",11.66,13.24,15.14,16.12,16.47]
["REMIND","NewRE","World","Primary Energy|Non-Biomass Renewables","EJ/yr",13.97,26.66,58.56,109.8,171.8]
["REMIND","NewRE","World","Primary Energy|Nuclear","EJ/yr",10.2,7.741,4.385,2.411,0.9662]
["REMIND","NewRE","World","Primary Energy|Oil","EJ/yr",187.5,236.2,271,261.3,217.6]
["REMIND","NewRE","World","Primary Energy|Oil|w/o CCS","EJ/yr",187.5,236.2,271,261.3,217.6]
["REMIND","NewRE","World","Primary Energy|Solar","EJ/yr",0.2366,3.66,20.07,55.47,104.2]
["REMIND","NewRE","World","Primary Energy|Wind","EJ/yr",1.743,9.219,22.34,37.01,49.33]
["REMIND","NewRE","World","Resource|Cumulative Extraction|Coal","EJ",634.4,1753,2324,2529,2594]
["REMIND","NewRE","World","Resource|Cumulative Extraction|Gas","EJ",111.3,123.6,118.5,83.78,49]
["REMIND","NewRE","World","Resource|Cumulative Extraction|Oil","EJ",189.9,239.2,274.5,264.5,220.2]
["REMIND","NewRE","World","Secondary Energy","EJ/yr",408.7,446.6,471.6,483.6,498.8]
["REMIND","NewRE","World","Secondary Energy|Electricity","EJ/yr",74.34,89.62,117.2,147.8,192.3]
["REMIND","NewRE","World","Secondary Energy|Electricity|Biomass","EJ/yr",0.583,1.617,3.835,5.843,8.719]
["REMIND","NewRE","World","Secondary Energy|Electricity|Biomass|w/ CCS","EJ/yr",0,0.0068,0.1774,1.413,4.751]
["REMIND","NewRE","World","Secondary Energy|Electricity|Biomass|w/o CCS","EJ/yr",0.583,1.61,3.657,4.431,3.968]
["REMIND","NewRE","World","Secondary Energy|Electricity|Coal","EJ/yr",28.47,19.12,7.516,1.468,0.0185]
["REMIND","NewRE","World","Secondary Energy|Electricity|Coal|w/ CCS","EJ/yr",0,0,0.0005,1E-3,0.0009]
["REMIND","NewRE","World","Secondary Energy|Electricity|Coal|w/o CCS","EJ/yr",28.47,19.12,7.515,1.467,0.0176]
["REMIND","NewRE","World","Secondary Energy|Electricity|Fossil","EJ/yr",49.58,53.6,50.38,29.58,10.76]
["REMIND","NewRE","World","Secondary Energy|Electricity|Fossil|w/ CCS","EJ/yr",0,0,0.0006,0.0011,1E-3]
["REMIND","NewRE","World","Secondary Energy|Electricity|Fossil|w/o CCS","EJ/yr",49.58,53.6,50.38,29.58,10.75]
["REMIND","NewRE","World","Secondary Energy|Electricity|Gas","EJ/yr",17.68,32.65,42.25,28.01,10.7]
["REMIND","NewRE","World","Secondary Energy|Electricity|Gas|w/ CCS","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","World","Secondary Energy|Electricity|Gas|w/o CCS","EJ/yr",17.68,32.65,42.25,28.01,10.7]
["REMIND","NewRE","World","Secondary Energy|Electricity|Geothermal","EJ/yr",0.332,0.544,1.012,1.14,1.2]
["REMIND","NewRE","World","Secondary Energy|Electricity|Hydro","EJ/yr",11.66,13.24,15.14,16.12,16.47]
["REMIND","NewRE","World","Secondary Energy|Electricity|Non-Biomass Renewables","EJ/yr",13.97,27,61.76,122.9,198.5]
["REMIND","NewRE","World","Secondary Energy|Electricity|Nuclear","EJ/yr",10.2,7.741,4.385,2.411,0.9662]
["REMIND","NewRE","World","Secondary Energy|Electricity|Oil","EJ/yr",3.437,1.821,0.612,0.1066,0.0358]
["REMIND","NewRE","World","Secondary Energy|Electricity|Oil|w/o CCS","EJ/yr",3.437,1.821,0.612,0.1066,0.0358]
["REMIND","NewRE","World","Secondary Energy|Electricity|Solar","EJ/yr",0.2366,3.679,21.55,64.5,125.6]
["REMIND","NewRE","World","Secondary Energy|Electricity|Solar|CSP","EJ/yr",0.0094,0.4237,4.506,20.98,52]
["REMIND","NewRE","World","Secondary Energy|Electricity|Solar|PV","EJ/yr",0.2272,3.256,17.04,43.52,73.56]
["REMIND","NewRE","World","Secondary Energy|Electricity|Wind","EJ/yr",1.743,9.532,24.06,41.15,55.23]
["REMIND","NewRE","World","Secondary Energy|Electricity|Wind|Onshore","EJ/yr",1.743,9.532,24.06,41.15,55.23]
["REMIND","NewRE","World","Secondary Energy|Gases","EJ/yr",66.68,59.23,43.77,37.91,34.16]
["REMIND","NewRE","World","Secondary Energy|Gases|Biomass","EJ/yr",3.771,3.781,3.557,2.468,0.7412]
["REMIND","NewRE","World","Secondary Energy|Gases|Coal","EJ/yr",1E-4,0.0003,0.0003,0.0003,0.0003]
["REMIND","NewRE","World","Secondary Energy|Gases|Natural Gas","EJ/yr",62.23,52.95,36.26,30.42,27.52]
["REMIND","NewRE","World","Secondary Energy|Gases|Other","EJ/yr",0.6802,2.503,3.955,5.017,5.901]
["REMIND","NewRE","World","Secondary Energy|Heat","EJ/yr",12.59,11.06,10.58,10.54,9.185]
["REMIND","NewRE","World","Secondary Energy|Hydrogen","EJ/yr",0.3757,0.3164,0.7251,2.412,4.734]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Biomass","EJ/yr",0,5.3E-3,0.1757,1.211,3.491]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Biomass|w/ CCS","EJ/yr",0,0.005,0.1754,1.21,3.491]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Biomass|w/o CCS","EJ/yr",0,0.0003,0.0003,0.0003,0.0003]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Coal","EJ/yr",0.0909,0.045,0.0252,0.022,0.0187]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Coal|w/ CCS","EJ/yr",0,0.0007,0.0103,0.0196,0.0184]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Coal|w/o CCS","EJ/yr",0.0909,0.0443,0.015,0.0024,0.0003]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Electricity","EJ/yr",0,0,0,0,0]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Gas","EJ/yr",0.2847,0.2662,0.5241,1.18,1.225]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Gas|w/ CCS","EJ/yr",0,0.0437,0.4276,1.169,1.224]
["REMIND","NewRE","World","Secondary Energy|Hydrogen|Gas|w/o CCS","EJ/yr",0.2847,0.2225,0.0966,0.0107,0.0004]
["REMIND","NewRE","World","Secondary Energy|Liquids","EJ/yr",162,214.3,250.6,253.3,240.9]
["REMIND","NewRE","World","Secondary Energy|Liquids|Biomass","EJ/yr",0.1845,4.284,5.673,15.74,42.96]
["REMIND","NewRE","World","Secondary Energy|Liquids|Coal","EJ/yr",0,0.0004,0.0006,0.0006,0.0006]
["REMIND","NewRE","World","Secondary Energy|Liquids|Oil","EJ/yr",161.8,210,244.9,237.5,197.9]
["REMIND","NewRE","World","Secondary Energy|Solids","EJ/yr",43.91,28.14,14.67,9.285,7.111]
["REMIND","NewRE","World","Secondary Energy|Solids|Biomass","EJ/yr",0.2035,1.368,2.766,3.478,3.555]
["REMIND","NewRE","World","Secondary Energy|Solids|Coal","EJ/yr",43.7,26.77,11.9,5.807,3.556]
["REMIND","NewRE","World","Water Consumption|Electricity","km3/yr",83.16,88.16,95.47,103.8,120.4]
["REMIND","NewRE","World","Water Consumption|Electricity|Biomass","km3/yr",0.1686,0.4003,0.8212,0.9251,0.7265]
["REMIND","NewRE","World","Water Consumption|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Consumption|Electricity|Biomass|w/o CCS","km3/yr",0.1686,0.4003,0.8212,0.9251,0.7265]
["REMIND","NewRE","World","Water Consumption|Electricity|Coal","km3/yr",14.59,9.269,3.392,0.5047,0.0054]
["REMIND","NewRE","World","Water Consumption|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Consumption|Electricity|Coal|w/o CCS","km3/yr",14.59,9.269,3.392,0.5047,0.0054]
["REMIND","NewRE","World","Water Consumption|Electricity|Cooling Pond","km3/yr",1.469,1.016,0.4642,0.1725,0.0472]
["REMIND","NewRE","World","Water Consumption|Electricity|Dry Cooling","km3/yr",0.0606,0.107,0.2586,0.5381,1.015]
["REMIND","NewRE","World","Water Consumption|Electricity|Fossil","km3/yr",22.04,19.26,13.77,6.366,1.702]
["REMIND","NewRE","World","Water Consumption|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Consumption|Electricity|Fossil|w/o CCS","km3/yr",22.04,19.26,13.77,6.366,1.702]
["REMIND","NewRE","World","Water Consumption|Electricity|Gas","km3/yr",5.579,8.874,9.947,5.796,1.684]
["REMIND","NewRE","World","Water Consumption|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Consumption|Electricity|Gas|w/o CCS","km3/yr",5.579,8.874,9.947,5.796,1.684]
["REMIND","NewRE","World","Water Consumption|Electricity|Geothermal","km3/yr",1.278,2.093,3.895,4.388,4.616]
["REMIND","NewRE","World","Water Consumption|Electricity|Hydro","km3/yr",55.05,62.52,71.49,76.15,77.75]
["REMIND","NewRE","World","Water Consumption|Electricity|Non-Biomass Renewables","km3/yr",56.34,64.99,78.89,95.42,117.5]
["REMIND","NewRE","World","Water Consumption|Electricity|Nuclear","km3/yr",4.61,3.505,1.991,1.099,0.4427]
["REMIND","NewRE","World","Water Consumption|Electricity|Oil","km3/yr",1.871,1.119,0.4287,0.0648,0.0121]
["REMIND","NewRE","World","Water Consumption|Electricity|Oil|w/o CCS","km3/yr",1.871,1.119,0.4287,0.0648,0.0121]
["REMIND","NewRE","World","Water Consumption|Electricity|Once Through","km3/yr",3.001,2.33,1.252,0.5063,0.1353]
["REMIND","NewRE","World","Water Consumption|Electricity|Solar","km3/yr",0.0126,0.3798,3.505,14.89,35.12]
["REMIND","NewRE","World","Water Consumption|Electricity|Solar|CSP","km3/yr",0.0064,0.2917,3.081,13.93,33.61]
["REMIND","NewRE","World","Water Consumption|Electricity|Solar|PV","km3/yr",0.0062,0.0881,0.4245,0.9594,1.507]
["REMIND","NewRE","World","Water Consumption|Electricity|Wet Tower","km3/yr",23.52,22,21.27,24.6,37.99]
["REMIND","NewRE","World","Water Consumption|Electricity|Wind","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Withdrawal|Electricity","km3/yr",505.4,390.4,217.5,106.1,64.46]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Biomass","km3/yr",4.128,6.299,7.003,6.569,4.219]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Biomass|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Biomass|w/o CCS","km3/yr",4.128,6.299,7.003,6.569,4.219]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Coal","km3/yr",290.3,184.5,67.67,11.83,0.1004]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Coal|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Coal|w/o CCS","km3/yr",290.3,184.5,67.67,11.83,0.1004]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Cooling Pond","km3/yr",25.91,16.63,6.712,1.981,0.5335]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Dry Cooling","km3/yr",0.0606,0.107,0.2586,0.5381,1.015]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Fossil","km3/yr",384.8,293.9,153.3,52.73,9.373]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Fossil|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Fossil|w/o CCS","km3/yr",384.8,293.9,153.3,52.73,9.373]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Gas","km3/yr",70.54,94.12,79.78,40.56,9.24]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Gas|w/ CCS","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Gas|w/o CCS","km3/yr",70.54,94.12,79.78,40.56,9.24]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Geothermal","km3/yr",1.278,2.093,3.895,4.388,4.616]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Hydro","km3/yr",0,0,0,0,0]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Non-Biomass Renewables","km3/yr",1.29,2.473,7.4,19.28,39.73]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Nuclear","km3/yr",115.1,87.64,49.84,27.56,11.14]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Oil","km3/yr",23.99,15.28,5.844,0.3298,0.0321]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Oil|w/o CCS","km3/yr",23.99,15.28,5.844,0.3298,0.0321]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Once Through","km3/yr",445.1,342.2,182,73.77,20.3]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Solar","km3/yr",0.0126,0.3798,3.505,14.89,35.12]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Solar|CSP","km3/yr",0.0064,0.2917,3.081,13.93,33.61]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Solar|PV","km3/yr",0.0062,0.0881,0.4245,0.9594,1.507]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Wet Tower","km3/yr",34.23,31.2,27.87,27.99,39.2]
["REMIND","NewRE","World","Water Withdrawal|Electricity|Wind","km3/yr",0,0,0,0,0]