
Ground testing on gas-turbine engine

Double turbine blades with Al2O3-modified PS-PVD 7YSZ TBCs were tested on gas-turbine engines, as seen in Fig. 1. The Fig. 1 shows the testing images of the gas-turbine engine in operation. The double turbine blades after testing, present no apparent TBCs spallation. 
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Supplementary Fig. 1 Ground testing of PS-PVD Al2O3-modified 7YSZ TBCs in gas-turbine engine.  
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