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[bookmark: _Ref515458481]Figure S1: Coulombic efficiency of the Co3O4 nanoparticles over 50 cycles.
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Figure S2: CV of the Co3O4/RGO nanocomposites at 0.1 mV/s.
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[bookmark: _GoBack]Figure S3: Nyquist plots of the Co3O4/RGO nanocomposites after 100 charge/discharge cycles performed at 100 mA/g.
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