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Supporting Information
Movie S1: Animation showing the measured time domain signal and power spectrum as a single cell passes through the ultrasound beam. The time between frames is 250 μs.
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