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[bookmark: _GoBack]Supplementary Figure S1. Comparison of (a) raw data and (b) ratiometric features. The measured impedance of 10 finger pairs for five subjects over five days. Values are the mean ± S.D. (at least n = 50).
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