Fabrication of Nanochitosan Incorporated Polypyrrole/Alginate Conducting Scaffold for Neural Tissue Engineering
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Video Legend
The comparison of wettability (water absorption) between the nanochitosan/PPy-Alg scaffold and PPy-Alg composite.
